*** Creating Trace Output File '.\Obj\lhc.tra' Ok.
### Preparing for ADS-LD.
### Creating ADS-LD Command Line
### List of Objects: adding '".\obj\misc.o"'
### List of Objects: adding '".\obj\stm32f10x_adc.o"'
### List of Objects: adding '".\obj\stm32f10x_bkp.o"'
### List of Objects: adding '".\obj\stm32f10x_crc.o"'
### List of Objects: adding '".\obj\stm32f10x_dac.o"'
### List of Objects: adding '".\obj\stm32f10x_dbgmcu.o"'
### List of Objects: adding '".\obj\stm32f10x_dma.o"'
### List of Objects: adding '".\obj\stm32f10x_exti.o"'
### List of Objects: adding '".\obj\stm32f10x_flash.o"'
### List of Objects: adding '".\obj\stm32f10x_fsmc.o"'
### List of Objects: adding '".\obj\stm32f10x_gpio.o"'
### List of Objects: adding '".\obj\stm32f10x_iwdg.o"'
### List of Objects: adding '".\obj\stm32f10x_pwr.o"'
### List of Objects: adding '".\obj\stm32f10x_rcc.o"'
### List of Objects: adding '".\obj\main.o"'
### List of Objects: adding '".\obj\stm32f10x_it.o"'
### List of Objects: adding '".\obj\qdmx_usb.o"'
### List of Objects: adding '".\obj\usb_desc.o"'
### List of Objects: adding '".\obj\usb_endp.o"'
### List of Objects: adding '".\obj\usb_istr.o"'
### List of Objects: adding '".\obj\usb_prop.o"'
### List of Objects: adding '".\obj\usb_pwr.o"'
### List of Objects: adding '".\obj\qdmx_adc.o"'
### List of Objects: adding '".\obj\core_cm3.o"'
### List of Objects: adding '".\obj\system_stm32f10x.o"'
### List of Objects: adding '".\obj\startup_stm32f10x_md.o"'
### List of Objects: adding '".\obj\usb_core.o"'
### List of Objects: adding '".\obj\usb_init.o"'
### List of Objects: adding '".\obj\usb_int.o"'
### List of Objects: adding '".\obj\usb_mem.o"'
### List of Objects: adding '".\obj\usb_regs.o"'
### List of Objects: adding '".\obj\usb_sil.o"'
### ADS-LD Command completed:
--device DARMSTM ".\obj\misc.o" ".\obj\stm32f10x_adc.o" ".\obj\stm32f10x_bkp.o" ".\obj\stm32f10x_crc.o" ".\obj\stm32f10x_dac.o" ".\obj\stm32f10x_dbgmcu.o" ".\obj\stm32f10x_dma.o" ".\obj\stm32f10x_exti.o" ".\obj\stm32f10x_flash.o" ".\obj\stm32f10x_fsmc.o" ".\obj\stm32f10x_gpio.o" ".\obj\stm32f10x_iwdg.o" ".\obj\stm32f10x_pwr.o" ".\obj\stm32f10x_rcc.o" ".\obj\main.o" ".\obj\stm32f10x_it.o" ".\obj\qdmx_usb.o" ".\obj\usb_desc.o" ".\obj\usb_endp.o" ".\obj\usb_istr.o" ".\obj\usb_prop.o" ".\obj\usb_pwr.o" ".\obj\qdmx_adc.o" ".\obj\core_cm3.o" ".\obj\system_stm32f10x.o" ".\obj\startup_stm32f10x_md.o" ".\obj\usb_core.o" ".\obj\usb_init.o" ".\obj\usb_int.o" ".\obj\usb_mem.o" ".\obj\usb_regs.o" ".\obj\usb_sil.o" --strict --scatter ".\Obj\lhc.sct" 

--autoat --summary_stderr --info summarysizes --map --xref --callgraph --symbols 

--info sizes --info totals --info unused --info veneers 

 --list ".\List\lhc.map" -o ".\Obj\lhc.axf"### Preparing Environment (PrepEnvAds)
### ADS-LD Output File: '.\Obj\lhc.axf'
### ADS-LD Command File: '.\Obj\lhc.lnp'
### Checking for dirty Components...
### Creating CmdFile '.\Obj\lhc.lnp', Handle=0x000002BC
### Writing '.lnp' file
### ADS-LD Command file '.\Obj\lhc.lnp' is ready.
### ADS-LD: About to start ADS-LD Thread.
### ADS-LD: executed with 0 errors
### Updating obj list
### LDADS_file() completed.
