#

##

##

    µVision3 Build Log
    Project:
    D:\Arm Programing\STM32F103C8\MDK\lhc.uv2
    Project File Date:  10/18/2010

    Output:
    Load "D:\\Arm Programing\\STM32F103C8\\MDK\\Obj\\lhc.AXF"
    VTarget = 3.293V
    Info: TotalIRLen = 9, IRPrint = 0x0011
    Info: Found Cortex-M3 r1p1, Little endian.
    Info: TPIU fitted.
    Info:   FPUnit: 6 code (BP) slots and 2 literal slots
    Info: Core is locked-up!
    Info: CPU halted
    Info: TotalIRLen = 9, IRPrint = 0x0011
    Info: Found Cortex-M3 r1p1, Little endian.
    Info: TPIU fitted.
    Info:   FPUnit: 6 code (BP) slots and 2 literal slots
    DLL version V4.05i, compiled May 18 2009 19:20:52
    Firmware: J-Link ARM V8 compiled Dec  1 2009 11:42:48
    Hardware: V8.00
    Hardware-Breakpoints: 6
    Software-Breakpoints: 2048
    Watchpoints:          0
    Found 2 JTAG devices, Total IRLen = 9:
     Id of device #0: 0x3BA00477
     Id of device #1: 0x16410041
    Cortex-M3 identified.
    JTAG speed: 5 kHz
    Info: TotalIRLen = 9, IRPrint = 0x0011
    Info: Found Cortex-M3 r1p1, Little endian.
    Info: TPIU fitted.
    Info:   FPUnit: 6 code (BP) slots and 2 literal slots
    Info: TotalIRLen = 9, IRPrint = 0x0011
    Info: Found Cortex-M3 r1p1, Little endian.
    Info: TPIU fitted.
    Info:   FPUnit: 6 code (BP) slots and 2 literal slots
    JTAG speed: 200 kHz
    Include "D:\\Arm Programing\\STM32F103C8\\MDK\\JLinkArm_STM32.ini"
    [FLASH]
    ^
    *** error 10: Syntax error
    Erase Done.
    Programming Done.
    Verify OK.