<?xml version="1.0" encoding="UTF-8"?>
<module fritzingVersion="0.7.0b.02.01.5801" moduleId="91c6fc103d5e4575e7164fa1230d1621">
    <version>1</version>
    <author>Mattia Francesco Moro</author>
    <title>attiny85</title>
    <label>U</label>
    <date>2012-02-14</date>
    <tags>
        <tag>IC</tag>
        <tag>DIP</tag>
        <tag>Microcontroller</tag>
        <tag>Atmel</tag>
        <tag>through-hole</tag>
    </tags>
    <properties>
        <property name="package">dip</property>
        <property name="version">Attiny85-20PU</property>
        <property name="family">Microcontroller</property>
        <property name="type">Atmel AVR</property>
        <property name="part number"></property>
		<property name="variant">dip08 THT</property>
    </properties>
    <description>Atmel ATtiny85 microcontroller. So small but so powerfull.</description>
    <views>
        <iconView>
            <layers image="icon/ATtiny85_icon.svg">
                <layer layerId="icon"/>
            </layers>
        </iconView>
        <breadboardView>
            <layers image="breadboard/ATtiny85_breadboard.svg">
                <layer layerId="breadboard"/>
            </layers>
        </breadboardView>
        <schematicView>
            <layers image="schematic/ATtiny85_schematic.svg">
                <layer layerId="schematic"/>
            </layers>
        </schematicView>
        <pcbView>
            <layers image="pcb/dip_8_300mil_pcb.svg">
                <layer layerId="copper0"/>
                <layer layerId="silkscreen"/>
                <layer layerId="copper1"/>
            </layers>
        </pcbView>
    </views>
    <connectors>
        <connector id="connector3" type="male" name="Pin 4">
            <description>GND </description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector3pin"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector3pin" terminalId="connector3terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper1" svgId="connector3pin"/>
                    <p layer="copper0" svgId="connector3pin"/>
                </pcbView>
            </views>
        </connector>
        <connector id="connector4" type="male" name="Pin 5">
            <description>PB0 (MOSI/DI/SDA/AIN0/OC0A/OC1A/AREF/PCINT0) </description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector4pin"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector4pin" terminalId="connector4terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper1" svgId="connector4pin"/>
                    <p layer="copper0" svgId="connector4pin"/>
                </pcbView>
            </views>
        </connector>
        <connector id="connector5" type="male" name="Pin 6">
            <description>PB1 (MISO/DO/AIN1/OC0B/OC1A/PCINT1) </description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector5pin"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector5pin" terminalId="connector5terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper1" svgId="connector5pin"/>
                    <p layer="copper0" svgId="connector5pin"/>
                </pcbView>
            </views>
        </connector>
        <connector id="connector6" type="male" name="Pin 7">
            <description>PB2 (SCK/USCK/SCL/ADC1/T0/INT0/PCINT2) </description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector6pin"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector6pin" terminalId="connector6terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper1" svgId="connector6pin"/>
                    <p layer="copper0" svgId="connector6pin"/>
                </pcbView>
            </views>
        </connector>
        <connector id="connector7" type="male" name="Pin 8">
            <description>VCC </description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector7pin"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector7pin" terminalId="connector7terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper1" svgId="connector7pin"/>
                    <p layer="copper0" svgId="connector7pin"/>
                </pcbView>
            </views>
        </connector>
        <connector id="connector0" type="male" name="Pin 1">
            <description>PB5 (PCINT5/RESET/ADC0/dW) </description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector0pin"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector0pin" terminalId="connector0terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper1" svgId="connector0pin"/>
                    <p layer="copper0" svgId="connector0pin"/>
                </pcbView>
            </views>
        </connector>
        <connector id="connector1" type="male" name="Pin 2">
            <description>PB3 (PCINT3/XTAL1/CLKI/OC1B/ADC3) </description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector1pin"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector1pin" terminalId="connector1terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper1" svgId="connector1pin"/>
                    <p layer="copper0" svgId="connector1pin"/>
                </pcbView>
            </views>
        </connector>
        <connector id="connector2" type="male" name="Pin 3">
            <description>PB4 (PCINT4/XTAL2/CLKO/OC1B/ADC2)</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector2pin"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector2pin" terminalId="connector2terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper1" svgId="connector2pin"/>
                    <p layer="copper0" svgId="connector2pin"/>
                </pcbView>
            </views>
        </connector>
    </connectors>
</module>
