<?xml version='1.0' encoding='UTF-8'?>
<module moduleId="chipkit_BasicIOShield" referenceFile="chipkit_BasicIOShield.fzp">
 <version>4</version>
 <author>Amber Mear/Digilent Inc.</author>
 <title>chipKIT Basic I/O Shield</title>
 <label>Basic IO Shield</label>
 <date>Wed Feb 19 2014</date>
 <tags>
  <tag>DIP</tag>
  <tag>fritzing core</tag>
    <tag>chipkit</tag>
 </tags>
 <properties>
  <property name="family">chipKIT</property>
  <property name="package">basicIOShield</property>
  <property name="variant">variant 3</property>
 </properties>
 <taxonomy>part.dip.44.pins</taxonomy>
 <description>&lt;!DOCTYPE HTML PUBLIC "-//W3C//DTD HTML 4.0//EN" "http://www.w3.org/TR/REC-html40/strict.dtd">
&lt;html>&lt;head>&lt;meta name="qrichtext" content="1" />&lt;style type="text/css">
p, li { white-space: pre-wrap; }
&lt;/style>&lt;/head>&lt;body style=" font-family:'MS Shell Dlg 2'; font-size:8.25pt; font-weight:400; font-style:normal;">
&lt;p style=" margin-top:0px; margin-bottom:0px; margin-left:0px; margin-right:0px; -qt-block-indent:0; text-indent:0px;">&lt;span style=" font-family:'Arial,Geneva,Verdana,Helvetica'; font-size:14px; color:#000000; background-color:#fffffd;">The chipKIT Basic I/O Shield is an input/output expansion board designed for use with chipKIT microcontroller boards such as the Uno32™ and the Max32™.  The Basic I/O Shield is designed to provide a range of input/output devices suitable for beginners learning about microcontrollers and various types of I/O devices, or for use by more advanced user to provide inputs or outputs for their own projects.  The Basic I/O Shield provides simple digital input devices such as switches and buttons, and digital output devices such as discrete LEDs and high current open FET drivers. It provides more advanced devices such as an I&lt;/span>&lt;span style=" font-family:'Arial,Geneva,Verdana,Helvetica'; color:#000000; background-color:#fffffd;">2&lt;/span>&lt;span style=" font-family:'Arial,Geneva,Verdana,Helvetica'; font-size:14px; color:#000000; background-color:#fffffd;">C EEPROM, an I&lt;/span>&lt;span style=" font-family:'Arial,Geneva,Verdana,Helvetica'; color:#000000; background-color:#fffffd;">2&lt;/span>&lt;span style=" font-family:'Arial,Geneva,Verdana,Helvetica'; font-size:14px; color:#000000; background-color:#fffffd;">C temperature sensor, and organic LED graphic display. A potentiometer is also provided for use as an analog input device. &lt;/span>&lt;/p>&lt;/body>&lt;/html></description>
 <views>
  <iconView>
   <layers image="icon/chipkit_BasicIOShield_icon.svg">
    <layer layerId="icon"/>
   </layers>
  </iconView>
  <breadboardView>
   <layers image="breadboard/chipkit_BasicIOShield_breadboard.svg">
    <layer layerId="breadboard"/>
   </layers>
  </breadboardView>
  <schematicView>
   <layers image="schematic/chipkit_BasicIOShield_schematic.svg">
    <layer layerId="schematic"/>
   </layers>
  </schematicView>
  <pcbView>
   <layers image="pcb/chipkit_BasicIOShield_pcb.svg">
    <layer layerId="silkscreen"/>
    <layer layerId="copper0"/>
    <layer layerId="copper1"/>
   </layers>
  </pcbView>
 </views>
 <connectors>
  <connector type="female" id="connector0" name="RST">
   <description>RESET</description>
   <views>
    <breadboardView>
     <p svgId="connector0pin" layer="breadboard" terminalId="connector0terminal"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector0pin" layer="schematic" terminalId="connector0terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector0pin" layer="copper0"/>
     <p svgId="connector0pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector type="female" id="connector1" name="3V3">
   <description>pin 2</description>
   <views>
    <breadboardView>
     <p svgId="connector1pin" layer="breadboard" terminalId="connector1terminal"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector1pin" layer="schematic" terminalId="connector1terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector1pin" layer="copper0"/>
     <p svgId="connector1pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector type="female" id="connector2" name="5V0">
   <description>5V Power Supply</description>
   <views>
    <breadboardView>
     <p svgId="connector2pin" layer="breadboard" terminalId="connector2terminal"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector2pin" layer="schematic" terminalId="connector2terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector2pin" layer="copper0"/>
     <p svgId="connector2pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector type="female" id="connector3" name="GND">
   <description>Ground</description>
   <views>
    <breadboardView>
     <p svgId="connector3pin" layer="breadboard" terminalId="connector3terminal"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector3pin" layer="schematic" terminalId="connector3terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector3pin" layer="copper0"/>
     <p svgId="connector3pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector type="female" id="connector4" name="GND">
   <description>Ground</description>
   <views>
    <breadboardView>
     <p svgId="connector4pin" layer="breadboard" terminalId="connector4terminal"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector4pin" layer="schematic" terminalId="connector4terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector4pin" layer="copper0"/>
     <p svgId="connector4pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector type="female" id="connector5" name="VIN">
   <description>pin 6</description>
   <views>
    <breadboardView>
     <p svgId="connector5pin" layer="breadboard" terminalId="connector5terminal"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector5pin" layer="schematic" terminalId="connector5terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector5pin" layer="copper0"/>
     <p svgId="connector5pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector type="female" id="connector6" name="A0">
   <description>pin 7</description>
   <views>
    <breadboardView>
     <p svgId="connector6pin" layer="breadboard" terminalId="connector6terminal"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector6pin" layer="schematic" terminalId="connector6terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector6pin" layer="copper0"/>
     <p svgId="connector6pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector type="female" id="connector7" name="A1">
   <description>pin 8</description>
   <views>
    <breadboardView>
     <p svgId="connector7pin" layer="breadboard" terminalId="connector7terminal"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector7pin" layer="schematic" terminalId="connector7terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector7pin" layer="copper0"/>
     <p svgId="connector7pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector type="female" id="connector8" name="A2">
   <description>pin 9</description>
   <views>
    <breadboardView>
     <p svgId="connector8pin" layer="breadboard" terminalId="connector8terminal"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector8pin" layer="schematic" terminalId="connector8terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector8pin" layer="copper0"/>
     <p svgId="connector8pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector type="female" id="connector9" name="A3">
   <description>pin 10</description>
   <views>
    <breadboardView>
     <p svgId="connector9pin" layer="breadboard" terminalId="connector9terminal"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector9pin" layer="schematic" terminalId="connector9terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector9pin" layer="copper0"/>
     <p svgId="connector9pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector type="female" id="connector10" name="A4">
   <description>pin 11</description>
   <views>
    <breadboardView>
     <p svgId="connector10pin" layer="breadboard" terminalId="connector10terminal"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector10pin" layer="schematic" terminalId="connector10terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector10pin" layer="copper0"/>
     <p svgId="connector10pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector type="female" id="connector11" name="A5">
   <description>pin 12</description>
   <views>
    <breadboardView>
     <p svgId="connector11pin" layer="breadboard" terminalId="connector11terminal"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector11pin" layer="schematic" terminalId="connector11terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector11pin" layer="copper0"/>
     <p svgId="connector11pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector type="female" id="connector12" name="D0">
   <description>pin 13</description>
   <views>
    <breadboardView>
     <p svgId="connector12pin" layer="breadboard" terminalId="connector12terminal"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector12pin" layer="schematic" terminalId="connector12terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector12pin" layer="copper0"/>
     <p svgId="connector12pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector type="female" id="connector13" name="D1">
   <description>pin 14</description>
   <views>
    <breadboardView>
     <p svgId="connector13pin" layer="breadboard" terminalId="connector13terminal"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector13pin" layer="schematic" terminalId="connector13terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector13pin" layer="copper0"/>
     <p svgId="connector13pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector type="female" id="connector14" name="D2">
   <description>pin 15</description>
   <views>
    <breadboardView>
     <p svgId="connector14pin" layer="breadboard" terminalId="connector14terminal"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector14pin" layer="schematic" terminalId="connector14terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector14pin" layer="copper0"/>
     <p svgId="connector14pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector type="female" id="connector15" name="D3">
   <description>pin 16</description>
   <views>
    <breadboardView>
     <p svgId="connector15pin" layer="breadboard" terminalId="connector15terminal"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector15pin" layer="schematic" terminalId="connector15terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector15pin" layer="copper0"/>
     <p svgId="connector15pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector type="female" id="connector16" name="D4">
   <description>pin 17</description>
   <views>
    <breadboardView>
     <p svgId="connector16pin" layer="breadboard" terminalId="connector16terminal"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector16pin" layer="schematic" terminalId="connector16terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector16pin" layer="copper0"/>
     <p svgId="connector16pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector type="female" id="connector17" name="D5">
   <description>pin 18</description>
   <views>
    <breadboardView>
     <p svgId="connector17pin" layer="breadboard" terminalId="connector17terminal"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector17pin" layer="schematic" terminalId="connector17terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector17pin" layer="copper0"/>
     <p svgId="connector17pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector type="female" id="connector18" name="D6">
   <description>pin 19</description>
   <views>
    <breadboardView>
     <p svgId="connector18pin" layer="breadboard" terminalId="connector18terminal"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector18pin" layer="schematic" terminalId="connector18terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector18pin" layer="copper0"/>
     <p svgId="connector18pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector type="female" id="connector19" name="D7">
   <description>pin 20</description>
   <views>
    <breadboardView>
     <p svgId="connector19pin" layer="breadboard" terminalId="connector19terminal"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector19pin" layer="schematic" terminalId="connector19terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector19pin" layer="copper0"/>
     <p svgId="connector19pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector type="female" id="connector20" name="D8">
   <description>pin 21</description>
   <views>
    <breadboardView>
     <p svgId="connector20pin" layer="breadboard" terminalId="connector20terminal"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector20pin" layer="schematic" terminalId="connector20terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector20pin" layer="copper0"/>
     <p svgId="connector20pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector type="female" id="connector21" name="D9">
   <description>pin 22</description>
   <views>
    <breadboardView>
     <p svgId="connector21pin" layer="breadboard" terminalId="connector21terminal"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector21pin" layer="schematic" terminalId="connector21terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector21pin" layer="copper0"/>
     <p svgId="connector21pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector type="female" id="connector22" name="D10">
   <description>pin 23</description>
   <views>
    <breadboardView>
     <p svgId="connector22pin" layer="breadboard" terminalId="connector22terminal"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector22pin" layer="schematic" terminalId="connector22terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector22pin" layer="copper0"/>
     <p svgId="connector22pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector type="female" id="connector23" name="D11">
   <description>pin 24</description>
   <views>
    <breadboardView>
     <p svgId="connector23pin" layer="breadboard" terminalId="connector23terminal"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector23pin" layer="schematic" terminalId="connector23terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector23pin" layer="copper0"/>
     <p svgId="connector23pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector type="female" id="connector24" name="D12">
   <description>pin 25</description>
   <views>
    <breadboardView>
     <p svgId="connector24pin" layer="breadboard" terminalId="connector24terminal"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector24pin" layer="schematic" terminalId="connector24terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector24pin" layer="copper0"/>
     <p svgId="connector24pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector type="female" id="connector25" name="D13">
   <description>pin 26</description>
   <views>
    <breadboardView>
     <p svgId="connector25pin" layer="breadboard" terminalId="connector25terminal"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector25pin" layer="schematic" terminalId="connector25terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector25pin" layer="copper0"/>
     <p svgId="connector25pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector type="female" id="connector26" name="GND">
   <description>pin 27</description>
   <views>
    <breadboardView>
     <p svgId="connector26pin" layer="breadboard" terminalId="connector26terminal"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector26pin" layer="schematic" terminalId="connector26terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector26pin" layer="copper0"/>
     <p svgId="connector26pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector type="female" id="connector27" name="A">
   <description>pin 28</description>
   <views>
    <breadboardView>
     <p svgId="connector27pin" layer="breadboard" terminalId="connector27terminal"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector27pin" layer="schematic" terminalId="connector27terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector27pin" layer="copper0"/>
     <p svgId="connector27pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector type="female" id="connector28" name="D26">
   <description>pin 29</description>
   <views>
    <breadboardView>
     <p svgId="connector28pin" layer="breadboard" terminalId="connector28terminal"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector28pin" layer="schematic" terminalId="connector28terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector28pin" layer="copper0"/>
     <p svgId="connector28pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector type="female" id="connector29" name="D27">
   <description>pin 30</description>
   <views>
    <breadboardView>
     <p svgId="connector29pin" layer="breadboard" terminalId="connector29terminal"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector29pin" layer="schematic" terminalId="connector29terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector29pin" layer="copper0"/>
     <p svgId="connector29pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector type="female" id="connector30" name="D28">
   <description>pin 31</description>
   <views>
    <breadboardView>
     <p svgId="connector30pin" layer="breadboard" terminalId="connector30terminal"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector30pin" layer="schematic" terminalId="connector30terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector30pin" layer="copper0"/>
     <p svgId="connector30pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector type="female" id="connector31" name="D29">
   <description>pin 32</description>
   <views>
    <breadboardView>
     <p svgId="connector31pin" layer="breadboard" terminalId="connector31terminal"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector31pin" layer="schematic" terminalId="connector31terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector31pin" layer="copper0"/>
     <p svgId="connector31pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector type="female" id="connector32" name="D30">
   <description>pin 33</description>
   <views>
    <breadboardView>
     <p svgId="connector32pin" layer="breadboard" terminalId="connector32terminal"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector32pin" layer="schematic" terminalId="connector32terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector32pin" layer="copper0"/>
     <p svgId="connector32pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector type="female" id="connector33" name="D31">
   <description>pin 34</description>
   <views>
    <breadboardView>
     <p svgId="connector33pin" layer="breadboard" terminalId="connector33terminal"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector33pin" layer="schematic" terminalId="connector33terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector33pin" layer="copper0"/>
     <p svgId="connector33pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector type="female" id="connector34" name="D32">
   <description>pin 35</description>
   <views>
    <breadboardView>
     <p svgId="connector34pin" layer="breadboard" terminalId="connector34terminal"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector34pin" layer="schematic" terminalId="connector34terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector34pin" layer="copper0"/>
     <p svgId="connector34pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector type="female" id="connector35" name="D33">
   <description>pin 36</description>
   <views>
    <breadboardView>
     <p svgId="connector35pin" layer="breadboard" terminalId="connector35terminal"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector35pin" layer="schematic" terminalId="connector35terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector35pin" layer="copper0"/>
     <p svgId="connector35pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector type="female" id="connector36" name="D34">
   <description>pin 37</description>
   <views>
    <breadboardView>
     <p svgId="connector36pin" layer="breadboard" terminalId="connector36terminal"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector36pin" layer="schematic" terminalId="connector36terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector36pin" layer="copper0"/>
     <p svgId="connector36pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector type="female" id="connector37" name="D35">
   <description>pin 38</description>
   <views>
    <breadboardView>
     <p svgId="connector37pin" layer="breadboard" terminalId="connector37terminal"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector37pin" layer="schematic" terminalId="connector37terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector37pin" layer="copper0"/>
     <p svgId="connector37pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector type="female" id="connector38" name="D36">
   <description>pin 39</description>
   <views>
    <breadboardView>
     <p svgId="connector38pin" layer="breadboard" terminalId="connector38terminal"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector38pin" layer="schematic" terminalId="connector38terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector38pin" layer="copper0"/>
     <p svgId="connector38pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector type="female" id="connector39" name="D37">
   <description>pin 40</description>
   <views>
    <breadboardView>
     <p svgId="connector39pin" layer="breadboard" terminalId="connector39terminal"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector39pin" layer="schematic" terminalId="connector39terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector39pin" layer="copper0"/>
     <p svgId="connector39pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector type="female" id="connector40" name="D38">
   <description>pin 41</description>
   <views>
    <breadboardView>
     <p svgId="connector40pin" layer="breadboard" terminalId="connector40terminal"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector40pin" layer="schematic" terminalId="connector40terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector40pin" layer="copper0"/>
     <p svgId="connector40pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector type="female" id="connector41" name="D39">
   <description>pin 42</description>
   <views>
    <breadboardView>
     <p svgId="connector41pin" layer="breadboard" terminalId="connector41terminal"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector41pin" layer="schematic" terminalId="connector41terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector41pin" layer="copper0"/>
     <p svgId="connector41pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector type="female" id="connector42" name="D40">
   <description>pin 43</description>
   <views>
    <breadboardView>
     <p svgId="connector42pin" layer="breadboard" terminalId="connector42terminal"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector42pin" layer="schematic" terminalId="connector42terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector42pin" layer="copper0"/>
     <p svgId="connector42pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector type="female" id="connector43" name="D41">
   <description>pin 44</description>
   <views>
    <breadboardView>
     <p svgId="connector43pin" layer="breadboard" terminalId="connector43terminal"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector43pin" layer="schematic" terminalId="connector43terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector43pin" layer="copper0"/>
     <p svgId="connector43pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
 </connectors>
 <url>http://digilentinc.com/Products/Detail.cfm?NavPath=2,892,936&amp;Prod=CHIPKIT-BASIC-IO-SHIELD</url>
</module>
