<?xml version='1.0' encoding='UTF-8'?>
<module fritzingVersion="0.9.0b" moduleId="linino_dogrj45">
    <author>fabian_atlthaus</author>
    <title>linino dogRJ45</title>
    <label>linino dogRJ45</label>
    <date>2014-06-22</date>
    <url>http://www.linino.org/modules/linino-one/</url>
    <tags>
        <tag>linino</tag>
        <tag>addon</tag>
	<tag>ethernet</tag>
    <tag>rj45</tag>
    <tag>dog hunter</tag>
        <tag>microcontroller</tag>
    </tags>
    <properties>
        <property name="family">Microcontroller Board (linino)</property>
        <property name="processor"></property>
        <property name="variant">linino dogRJ45</property>
    </properties>
    <description>Designed to meet IEEE 802.3 Fast Ethernet switch with auto-crossover, auto-polarity, and auto-negotiation.
10/100 Mbps Fast Ethernet port basic switch feature including port mirroring, broadcast storm support, flow control in full-duplex, and back pressure in half duplex.</description>
    <views>
        <iconView>
            <layers image="icon/linino_one(rev1)_icon.svg">
                <layer layerId="icon"/>
            </layers>
        </iconView>
        <breadboardView>
            <layers image="breadboard/linino_dogrj45_breadboard.svg">
                <layer layerId="breadboard"/>
            </layers>
        </breadboardView>
        <schematicView>
            <layers image="schematic/linino_dogrj45_schematic.svg">
                <layer layerId="schematic"/>
            </layers>
        </schematicView>
        <pcbView>
            <layers image="pcb/linino_dogrj45_pcb.svg">
                <layer layerId="copper1"/>
                <layer layerId="copper0"/>
                <layer layerId="silkscreen"/>
            </layers>
        </pcbView>
    </views>
<connectors>
    <connector type="male" id="connector0" name="RX +">
            <description>RX +</description>
            <views>
                <breadboardView>
                    <p svgId="connector0pin" layer="breadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector0pin" layer="schematic" terminalId="connector0terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector0pin" layer="copper0"/>
                    <p svgId="connector0pin" layer="copper1"/>
                </pcbView>
            </views>
    </connector>
        <connector type="male" id="connector1" name="RX -">
            <description>RX -</description>
            <views>
                <breadboardView>
                    <p svgId="connector1pin" layer="breadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector1pin" layer="schematic" terminalId="connector1terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector1pin" layer="copper0"/>
                    <p svgId="connector1pin" layer="copper1"/>
                </pcbView>
            </views>
        </connector>
        <connector type="male" id="connector2" name="TX +">
            <description>TX +</description>
            <views>
                <breadboardView>
                    <p svgId="connector2pin" layer="breadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector2pin" layer="schematic" terminalId="connector2terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector2pin" layer="copper0"/>
                    <p svgId="connector2pin" layer="copper1"/>
                </pcbView>
            </views>
        </connector>
        <connector type="male" id="connector3" name="TX -">
            <description>TX -</description>
            <views>
                <breadboardView>
                    <p svgId="connector3pin" layer="breadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector3pin" layer="schematic" terminalId="connector3terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector3pin" layer="copper0"/>
                    <p svgId="connector3pin" layer="copper1"/>
                </pcbView>
            </views>
        </connector>
    
      
        <connector type="male" id="connector39" name="GND">
            <description>GND</description>
            <views>
                <breadboardView>
                    <p svgId="connector39pin" layer="breadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector39pin" layer="schematic" terminalId="connector39terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector39pin" layer="copper0"/>
                    <p svgId="connector39pin" layer="copper1"/>
                </pcbView>
            </views>
        </connector>
        <connector type="male" id="connector40" name="GND">
            <description>GND</description>
            <views>
                <breadboardView>
                    <p svgId="connector40pin" layer="breadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector40pin" layer="schematic" terminalId="connector40terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector40pin" layer="copper0"/>
                    <p svgId="connector40pin" layer="copper1"/>
                </pcbView>
            </views>
        </connector>
        <connector type="male" id="connector41" name="GND">
            <description>GND</description>
            <views>
                <breadboardView>
                    <p svgId="connector41pin" layer="breadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector41pin" layer="schematic" terminalId="connector41terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector41pin" layer="copper0"/>
                    <p svgId="connector41pin" layer="copper1"/>
                </pcbView>
            </views>
        </connector>
        <connector type="male" id="connector42" name="VCC_CT">
            <description>VCC_CT</description>
            <views>
                <breadboardView>
                    <p svgId="connector42pin" layer="breadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector42pin" layer="schematic" terminalId="connector42terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector42pin" layer="copper0"/>
                    <p svgId="connector42pin" layer="copper1"/>
                </pcbView>
            </views>           
        </connector>
        </connectors>
    <buses>
        <bus id="GND">
	<nodeMember connectorId="connector41"/>
	<nodeMember connectorId="connector40"/>
    <nodeMember connectorId="connector39"/>
        </bus>
   </buses>
</module>
