<?xml version='1.0' encoding='UTF-8'?>
<module fritzingVersion='0.5.2b.02.18.4756' moduleId='Op Amp Breakout-v16'>
<version>4</version>
<date>2011-07-08</date>
<author>SparkFun</author>
<description>&lt;p&gt;


	&lt;span style=&quot;font-weight: bold;&quot;&gt;Description:&lt;/span&gt; This is a simple Op Amp breakout board, set up as a 2-stage amplifier with a gain of 100 (gain of 10 for each stage). The on-board trim pot sets the signal level between the stages, not the feedback path. The bandwidth is set to 15.9kHz by a pair of feedback capacitors, or over 100kHz with the caps removed. The LMV358 opamp can source up to 160mA and works well as a low impedance driver/buffer.&lt;br /&gt;


	&lt;br /&gt;


	&lt;span style=&quot;font-weight: bold;&quot;&gt;Documents:&lt;/span&gt;&lt;/p&gt;


&lt;ul&gt;


	&lt;li&gt;


		&lt;a href=&quot;http://www.sparkfun.com/datasheets/BreakoutBoards/OpAmp_Breakout-v16.pdf&quot; target=&quot;_blank&quot;&gt;Schematic&lt;/a&gt;&lt;/li&gt;


	&lt;li&gt;


		&lt;a href=&quot;http://focus.ti.com/lit/ds/symlink/lmv324.pdf&quot; target=&quot;_blank&quot;&gt;LMV358 datasheet&lt;/a&gt;&lt;/li&gt;


	&lt;li&gt;


		&lt;a href=&quot;http://www.sparkfun.com/datasheets/BreakoutBoards/OpAmp_Breakout-v16.zip&quot; target=&quot;_blank&quot;&gt;Eagle Files&lt;/a&gt;&lt;/li&gt;


&lt;/ul&gt;


&lt;p&gt;


	&lt;strong&gt;Replaces: &lt;/strong&gt;&lt;a href=&quot;http://www.sparkfun.com/commerce/product_info.php?products_id=8704&quot;&gt;BOB-08704&lt;/a&gt;&lt;/p&gt;</description>
<title>OpAmp Breakout</title>
<url>http://www.sparkfun.com/products/9816</url>
<tags>
<tag>Opamp</tag>
<tag>Amplifier</tag>
<tag>Operational</tag>
<tag>Amp</tag>
</tags>
<properties>
<property name='family'>Amplifier Breakout</property>
</properties>
<views>
<breadboardView>
<layers image='breadboard/Op Amp Breakout-v16_breadboard.svg'>
<layer layerId='breadboard'/>
</layers>
</breadboardView>
<schematicView>
<layers image='schematic/Op Amp Breakout-v16_schematic.svg'>
<layer layerId='schematic'/>
</layers>
</schematicView>
<pcbView>
<layers image='pcb/Op Amp Breakout-v16_pcb.svg'>
<layer layerId='copper1'/>
<layer layerId='silkscreen'/>
<layer layerId='copper0'/>
</layers>
</pcbView>
<iconView>
<layers image='breadboard/Op Amp Breakout-v16_breadboard.svg'>
<layer layerId='icon'/>
</layers>
</iconView>
</views>
<connectors>
<connector id='connector20' type='male' name='VCC'>
<description>VCC</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector20pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector20pin' terminalId='connector20terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector20pad'/><p layer='copper1' svgId='connector20pad'/></pcbView>
</views>
</connector>
<connector id='connector21' type='male' name='GND'>
<description>GND</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector21pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector21pin' terminalId='connector21terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector21pad'/><p layer='copper1' svgId='connector21pad'/></pcbView>
</views>
</connector>
<connector id='connector22' type='male' name='OUT'>
<description>OUT</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector22pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector22pin' terminalId='connector22terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector22pad'/><p layer='copper1' svgId='connector22pad'/></pcbView>
</views>
</connector>
<connector id='connector23' type='male' name='IN'>
<description>IN</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector23pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector23pin' terminalId='connector23terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector23pad'/><p layer='copper1' svgId='connector23pad'/></pcbView>
</views>
</connector>
</connectors>
<buses>
</buses>
</module>
