<?xml version='1.0' encoding='UTF-8'?>
<module referenceFile="dquidio.fzp" moduleId="dquidio">
 <version>4</version>
<author>fabian althaus</author>
 <title>dquidio board</title>
 <label>Microcontroller </label>
 <date>Fr Jan 9 2015</date>
 <tags>
  <tag>Microcontroller</tag>
  <tag>fritzing core</tag>
 </tags>
 <properties>
  <property name="part number"></property>
  <property name="variant">Dquid IO</property>
  <property name="family">Microcontrollerboard (DquidIO)</property>
  <property name="layer"></property>
  <property name="package">Bluethoot Wlan</property>
 </properties>
 <taxonomy>microcontroller</taxonomy>
 <description>the dquidio board. for more information visit:
http://www.dquid.com/landing/dquid-io</description>
 <views>
  <iconView>
   <layers image="icon/dquidio_icon.svg">
    <layer layerId="icon"/>
   </layers>
  </iconView>
  <breadboardView>
   <layers image="breadboard/dquidio_breadboard.svg">
    <layer layerId="breadboard"/>
   </layers>
  </breadboardView>
  <schematicView>
   <layers image="schematic/dquidio_schematic.svg">
    <layer layerId="schematic"/>
   </layers>
  </schematicView>
  <pcbView>
   <layers image="pcb/dquidio_pcb.svg">
    <layer layerId="silkscreen"/>
    <layer layerId="copper0"/>
    <layer layerId="copper1"/>
   </layers>
  </pcbView>
 </views>
 <connectors>
  <connector type="male" id="connector0" name="12V_Input">
   <description>pin 1 - User 12V – Input</description>
   <views>
    <breadboardView>
     <p svgId="connector0pin" terminalId="connector0terminal" layer="breadboard"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector0pin" terminalId="connector0terminal" layer="schematic"/>
    </schematicView>
    <pcbView>
     <p svgId="connector0pin" layer="copper0"/>
     <p svgId="connector0pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector type="male" id="connector1" name="5V_Output">
   <description>pin 2 - 5V- Output</description>
   <views>
    <breadboardView>
     <p svgId="connector1pin" terminalId="connector1terminal" layer="breadboard"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector1pin" terminalId="connector1terminal" layer="schematic"/>
    </schematicView>
    <pcbView>
     <p svgId="connector1pin" layer="copper0"/>
     <p svgId="connector1pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector type="male" id="connector2" name="RS-232 Rx">
   <description>pin 3 - to be managed via Firmware</description>
   <views>
    <breadboardView>
     <p svgId="connector2pin" terminalId="connector2terminal" layer="breadboard"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector2pin" terminalId="connector2terminal" layer="schematic"/>
    </schematicView>
    <pcbView>
     <p svgId="connector2pin" layer="copper0"/>
     <p svgId="connector2pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector type="male" id="connector3" name="RS-232 Tx">
   <description>pin 4 - to be managed via Firmware</description>
   <views>
    <breadboardView>
     <p svgId="connector3pin" terminalId="connector3terminal" layer="breadboard"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector3pin" terminalId="connector3terminal" layer="schematic"/>
    </schematicView>
    <pcbView>
     <p svgId="connector3pin" layer="copper0"/>
     <p svgId="connector3pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector type="male" id="connector4" name="GND">
   <description>pin 5 - GND</description>
   <views>
    <breadboardView>
     <p svgId="connector4pin" terminalId="connector4terminal" layer="breadboard"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector4pin" terminalId="connector4terminal" layer="schematic"/>
    </schematicView>
    <pcbView>
     <p svgId="connector4pin" layer="copper0"/>
     <p svgId="connector4pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector type="male" id="connector5" name="GND">
   <description>pin 6 - GND</description>
   <views>
    <breadboardView>
     <p svgId="connector5pin" terminalId="connector5terminal" layer="breadboard"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector5pin" terminalId="connector5terminal" layer="schematic"/>
    </schematicView>
    <pcbView>
     <p svgId="connector5pin" layer="copper0"/>
     <p svgId="connector5pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector type="male" id="connector6" name="GND">
   <description>pin 7 - GND</description>
   <views>
    <breadboardView>
     <p svgId="connector6pin" terminalId="connector6terminal" layer="breadboard"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector6pin" terminalId="connector6terminal" layer="schematic"/>
    </schematicView>
    <pcbView>
     <p svgId="connector6pin" layer="copper0"/>
     <p svgId="connector6pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector type="male" id="connector7" name="GND">
   <description>pin 8 - GND</description>
   <views>
    <breadboardView>
     <p svgId="connector7pin" terminalId="connector7terminal" layer="breadboard"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector7pin" terminalId="connector7terminal" layer="schematic"/>
    </schematicView>
    <pcbView>
     <p svgId="connector7pin" layer="copper0"/>
     <p svgId="connector7pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector type="male" id="connector8" name="I2C_SCL">
   <description>pin 9 - to be managed via Firmware</description>
   <views>
    <breadboardView>
     <p svgId="connector8pin" terminalId="connector8terminal" layer="breadboard"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector8pin" terminalId="connector8terminal" layer="schematic"/>
    </schematicView>
    <pcbView>
     <p svgId="connector8pin" layer="copper0"/>
     <p svgId="connector8pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector type="male" id="connector9" name="I2C_SDA">
   <description>pin 10 - to be managed via Firmware</description>
   <views>
    <breadboardView>
     <p svgId="connector9pin" terminalId="connector9terminal" layer="breadboard"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector9pin" terminalId="connector9terminal" layer="schematic"/>
    </schematicView>
    <pcbView>
     <p svgId="connector9pin" layer="copper0"/>
     <p svgId="connector9pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector type="male" id="connector10" name="UART Tx">
   <description>pin 11 - to be managed via Firmware</description>
   <views>
    <breadboardView>
     <p svgId="connector10pin" terminalId="connector10terminal" layer="breadboard"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector10pin" terminalId="connector10terminal" layer="schematic"/>
    </schematicView>
    <pcbView>
     <p svgId="connector10pin" layer="copper0"/>
     <p svgId="connector10pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector type="male" id="connector11" name="UART Rx">
   <description>pin 12 - to be managed via Firmware</description>
   <views>
    <breadboardView>
     <p svgId="connector11pin" terminalId="connector11terminal" layer="breadboard"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector11pin" terminalId="connector11terminal" layer="schematic"/>
    </schematicView>
    <pcbView>
     <p svgId="connector11pin" layer="copper0"/>
     <p svgId="connector11pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector type="male" id="connector12" name="OUTPUT 1">
   <description>pin 13 - can be configured via DQuid APP</description>
   <views>
    <breadboardView>
     <p svgId="connector12pin" terminalId="connector12terminal" layer="breadboard"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector12pin" terminalId="connector12terminal" layer="schematic"/>
    </schematicView>
    <pcbView>
     <p svgId="connector12pin" layer="copper0"/>
     <p svgId="connector12pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector type="male" id="connector13" name="OUTPUT 2">
   <description>pin 14 - can be configured via DQuid APP</description>
   <views>
    <breadboardView>
     <p svgId="connector13pin" terminalId="connector13terminal" layer="breadboard"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector13pin" terminalId="connector13terminal" layer="schematic"/>
    </schematicView>
    <pcbView>
     <p svgId="connector13pin" layer="copper0"/>
     <p svgId="connector13pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector type="male" id="connector14" name="OUTPUT 3">
   <description>pin 15 - can be configured via DQuid APP</description>
   <views>
    <breadboardView>
     <p svgId="connector14pin" terminalId="connector14terminal" layer="breadboard"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector14pin" terminalId="connector14terminal" layer="schematic"/>
    </schematicView>
    <pcbView>
     <p svgId="connector14pin" layer="copper0"/>
     <p svgId="connector14pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector type="male" id="connector15" name="OUTPUT 4">
   <description>pin 16 - can be configured via DQuid APP</description>
   <views>
    <breadboardView>
     <p svgId="connector15pin" terminalId="connector15terminal" layer="breadboard"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector15pin" terminalId="connector15terminal" layer="schematic"/>
    </schematicView>
    <pcbView>
     <p svgId="connector15pin" layer="copper0"/>
     <p svgId="connector15pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector type="male" id="connector16" name="INPUT 1">
   <description>pin 17 - can be configured via DQuid APP</description>
   <views>
    <breadboardView>
     <p svgId="connector16pin" terminalId="connector16terminal" layer="breadboard"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector16pin" terminalId="connector16terminal" layer="schematic"/>
    </schematicView>
    <pcbView>
     <p svgId="connector16pin" layer="copper0"/>
     <p svgId="connector16pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector type="male" id="connector17" name="INPUT 2">
   <description>pin 18 - can be configured via DQuid APP</description>
   <views>
    <breadboardView>
     <p svgId="connector17pin" terminalId="connector17terminal" layer="breadboard"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector17pin" terminalId="connector17terminal" layer="schematic"/>
    </schematicView>
    <pcbView>
     <p svgId="connector17pin" layer="copper0"/>
     <p svgId="connector17pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector type="male" id="connector18" name="INPUT 3">
   <description>pin 19 - can be configured via DQuid APP</description>
   <views>
    <breadboardView>
     <p svgId="connector18pin" terminalId="connector18terminal" layer="breadboard"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector18pin" terminalId="connector18terminal" layer="schematic"/>
    </schematicView>
    <pcbView>
     <p svgId="connector18pin" layer="copper0"/>
     <p svgId="connector18pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector type="male" id="connector19" name="INPUT 4">
   <description>pin 20 - can be configured via DQuid APP</description>
   <views>
    <breadboardView>
     <p svgId="connector19pin" terminalId="connector19terminal" layer="breadboard"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector19pin" terminalId="connector19terminal" layer="schematic"/>
    </schematicView>
    <pcbView>
     <p svgId="connector19pin" layer="copper0"/>
     <p svgId="connector19pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector type="male" id="connector20" name="pin21">
   <description>pin 21</description>
   <views>
    <breadboardView>
     <p svgId="connector20pin" terminalId="connector20terminal" layer="breadboard"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector20pin" terminalId="connector20terminal" layer="schematic"/>
    </schematicView>
    <pcbView>
     <p svgId="connector20pin" layer="copper0"/>
     <p svgId="connector20pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector type="male" id="connector21" name="pin22">
   <description>pin 22</description>
   <views>
    <breadboardView>
     <p svgId="connector21pin" terminalId="connector21terminal" layer="breadboard"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector21pin" terminalId="connector21terminal" layer="schematic"/>
    </schematicView>
    <pcbView>
     <p svgId="connector21pin" layer="copper0"/>
     <p svgId="connector21pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector type="male" id="connector22" name="pin23">
   <description>pin 23</description>
   <views>
    <breadboardView>
     <p svgId="connector22pin" terminalId="connector22terminal" layer="breadboard"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector22pin" terminalId="connector22terminal" layer="schematic"/>
    </schematicView>
    <pcbView>
     <p svgId="connector22pin" layer="copper0"/>
     <p svgId="connector22pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector type="male" id="connector23" name="pin24">
   <description>pin 24</description>
   <views>
    <breadboardView>
     <p svgId="connector23pin" terminalId="connector23terminal" layer="breadboard"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector23pin" terminalId="connector23terminal" layer="schematic"/>
    </schematicView>
    <pcbView>
     <p svgId="connector23pin" layer="copper0"/>
     <p svgId="connector23pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector type="male" id="connector24" name="pin25">
   <description>pin 25</description>
   <views>
    <breadboardView>
     <p svgId="connector24pin" terminalId="connector24terminal" layer="breadboard"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector24pin" terminalId="connector24terminal" layer="schematic"/>
    </schematicView>
    <pcbView>
     <p svgId="connector24pin" layer="copper0"/>
     <p svgId="connector24pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector type="male" id="connector25" name="pin26">
   <description>pin 26</description>
   <views>
    <breadboardView>
     <p svgId="connector25pin" terminalId="connector25terminal" layer="breadboard"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector25pin" terminalId="connector25terminal" layer="schematic"/>
    </schematicView>
    <pcbView>
     <p svgId="connector25pin" layer="copper0"/>
     <p svgId="connector25pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector type="male" id="connector26" name="pin27">
   <description>pin 27</description>
   <views>
    <breadboardView>
     <p svgId="connector26pin" terminalId="connector26terminal" layer="breadboard"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector26pin" terminalId="connector26terminal" layer="schematic"/>
    </schematicView>
    <pcbView>
     <p svgId="connector26pin" layer="copper0"/>
     <p svgId="connector26pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector type="male" id="connector27" name="pin28">
   <description>pin 28</description>
   <views>
    <breadboardView>
     <p svgId="connector27pin" terminalId="connector27terminal" layer="breadboard"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector27pin" terminalId="connector27terminal" layer="schematic"/>
    </schematicView>
    <pcbView>
     <p svgId="connector27pin" layer="copper0"/>
     <p svgId="connector27pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector type="male" id="connector28" name="pin29">
   <description>pin 29</description>
   <views>
    <breadboardView>
     <p svgId="connector28pin" terminalId="connector28terminal" layer="breadboard"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector28pin" terminalId="connector28terminal" layer="schematic"/>
    </schematicView>
    <pcbView>
     <p svgId="connector28pin" layer="copper0"/>
     <p svgId="connector28pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector type="male" id="connector29" name="pin30">
   <description>pin 30</description>
   <views>
    <breadboardView>
     <p svgId="connector29pin" terminalId="connector29terminal" layer="breadboard"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector29pin" terminalId="connector29terminal" layer="schematic"/>
    </schematicView>
    <pcbView>
     <p svgId="connector29pin" layer="copper0"/>
     <p svgId="connector29pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector type="male" id="connector30" name="pin31">
   <description>pin 31</description>
   <views>
    <breadboardView>
     <p svgId="connector30pin" terminalId="connector30terminal" layer="breadboard"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector30pin" terminalId="connector30terminal" layer="schematic"/>
    </schematicView>
    <pcbView>
     <p svgId="connector30pin" layer="copper0"/>
     <p svgId="connector30pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector type="male" id="connector31" name="pin32">
   <description>pin 32</description>
   <views>
    <breadboardView>
     <p svgId="connector31pin" terminalId="connector31terminal" layer="breadboard"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector31pin" terminalId="connector31terminal" layer="schematic"/>
    </schematicView>
    <pcbView>
     <p svgId="connector31pin" layer="copper0"/>
     <p svgId="connector31pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector type="male" id="connector32" name="pin33">
   <description>pin 33</description>
   <views>
    <breadboardView>
     <p svgId="connector32pin" terminalId="connector32terminal" layer="breadboard"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector32pin" terminalId="connector32terminal" layer="schematic"/>
    </schematicView>
    <pcbView>
     <p svgId="connector32pin" layer="copper0"/>
     <p svgId="connector32pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector type="male" id="connector33" name="pin34">
   <description>pin 34</description>
   <views>
    <breadboardView>
     <p svgId="connector33pin" terminalId="connector33terminal" layer="breadboard"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector33pin" terminalId="connector33terminal" layer="schematic"/>
    </schematicView>
    <pcbView>
     <p svgId="connector33pin" layer="copper0"/>
     <p svgId="connector33pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector type="male" id="connector34" name="pin35">
   <description>pin 35</description>
   <views>
    <breadboardView>
     <p svgId="connector34pin" terminalId="connector34terminal" layer="breadboard"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector34pin" terminalId="connector34terminal" layer="schematic"/>
    </schematicView>
    <pcbView>
     <p svgId="connector34pin" layer="copper0"/>
     <p svgId="connector34pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector type="male" id="connector35" name="pin36">
   <description>pin 36</description>
   <views>
    <breadboardView>
     <p svgId="connector35pin" terminalId="connector35terminal" layer="breadboard"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector35pin" terminalId="connector35terminal" layer="schematic"/>
    </schematicView>
    <pcbView>
     <p svgId="connector35pin" layer="copper0"/>
     <p svgId="connector35pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector type="male" id="connector36" name="pin37">
   <description>pin 37</description>
   <views>
    <breadboardView>
     <p svgId="connector36pin" terminalId="connector36terminal" layer="breadboard"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector36pin" terminalId="connector36terminal" layer="schematic"/>
    </schematicView>
    <pcbView>
     <p svgId="connector36pin" layer="copper0"/>
     <p svgId="connector36pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector type="male" id="connector37" name="pin38">
   <description>pin 38</description>
   <views>
    <breadboardView>
     <p svgId="connector37pin" terminalId="connector37terminal" layer="breadboard"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector37pin" terminalId="connector37terminal" layer="schematic"/>
    </schematicView>
    <pcbView>
     <p svgId="connector37pin" layer="copper0"/>
     <p svgId="connector37pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector type="male" id="connector38" name="pin39">
   <description>pin 39</description>
   <views>
    <breadboardView>
     <p svgId="connector38pin" terminalId="connector38terminal" layer="breadboard"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector38pin" terminalId="connector38terminal" layer="schematic"/>
    </schematicView>
    <pcbView>
     <p svgId="connector38pin" layer="copper0"/>
     <p svgId="connector38pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector type="male" id="connector39" name="pin40">
   <description>pin 40</description>
   <views>
    <breadboardView>
     <p svgId="connector39pin" terminalId="connector39terminal" layer="breadboard"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector39pin" terminalId="connector39terminal" layer="schematic"/>
    </schematicView>
    <pcbView>
     <p svgId="connector39pin" layer="copper0"/>
     <p svgId="connector39pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
 </connectors>
<buses>
<bus id='gnd'>
<nodeMember connectorId='connector4'/>
<nodeMember connectorId='connector5'/>
<nodeMember connectorId='connector6'/>
<nodeMember connectorId='connector7'/>
</bus>
</buses>
</module>
