<?xml version="1.0" encoding="UTF-8"?><module fritzingVersion="0.7.2b" moduleId="SparkFun-Connectors-USB_AB-">
<!-- generated from Sparkfun Eagle Library 'SparkFun-Connectors' USB_AB  -->
<version>4</version>
<date>2013-02-13</date>
<label>U</label>
<author>www.fritzing.org</author>
<description>This is a USB AB connector that is compatible with USB OTG. i.e. this connector can serve as a host or device</description>
<title>USB_AB</title>
<tags>
<tag>USB_AB</tag>
<tag>USB-AB-MICRO-SMD</tag>
</tags>
<properties>
<property name="package">usb-ab-micro-smd</property>
<property name="family">sparkfun USB Connector</property>
</properties>
<views>
<breadboardView>
<layers image="breadboard/sparkfun-connectors_usb-ab-micro-smd_breadboard.svg">
<layer layerId="breadboard"/>
</layers>
</breadboardView>
<schematicView>
<layers image="schematic/sparkfun-connectors_usb_ab_schematic.svg">
<layer layerId="schematic"/>
</layers>
</schematicView>
<pcbView>
<layers image="pcb/sparkfun-connectors_usb-ab-micro-smd_pcb.svg">
<layer layerId="copper1"/>
<layer layerId="silkscreen"/>
</layers>
</pcbView>
<iconView>
<layers image="icon/usb-ab-micro-smd.svg">
<layer layerId="icon"/>
</layers>
</iconView>
</views>
<connectors>
<connector id="connector4" name="D+" type="male">
<description>D+</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector4pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector4pin" terminalId="connector4terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector4pad"/>
</pcbView>
</views>
</connector>
<connector id="connector5" name="D-" type="male">
<description>D-</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector5pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector5pin" terminalId="connector5terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector5pad"/>
</pcbView>
</views>
</connector>
<connector id="connector6" name="GND" type="male">
<description>GND</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector6pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector6pin" terminalId="connector6terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector6pad"/>
</pcbView>
</views>
</connector>
<connector id="connector7" name="USBID" type="male">
<description>USBID</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector7pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector7pin" terminalId="connector7terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector7pad"/>
</pcbView>
</views>
</connector>
<connector id="connector8" name="VBUS" type="male">
<description>VBUS</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector8pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector8pin" terminalId="connector8terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector8pad"/>
</pcbView>
</views>
</connector>
</connectors>
<buses>
</buses>
</module>