<?xml version="1.0" encoding="UTF-8"?>
<module fritzingVersion="0.5.2b.02.18.4756" moduleId="297c7ab01279c7b7f5c4ca77ec94554c">
    <version>4</version>
    <author>Dirk van Oosterbosch</author>
    <title>Dial Potentiometer with switch</title>
    <label>R</label>
    <date>2010-02-10</date>
    <tags>
        <tag>potentiometer</tag>
        <tag>poti</tag>
        <tag>adjustable</tag>
        <tag>resistor</tag>
        <tag>switch</tag>
        <tag>thumb wheel</tag>
        <tag>dial</tag>
    </tags>
    <properties>
        <property name="size">Dial - 25mm</property>
        <property name="family">Potentiometer</property>
        <property name="track">Logarithmic</property>
        <property name="type">Thumb Wheel Potentiometer with switch</property>
        <property name="maximum resistance">10kΩ</property>
    </properties>
    <description>A thumb wheel adjustable resistor (potentiometer) with internal swith.</description>
    <views>
        <iconView>
            <layers image="icon/Dial_Potentiometer_with_switch.svg">
                <layer layerId="icon"/>
            </layers>
        </iconView>
        <breadboardView>
            <layers image="breadboard/potentiometer_w_switch.svg">
                <layer layerId="breadboard"/>
            </layers>
        </breadboardView>
        <schematicView fliphorizontal="true">
            <layers image="schematic/Dial_Potentiometer_with_switch_schematic.svg">
                <layer layerId="schematic"/>
            </layers>
        </schematicView>
        <pcbView>
            <layers image="pcb/Dial_Potentiometer_with_switch_pcb.svg">
                <layer layerId="copper0"/>
                <layer layerId="silkscreen"/>
                <layer layerId="copper1"/>
            </layers>
        </pcbView>
    </views>
    <connectors>
        <connector id="connector3" type="male" name="switch leg1">
            <description>leg 1 of switch</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector3pin" terminalId="connector3terminal"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector3pin" terminalId="connector3terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper1" svgId="connector3pin"/>
                    <p layer="copper0" svgId="connector3pin"/>
                </pcbView>
            </views>
        </connector>
        <connector id="connector4" type="male" name="switch leg2">
            <description>leg 2 of switch</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector4pin" terminalId="connector4terminal"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector4pin" terminalId="connector4terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper1" svgId="connector4pin"/>
                    <p layer="copper0" svgId="connector4pin"/>
                </pcbView>
            </views>
        </connector>
        <connector id="connector0" type="male" name="leg1">
            <description>leg1</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector0pin"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector0pin" terminalId="connector0terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper0" svgId="connector0pin"/>
                    <p layer="copper1" svgId="connector0pin"/>
                </pcbView>
            </views>
        </connector>
        <connector id="connector1" type="male" name="wiper">
            <description>wiper</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector1pin"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector1pin" terminalId="connector1terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper0" svgId="connector1pin"/>
                    <p layer="copper1" svgId="connector1pin"/>
                </pcbView>
            </views>
        </connector>
        <connector id="connector2" type="male" name="leg2">
            <description>leg2</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector2pin"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector2pin" terminalId="connector2terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper0" svgId="connector2pin"/>
                    <p layer="copper1" svgId="connector2pin"/>
                </pcbView>
            </views>
        </connector>
    </connectors>
</module>
