<?xml version="1.0" encoding="UTF-8"?><module fritzingVersion="0.1.1255" moduleId="ALPS_STEC12E07">
 <version replacedby="alps_stec12e07_fix">4</version>
 <author>Stefan Hermann</author>
 <title>Rotary Encoder</title>
 <label>RE</label>
 <date>2011-09-15</date>
 <tags>
  <tag>Rotary</tag>
  <tag>Encoder</tag>
  <tag>digital</tag>
	<tag>input</tag>
  <tag>fritzing core</tag>
 </tags>
 <properties>
  <property name="family">//obsolete// rotary encoder</property>	
  <property name="package">THT</property>
  <property name="type">ALPS STEC12E07</property>
 </properties>
 <description>Rotary Encoder from ALPS STEC12E07.</description>
 <views>
  <iconView>
   <layers image="icon/Rotary_Encoder.svg">
    <layer layerId="icon"/>
   </layers>
  </iconView>
  <breadboardView>
   <layers image="breadboard/Rotary_Encoder.svg">
    <layer layerId="breadboard"/>
   </layers>
  </breadboardView>
  <schematicView fliphorizontal="false" flipvertical="false">
   <layers image="schematic/Rotary_Encoder.svg">
    <layer layerId="schematic"/>
   </layers>
  </schematicView>
  <pcbView>
   <layers image="pcb/Rotary_Encoder.svg">
    <layer layerId="copper0"/>
    <layer layerId="silkscreen"/>
   <layer layerId="copper1"/>
   </layers>
  </pcbView>
 </views>
 <connectors>
  <connector id="connector0" name="EncoderPinA" type="male">
   <description>output Pin A</description>
   <views>
    <breadboardView>
     <p layer="breadboard" svgId="connector0pin" terminalId="connector0terminal"/>
    </breadboardView>
    <schematicView>
     <p layer="schematic" svgId="connector0pin" terminalId="connector0terminal"/>
    </schematicView>
    <pcbView>
     <p layer="copper0" svgId="connector0pad"/>
    <p layer="copper1" svgId="connector0pad"/>
    </pcbView>
   </views>
  </connector>
  <connector id="connector1" name="EncoderPinC" type="male">
   <description>common Pin C</description>
   <views>
    <breadboardView>
     <p layer="breadboard" svgId="connector1pin" terminalId="connector1terminal"/>
    </breadboardView>
    <schematicView>
     <p layer="schematic" svgId="connector1pin" terminalId="connector1terminal"/>
    </schematicView>
    <pcbView>
     <p layer="copper0" svgId="connector1pad"/>
    <p layer="copper1" svgId="connector1pad"/>
    </pcbView>
   </views>
  </connector>
	<connector id="connector2" name="EncoderPinB" type="male">
   <description>output Pin B</description>
   <views>
    <breadboardView>
     <p layer="breadboard" svgId="connector2pin" terminalId="connector2terminal"/>
    </breadboardView>
    <schematicView>
     <p layer="schematic" svgId="connector2pin" terminalId="connector2terminal"/>
    </schematicView>
    <pcbView>
     <p layer="copper0" svgId="connector2pad"/>
    <p layer="copper1" svgId="connector2pad"/>
    </pcbView>
   </views>
  </connector>

 </connectors>
</module>
