<?xml version="1.0" encoding="UTF-8"?>
<module fritzingVersion="0.6.3b.08.16.5401" moduleId="fuse_with_handler_cff5">
    <author>Carlos Hansen</author>
    <title>Fuse with Handler</title>
    <label>Fuse</label>
    <date>2011-11-16</date>
    <tags>
        <tag>Fuse</tag>
        <tag>FuseHandler</tag>
        <tag>HTC-15m</tag>
        <tag>Bussmann</tag>
        <tag>protection</tag>
    </tags>
    <properties>
        <property name="Manufacturer">Bussmann</property>
        <property name="family">Fuse</property>
        <property name="Part Number">Htc-15m</property>
        <property name="Datasheet">http://www1.cooperbussmann.com/pdf/d5543d84-3b93-45e2-afde-4a74ca0255f9.pdf</property>
        <property name="Size">5 x 20 mm</property>
    </properties>
    <description>Device used to protect against excessive current.</description>
    <views>
        <iconView>
            <layers image="icon/Fuse_with_Handler_icon.svg">
                <layer layerId="breadboard"/>
                <layer layerId="icon"/>
            </layers>
        </iconView>
        <breadboardView>
            <layers image="breadboard/Fuse_with_Handler_breadboard.svg">
                <layer layerId="breadboard"/>
            </layers>
        </breadboardView>
        <schematicView>
            <layers image="schematic/Fuse_with_Handler_schematic.svg">
                <layer layerId="schematic"/>
            </layers>
        </schematicView>
        <pcbView>
            <layers image="pcb/Fuse_with_Handler_pcb.svg">
                <layer layerId="copper0"/>
                <layer layerId="copper1"/>
                <layer layerId="silkscreen"/>
            </layers>
        </pcbView>
    </views>
    <connectors>
        <connector id="connector0" type="male" name="Connector1">
            <description>Connector</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector0pin" legId="connector0leg"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector0pin" terminalId="connector0terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper1" svgId="connector0pin"/>
                    <p layer="copper0" svgId="connector0pin"/>
                </pcbView>
            </views>
        </connector>
        <connector id="connector1" type="male" name="Connector2">
            <description>Connector</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector1pin" legId="connector1leg"/>									
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector1pin" terminalId="connector1terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper1" svgId="connector1pin"/>
                    <p layer="copper0" svgId="connector1pin"/>
                </pcbView>
            </views>
        </connector>
    </connectors>
</module>
