<?xml version='1.0' encoding='UTF-8'?>
<module fritzingVersion="0.9.0b" moduleId="linino_one_rev1">
    <author>fabian_atlthaus</author>
    <title>linino one</title>
    <label>linino one</label>
    <date>2014-06-22</date>
    <url>http://www.linino.org/modules/linino-one/</url>
    <tags>
        <tag>linino</tag>
	<tag>one</tag>
	<tag>wifi</tag>
        <tag>microcontroller</tag>
    </tags>
    <properties>
        <property name="family">Microcontroller Board (linino)</property>
        <property name="processor">AT32u4</property>
        <property name="variant">linino one (rev1)</property>
    </properties>
    <description>The Linino &#8482; ONE  is a MIPS board based on the Atheros AR9331 and the ATmega32u4 (datasheet). The Atheros processor supports Linino, a Linux distribution based on OpenWRT. The board has built-in WiFi support,  20 digital input/output pins (of which 7 can be used as PWM outputs and 12 as analog inputs), a 16 MHz crystal oscillator, a micro USB connection, an ICSP header, 2 reset buttons and 1 user button.</description>
    <views>
        <iconView>
            <layers image="icon/linino_one(rev1)_icon.svg">
                <layer layerId="icon"/>
            </layers>
        </iconView>
        <breadboardView>
            <layers image="breadboard/linino_one(rev1)_breadboard.svg">
                <layer layerId="breadboard"/>
            </layers>
        </breadboardView>
        <schematicView>
            <layers image="schematic/linino_one(rev1)_schematic.svg">
                <layer layerId="schematic"/>
            </layers>
        </schematicView>
        <pcbView>
            <layers image="pcb/linino_one(rev1)_pcb.svg">
                <layer layerId="copper1"/>
                <layer layerId="copper0"/>
                <layer layerId="silkscreen"/>
            </layers>
        </pcbView>
    </views>
<connectors>
    <connector type="male" id="connector0" name="RD +">
            <description>RD+</description>
            <views>
                <breadboardView>
                    <p svgId="connector0pin" layer="breadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector0pin" layer="schematic" terminalId="connector0terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector0pin" layer="copper0"/>
                    <p svgId="connector0pin" layer="copper1"/>
                </pcbView>
            </views>
    </connector>
        <connector type="male" id="connector1" name="RD -">
            <description>RD-</description>
            <views>
                <breadboardView>
                    <p svgId="connector1pin" layer="breadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector1pin" layer="schematic" terminalId="connector1terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector1pin" layer="copper0"/>
                    <p svgId="connector1pin" layer="copper1"/>
                </pcbView>
            </views>
        </connector>
        <connector type="male" id="connector2" name="TD +">
            <description>TD+</description>
            <views>
                <breadboardView>
                    <p svgId="connector2pin" layer="breadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector2pin" layer="schematic" terminalId="connector2terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector2pin" layer="copper0"/>
                    <p svgId="connector2pin" layer="copper1"/>
                </pcbView>
            </views>
        </connector>
        <connector type="male" id="connector3" name="TD -">
            <description>TD-</description>
            <views>
                <breadboardView>
                    <p svgId="connector3pin" layer="breadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector3pin" layer="schematic" terminalId="connector3terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector3pin" layer="copper0"/>
                    <p svgId="connector3pin" layer="copper1"/>
                </pcbView>
            </views>
        </connector>
    
        <connector type="male" id="connector4" name="AR_Vin">
            <description>AR_VIN</description>
            <views>
                <breadboardView>
                    <p svgId="connector4pin" layer="breadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector4pin" layer="schematic" terminalId="connector4terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector4pin" layer="copper0"/>
                    <p svgId="connector4pin" layer="copper1"/>
                </pcbView>
            </views>
        </connector>
     
        <connector type="male" id="connector5" name="GND">
            <description>GND</description>
            <views>
                <breadboardView>
                    <p svgId="connector5pin" layer="breadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector5pin" layer="schematic" terminalId="connector5terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector5pin" layer="copper0"/>
                    <p svgId="connector5pin" layer="copper1"/>
                </pcbView>
            </views>
        </connector>
       <connector type="male" id="connector6" name="D13">
            <description>D13</description>
            <views>
                <breadboardView>
                    <p svgId="connector6pin" layer="breadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector6pin" layer="schematic" terminalId="connector6terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector6pin" layer="copper0"/>
                    <p svgId="connector6pin" layer="copper1"/>
                </pcbView>
            </views>
        </connector>
        <connector type="male" id="connector7" name="3V3">
            <description>Digital I/O</description>
            <views>
                <breadboardView>
                    <p svgId="connector7pin" layer="breadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector7pin" layer="schematic" terminalId="connector7terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector7pin" layer="copper0"/>
                    <p svgId="connector7pin" layer="copper1"/>
                </pcbView>
            </views>
        </connector>
	      <connector type="male" id="connector8" name="REF">
            <description>Ref</description>
            <views>
                <breadboardView>
                    <p svgId="connector8pin" layer="breadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector8pin" layer="schematic" terminalId="connector8terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector8pin" layer="copper0"/>
                    <p svgId="connector8pin" layer="copper1"/>
                </pcbView>
            </views>
        </connector>
	    <connector type="male" id="connector9" name="A0">
            <description>A0</description>
            <views>
                <breadboardView>
                    <p svgId="connector9pin" layer="breadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector9pin" layer="schematic" terminalId="connector9terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector9pin" layer="copper0"/>
                    <p svgId="connector9pin" layer="copper1"/>
                </pcbView>
            </views>
        </connector>
	   <connector type="male" id="connector10" name="A1">
            <description>A1 - analog input</description>
            <views>
                <breadboardView>
                    <p svgId="connector10pin" layer="breadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector10pin" layer="schematic" terminalId="connector10terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector10pin" layer="copper0"/>
                    <p svgId="connector10pin" layer="copper1"/>
                </pcbView>
            </views>
        </connector>
        <connector type="male" id="connector11" name="A2">
            <description>A2 - analog input</description>
            <views>
                <breadboardView>
                    <p svgId="connector11pin" layer="breadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector11pin" layer="schematic" terminalId="connector11terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector11pin" layer="copper0"/>
                    <p svgId="connector11pin" layer="copper1"/>
                </pcbView>
            </views>
        </connector>
        <connector type="male" id="connector12" name="A3">
            <description>A3 - analog input</description>
            <views>
                <breadboardView>
                    <p svgId="connector12pin" layer="breadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector12pin" layer="schematic" terminalId="connector12terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector12pin" layer="copper0"/>
                    <p svgId="connector12pin" layer="copper1"/>
                </pcbView>
            </views>
        </connector>
        <connector type="male" id="connector13" name="A4">
            <description>A4 - analog input</description>
            <views>
                <breadboardView>
                    <p svgId="connector13pin" layer="breadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector13pin" layer="schematic" terminalId="connector13terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector13pin" layer="copper0"/>
                    <p svgId="connector13pin" layer="copper1"/>
                </pcbView>
            </views>
        </connector>
        <connector type="male" id="connector14" name="A5">
            <description>A5 - analog input</description>
            <views>
                <breadboardView>
                    <p svgId="connector14pin" layer="breadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector14pin" layer="schematic" terminalId="connector14terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector14pin" layer="copper0"/>
                    <p svgId="connector14pin" layer="copper1"/>
                </pcbView>
            </views>
        </connector>
        <connector type="male" id="connector15" name="USB -">
            <description>USB -</description>
            <views>
                <breadboardView>
                    <p svgId="connector15pin" layer="breadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector15pin" layer="schematic" terminalId="connector15terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector15pin" layer="copper0"/>
                    <p svgId="connector15pin" layer="copper1"/>
                </pcbView>
            </views>
        </connector>
        <connector type="male" id="connector16" name="USB +">
            <description>USB +</description>
            <views>
                <breadboardView>
                    <p svgId="connector16pin" layer="breadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector16pin" layer="schematic" terminalId="connector16terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector16pin" layer="copper0"/>
                    <p svgId="connector16pin" layer="copper1"/>
                </pcbView>
            </views>
        </connector>
        <connector type="male" id="connector17" name="5V">
            <description>Digital I/O</description>
            <views>
                <breadboardView>
                    <p svgId="connector17pin" layer="breadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector17pin" layer="schematic" terminalId="connector17terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector17pin" layer="copper0"/>
                    <p svgId="connector17pin" layer="copper1"/>
                </pcbView>
            </views>
        </connector>
        <connector type="male" id="connector18" name="RST">
            <description>RST</description>
            <views>
                <breadboardView>
                    <p svgId="connector18pin" layer="breadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector18pin" layer="schematic" terminalId="connector18terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector18pin" layer="copper0"/>
                    <p svgId="connector18pin" layer="copper1"/>
                </pcbView>
            </views>
        </connector>
        <connector type="male" id="connector19" name="GND">
            <description>GND</description>
            <views>
                <breadboardView>
                    <p svgId="connector19pin" layer="breadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector19pin" layer="schematic" terminalId="connector19terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector19pin" layer="copper0"/>
                    <p svgId="connector19pin" layer="copper1"/>
                </pcbView>
            </views>
        </connector>
          <connector type="male" id="connector23" name="RX">
            <description>RX</description>
            <views>
                <breadboardView>
                    <p svgId="connector23pin" layer="breadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector23pin" layer="schematic" terminalId="connector23terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector23pin" layer="copper0"/>
                    <p svgId="connector23pin" layer="copper1"/>
                </pcbView>
            </views>
        </connector>
        <connector type="male" id="connector24" name="RST">
            <description>RST</description>
            <views>
                <breadboardView>
                    <p svgId="connector24pin" layer="breadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector24pin" layer="schematic" terminalId="connector24terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector24pin" layer="copper0"/>
                    <p svgId="connector24pin" layer="copper1"/>
                </pcbView>
            </views>
        </connector>
        <connector type="male" id="connector25" name="GND">
            <description>GND</description>
            <views>
                <breadboardView>
                    <p svgId="connector25pin" layer="breadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector25pin" layer="schematic" terminalId="connector25terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector25pin" layer="copper0"/>
                    <p svgId="connector25pin" layer="copper1"/>
                </pcbView>
            </views>
        </connector>
        <connector type="male" id="connector26" name="D2">
            <description>D2</description>
            <views>
                <breadboardView>
                    <p svgId="connector26pin" layer="breadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector26pin" layer="schematic" terminalId="connector26terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector26pin" layer="copper0"/>
                    <p svgId="connector26pin" layer="copper1"/>
                </pcbView>
            </views>
        </connector>
        <connector type="male" id="connector27" name="D3">
            <description>D3</description>
            <views>
                <breadboardView>
                    <p svgId="connector27pin" layer="breadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector27pin" layer="schematic" terminalId="connector27terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector27pin" layer="copper0"/>
                    <p svgId="connector27pin" layer="copper1"/>
                </pcbView>
            </views>
        </connector>
        <connector type="male" id="connector28" name="D4">
            <description>D4</description>
            <views>
                <breadboardView>
                    <p svgId="connector28pin" layer="breadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector28pin" layer="schematic" terminalId="connector28terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector28pin" layer="copper0"/>
                    <p svgId="connector28pin" layer="copper1"/>
                </pcbView>
            </views>
        </connector>
        <connector type="male" id="connector29" name="D5">
            <description>D5</description>
            <views>
                <breadboardView>
                    <p svgId="connector29pin" layer="breadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector29pin" layer="schematic" terminalId="connector29terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector29pin" layer="copper0"/>
                    <p svgId="connector29pin" layer="copper1"/>
                </pcbView>
            </views>
        </connector>
        <connector type="male" id="connector30" name="D6">
            <description>D6</description>
            <views>
                <breadboardView>
                    <p svgId="connector30pin" layer="breadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector30pin" layer="schematic" terminalId="connector30terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector30pin" layer="copper0"/>
                    <p svgId="connector30pin" layer="copper1"/>
                </pcbView>
            </views>
        </connector>
        <connector type="male" id="connector31" name="D7">
            <description>D7</description>
            <views>
                <breadboardView>
                    <p svgId="connector31pin" layer="breadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector31pin" layer="schematic" terminalId="connector31terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector31pin" layer="copper0"/>
                    <p svgId="connector31pin" layer="copper1"/>
                </pcbView>
            </views>
        </connector>
        <connector type="male" id="connector32" name="D8">
            <description>D8</description>
            <views>
                <breadboardView>
                    <p svgId="connector32pin" layer="breadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector32pin" layer="schematic" terminalId="connector32terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector32pin" layer="copper0"/>
                    <p svgId="connector32pin" layer="copper1"/>
                </pcbView>
            </views>
        </connector>
        <connector type="male" id="connector33" name="D9">
            <description>D9</description>
            <views>
                <breadboardView>
                    <p svgId="connector33pin" layer="breadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector33pin" layer="schematic" terminalId="connector33terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector33pin" layer="copper0"/>
                    <p svgId="connector33pin" layer="copper1"/>
                </pcbView>
            </views>
        </connector>
        <connector type="male" id="connector34" name="D10">
            <description>D10</description>
            <views>
                <breadboardView>
                    <p svgId="connector34pin" layer="breadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector34pin" layer="schematic" terminalId="connector34terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector34pin" layer="copper0"/>
                    <p svgId="connector34pin" layer="copper1"/>
                </pcbView>
            </views>
        </connector>
        <connector type="male" id="connector35" name="D11">
            <description>D11</description>
            <views>
                <breadboardView>
                    <p svgId="connector35pin" layer="breadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector35pin" layer="schematic" terminalId="connector35terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector35pin" layer="copper0"/>
                    <p svgId="connector35pin" layer="copper1"/>
                </pcbView>
            </views>
        </connector>
        <connector type="male" id="connector36" name="D12">
            <description>D12</description>
            <views>
                <breadboardView>
                    <p svgId="connector36pin" layer="breadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector36pin" layer="schematic" terminalId="connector36terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector36pin" layer="copper0"/>
                    <p svgId="connector36pin" layer="copper1"/>
                </pcbView>
            </views>
        </connector>
        <connector type="male" id="connector37" name="AR_GP6">
            <description>AR_GP6</description>
            <views>
                <breadboardView>
                    <p svgId="connector37pin" layer="breadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector37pin" layer="schematic" terminalId="connector37terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector37pin" layer="copper0"/>
                    <p svgId="connector37pin" layer="copper1"/>
                </pcbView>
            </views>
        </connector>
        <connector type="male" id="connector38" name="AR_GP23">
            <description>AR_GP23</description>
            <views>
                <breadboardView>
                    <p svgId="connector38pin" layer="breadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector38pin" layer="schematic" terminalId="connector38terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector38pin" layer="copper0"/>
                    <p svgId="connector38pin" layer="copper1"/>
                </pcbView>
            </views>
        </connector>
        <connector type="male" id="connector39" name="GND">
            <description>GND</description>
            <views>
                <breadboardView>
                    <p svgId="connector39pin" layer="breadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector39pin" layer="schematic" terminalId="connector39terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector39pin" layer="copper0"/>
                    <p svgId="connector39pin" layer="copper1"/>
                </pcbView>
            </views>
        </connector>
        <connector type="male" id="connector40" name="GND">
            <description>GND</description>
            <views>
                <breadboardView>
                    <p svgId="connector40pin" layer="breadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector40pin" layer="schematic" terminalId="connector40terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector40pin" layer="copper0"/>
                    <p svgId="connector40pin" layer="copper1"/>
                </pcbView>
            </views>
        </connector>
        <connector type="male" id="connector41" name="GND">
            <description>GND</description>
            <views>
                <breadboardView>
                    <p svgId="connector41pin" layer="breadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector41pin" layer="schematic" terminalId="connector41terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector41pin" layer="copper0"/>
                    <p svgId="connector41pin" layer="copper1"/>
                </pcbView>
            </views>
        </connector>
        <connector type="male" id="connector42" name="VCC_GT">
            <description>VCC_GT</description>
            <views>
                <breadboardView>
                    <p svgId="connector42pin" layer="breadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector42pin" layer="schematic" terminalId="connector42terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector42pin" layer="copper0"/>
                    <p svgId="connector42pin" layer="copper1"/>
                </pcbView>
            </views>           
        </connector>
                <connector type="male" id="connector45" name="TX">
            <description>Tx</description>
            <views>
                <breadboardView>
                    <p svgId="connector45pin" layer="breadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector45pin" layer="schematic" terminalId="connector45terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector45pin" layer="copper0"/>
                    <p svgId="connector45pin" layer="copper1"/>
                </pcbView>
            </views>
        </connector>
        <connector type="male" id="connector46" name="SS">
            <description>SS</description>
            <views>
                <breadboardView>
                    <p svgId="connector46pin" layer="breadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector46pin" layer="schematic" terminalId="connector46terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector46pin" layer="copper0"/>
                    <p svgId="connector46pin" layer="copper1"/>
                </pcbView>
            </views>
        </connector>
        <connector type="male" id="connector47" name="MOSI">
            <description>Mosi</description>
            <views>
                <breadboardView>
                    <p svgId="connector47pin" layer="breadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector47pin" layer="schematic" terminalId="connector47terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector47pin" layer="copper0"/>
                    <p svgId="connector47pin" layer="copper1"/>
                </pcbView>
            </views>
        </connector>
        <connector type="male" id="connector48" name="NC">
            <description>NC</description>
            <views>
                <breadboardView>
                    <p svgId="connector48pin" layer="breadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector48pin" layer="schematic" terminalId="connector48terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector48pin" layer="copper0"/>
                    <p svgId="connector48pin" layer="copper1"/>
                </pcbView>
            </views>
        </connector>
        <connector type="male" id="connector49" name="VIN">
            <description>Vin</description>
            <views>
                <breadboardView>
                    <p svgId="connector49pin" layer="breadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector49pin" layer="schematic" terminalId="connector49terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector49pin" layer="copper0"/>
                    <p svgId="connector49pin" layer="copper1"/>
                </pcbView>
            </views>
        </connector>
        <connector type="male" id="connector50" name="MISO">
            <description>MISO</description>
            <views>
                <breadboardView>
                    <p svgId="connector50pin" layer="breadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector50pin" layer="schematic" terminalId="connector50terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector50pin" layer="copper0"/>
                    <p svgId="connector50pin" layer="copper1"/>
                </pcbView>
            </views>
        </connector>
        <connector type="male" id="connector51" name="SCK">
            <description>SCK</description>
            <views>
                <breadboardView>
                    <p svgId="connector51pin" layer="breadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector51pin" layer="schematic" terminalId="connector51terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector51pin" layer="copper0"/>
                    <p svgId="connector51pin" layer="copper1"/>
                </pcbView>
            </views>
        </connector>
        <connector type="male" id="connector52" name="NC">
            <description>NC</description>
            <views>
                <breadboardView>
                    <p svgId="connector52pin" layer="breadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector52pin" layer="schematic" terminalId="connector52terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector52pin" layer="copper0"/>
                    <p svgId="connector52pin" layer="copper1"/>
                </pcbView>
            </views>
        </connector>

        </connectors>
    <buses>
        <bus id="GND">
	<nodeMember connectorId="connector5"/>
	<nodeMember connectorId="connector19"/>
	<nodeMember connectorId="connector41"/>
	<nodeMember connectorId="connector40"/>
	<nodeMember connectorId="connector39"/>
	<nodeMember connectorId="connector25"/>
        </bus>
	        <bus id="RST">
	<nodeMember connectorId="connector18"/>
	<nodeMember connectorId="connector24"/>
        </bus>
   </buses>
</module>
