<?xml version='1.0' encoding='UTF-8'?>
<module fritzingVersion="0.4.4b.10.03.4492" moduleId="288ea56ea458fbe4774256402d9b0e34">
    <author>lionelmichel</author>
    <title>Teensy++ 2.0</title>
    <label>Teensy++</label>
    <date>2010-11-05</date>
    <tags>
        <tag>Teensy++ 2.0</tag>
        <tag>microcontroller</tag>
    </tags>
    <properties>
        <property name="family">Microcontroller Board (Teensy)</property>
        <property name="processor">ATmega</property>
        <property name="variant">Teensy++ 2.0</property>
    </properties>
    <description>The Teensy is a complete USB-based microcontoller development system, in a very small footprint, capable of implementing many types of projects. All programming is done via the USB port. No special programmer is needed, only a standard "Mini-B" USB cable and a PC or Macintosh with a USB port.</description>
    <views>
        <iconView>
            <layers image="icon/Teensy_2.0_++_icon.svg">
                <layer layerId="icon"/>
            </layers>
        </iconView>
        <breadboardView>
            <layers image="breadboard/Teensy_2.0_++_breadboard.svg">
                <layer layerId="breadboard"/>
            </layers>
        </breadboardView>
        <schematicView>
            <layers image="schematic/Teensy_2.0_++_schematic.svg">
                <layer layerId="schematic"/>
            </layers>
        </schematicView>
        <pcbView>
            <layers image="pcb/Teensy_2.0_++_pcb.svg">
                <layer layerId="copper1"/>
                <layer layerId="copper0"/>
                <layer layerId="silkscreen"/>
            </layers>
        </pcbView>
    </views>
    <connectors>
        <connector type="male" id="connector3" name="D1">
            <description>Digital I/O</description>
            <views>
                <breadboardView>
                    <p svgId="connector3pin" layer="breadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector3pin" layer="schematic" terminalId="connector3terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector3pin" layer="copper0"/>
                    <p svgId="connector3pin" layer="copper1"/>
                </pcbView>
            </views>
        </connector>
        <connector type="female" id="connector20" name="VCC">
            <description>+5V</description>
            <views>
                <breadboardView>
                    <p svgId="connector20pin" layer="breadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector20pin" layer="schematic" terminalId="connector20terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector20pin" layer="copper0"/>
                    <p svgId="connector20pin" layer="copper1"/>
                </pcbView>
            </views>
        </connector>
        <connector type="male" id="connector4" name="D2">
            <description>Digital I/O</description>
            <views>
                <breadboardView>
                    <p svgId="connector4pin" layer="breadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector4pin" layer="schematic" terminalId="connector4terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector4pin" layer="copper0"/>
                    <p svgId="connector4pin" layer="copper1"/>
                </pcbView>
            </views>
        </connector>
        <connector type="female" id="connector21" name="GND">
            <description>Ground</description>
            <views>
                <breadboardView>
                    <p svgId="connector21pin" layer="breadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector21pin" layer="schematic" terminalId="connector21terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector21pin" layer="copper0"/>
                    <p svgId="connector21pin" layer="copper1"/>
                </pcbView>
            </views>
        </connector>
        <connector type="male" id="connector5" name="D3">
            <description>Digital I/O</description>
            <views>
                <breadboardView>
                    <p svgId="connector5pin" layer="breadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector5pin" layer="schematic" terminalId="connector5terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector5pin" layer="copper0"/>
                    <p svgId="connector5pin" layer="copper1"/>
                </pcbView>
            </views>
        </connector>
        <connector type="female" id="connector22" name="RST">
            <description>Reset</description>
            <views>
                <breadboardView>
                    <p svgId="connector22pin" layer="breadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector22pin" layer="schematic" terminalId="connector22terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector22pin" layer="copper0"/>
                    <p svgId="connector22pin" layer="copper1"/>
                </pcbView>
            </views>
        </connector>
        <connector type="male" id="connector6" name="D4">
            <description>Digital I/O</description>
            <views>
                <breadboardView>
                    <p svgId="connector6pin" layer="breadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector6pin" layer="schematic" terminalId="connector6terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector6pin" layer="copper0"/>
                    <p svgId="connector6pin" layer="copper1"/>
                </pcbView>
            </views>
        </connector>
        <connector type="male" id="connector7" name="D5">
            <description>Digital I/O</description>
            <views>
                <breadboardView>
                    <p svgId="connector7pin" layer="breadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector7pin" layer="schematic" terminalId="connector7terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector7pin" layer="copper0"/>
                    <p svgId="connector7pin" layer="copper1"/>
                </pcbView>
            </views>
        </connector>
        <connector type="male" id="connector23" name="F7">
            <description>Analog Input</description>
            <views>
                <breadboardView>
                    <p svgId="connector23pin" layer="breadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector23pin" layer="schematic" terminalId="connector23terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector23pin" layer="copper0"/>
                    <p svgId="connector23pin" layer="copper1"/>
                </pcbView>
            </views>
        </connector>
        <connector type="male" id="connector8" name="D6">
            <description>Digital I/O</description>
            <views>
                <breadboardView>
                    <p svgId="connector8pin" layer="breadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector8pin" layer="schematic" terminalId="connector8terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector8pin" layer="copper0"/>
                    <p svgId="connector8pin" layer="copper1"/>
                </pcbView>
            </views>
        </connector>
        <connector type="male" id="connector24" name="F6">
            <description>Analog Input</description>
            <views>
                <breadboardView>
                    <p svgId="connector24pin" layer="breadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector24pin" layer="schematic" terminalId="connector24terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector24pin" layer="copper0"/>
                    <p svgId="connector24pin" layer="copper1"/>
                </pcbView>
            </views>
        </connector>
        <connector type="male" id="connector9" name="D7">
            <description>Digital I/O</description>
            <views>
                <breadboardView>
                    <p svgId="connector9pin" layer="breadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector9pin" layer="schematic" terminalId="connector9terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector9pin" layer="copper0"/>
                    <p svgId="connector9pin" layer="copper1"/>
                </pcbView>
            </views>
        </connector>
        <connector type="male" id="connector25" name="F5">
            <description>Analog Input</description>
            <views>
                <breadboardView>
                    <p svgId="connector25pin" layer="breadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector25pin" layer="schematic" terminalId="connector25terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector25pin" layer="copper0"/>
                    <p svgId="connector25pin" layer="copper1"/>
                </pcbView>
            </views>
        </connector>
        <connector type="male" id="connector26" name="F4">
            <description>Analog Input</description>
            <views>
                <breadboardView>
                    <p svgId="connector26pin" layer="breadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector26pin" layer="schematic" terminalId="connector26terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector26pin" layer="copper0"/>
                    <p svgId="connector26pin" layer="copper1"/>
                </pcbView>
            </views>
        </connector>
        <connector type="male" id="connector27" name="F3">
            <description>Analog Input</description>
            <views>
                <breadboardView>
                    <p svgId="connector27pin" layer="breadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector27pin" layer="schematic" terminalId="connector27terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector27pin" layer="copper0"/>
                    <p svgId="connector27pin" layer="copper1"/>
                </pcbView>
            </views>
        </connector>
        <connector type="male" id="connector28" name="F2">
            <description>Analog Input</description>
            <views>
                <breadboardView>
                    <p svgId="connector28pin" layer="breadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector28pin" layer="schematic" terminalId="connector28terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector28pin" layer="copper0"/>
                    <p svgId="connector28pin" layer="copper1"/>
                </pcbView>
            </views>
        </connector>
        <connector type="male" id="connector29" name="F1">
            <description>Analog Input</description>
            <views>
                <breadboardView>
                    <p svgId="connector29pin" layer="breadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector29pin" layer="schematic" terminalId="connector29terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector29pin" layer="copper0"/>
                    <p svgId="connector29pin" layer="copper1"/>
                </pcbView>
            </views>
        </connector>
        <connector type="male" id="connector30" name="F0">
            <description>Analog Input</description>
            <views>
                <breadboardView>
                    <p svgId="connector30pin" layer="breadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector30pin" layer="schematic" terminalId="connector30terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector30pin" layer="copper0"/>
                    <p svgId="connector30pin" layer="copper1"/>
                </pcbView>
            </views>
        </connector>
        <connector type="male" id="connector31" name="AREF">
            <description>AREF</description>
            <views>
                <breadboardView>
                    <p svgId="connector31pin" layer="breadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector31pin" layer="schematic" terminalId="connector31terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector31pin" layer="copper0"/>
                    <p svgId="connector31pin" layer="copper1"/>
                </pcbView>
            </views>
        </connector>
        <connector type="male" id="connector32" name="GND">
            <description>Ground</description>
            <views>
                <breadboardView>
                    <p svgId="connector32pin" layer="breadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector32pin" layer="schematic" terminalId="connector32terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector32pin" layer="copper0"/>
                    <p svgId="connector32pin" layer="copper1"/>
                </pcbView>
            </views>
        </connector>
        <connector type="male" id="connector33" name="E6">
            <description>Digital I/O</description>
            <views>
                <breadboardView>
                    <p svgId="connector33pin" layer="breadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector33pin" layer="schematic" terminalId="connector33terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector33pin" layer="copper0"/>
                    <p svgId="connector33pin" layer="copper1"/>
                </pcbView>
            </views>
        </connector>
        <connector type="male" id="connector34" name="E7">
            <description>Digital I/O</description>
            <views>
                <breadboardView>
                    <p svgId="connector34pin" layer="breadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector34pin" layer="schematic" terminalId="connector34terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector34pin" layer="copper0"/>
                    <p svgId="connector34pin" layer="copper1"/>
                </pcbView>
            </views>
        </connector>
        <connector type="male" id="connector35" name="B0">
            <description>Digital I/O</description>
            <views>
                <breadboardView>
                    <p svgId="connector35pin" layer="breadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector35pin" layer="schematic" terminalId="connector35terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector35pin" layer="copper0"/>
                    <p svgId="connector35pin" layer="copper1"/>
                </pcbView>
            </views>
        </connector>
        <connector type="male" id="connector36" name="B1">
            <description>Digital I/O</description>
            <views>
                <breadboardView>
                    <p svgId="connector36pin" layer="breadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector36pin" layer="schematic" terminalId="connector36terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector36pin" layer="copper0"/>
                    <p svgId="connector36pin" layer="copper1"/>
                </pcbView>
            </views>
        </connector>
        <connector type="male" id="connector37" name="B2">
            <description>Digital I/O</description>
            <views>
                <breadboardView>
                    <p svgId="connector37pin" layer="breadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector37pin" layer="schematic" terminalId="connector37terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector37pin" layer="copper0"/>
                    <p svgId="connector37pin" layer="copper1"/>
                </pcbView>
            </views>
        </connector>
        <connector type="male" id="connector38" name="B3">
            <description>Digital I/O</description>
            <views>
                <breadboardView>
                    <p svgId="connector38pin" layer="breadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector38pin" layer="schematic" terminalId="connector38terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector38pin" layer="copper0"/>
                    <p svgId="connector38pin" layer="copper1"/>
                </pcbView>
            </views>
        </connector>
        <connector type="male" id="connector39" name="B4">
            <description>Digital I/O</description>
            <views>
                <breadboardView>
                    <p svgId="connector39pin" layer="breadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector39pin" layer="schematic" terminalId="connector39terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector39pin" layer="copper0"/>
                    <p svgId="connector39pin" layer="copper1"/>
                </pcbView>
            </views>
        </connector>
        <connector type="male" id="connector40" name="B5">
            <description>Digital I/O</description>
            <views>
                <breadboardView>
                    <p svgId="connector40pin" layer="breadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector40pin" layer="schematic" terminalId="connector40terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector40pin" layer="copper0"/>
                    <p svgId="connector40pin" layer="copper1"/>
                </pcbView>
            </views>
        </connector>
        <connector type="male" id="connector41" name="B6">
            <description>Digital I/O</description>
            <views>
                <breadboardView>
                    <p svgId="connector41pin" layer="breadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector41pin" layer="schematic" terminalId="connector41terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector41pin" layer="copper0"/>
                    <p svgId="connector41pin" layer="copper1"/>
                </pcbView>
            </views>
        </connector>
        <connector type="male" id="connector42" name="VCC">
            <description>+5V</description>
            <views>
                <breadboardView>
                    <p svgId="connector42pin" layer="breadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector42pin" layer="schematic" terminalId="connector42terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector42pin" layer="copper0"/>
                    <p svgId="connector42pin" layer="copper1"/>
                </pcbView>
            </views>
        </connector>
        <connector type="female" id="connector43" name="E4">
            <description>Digital I/O</description>
            <views>
                <breadboardView>
                    <p svgId="connector43pin" layer="breadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector43pin" layer="schematic" terminalId="connector43terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector43pin" layer="copper0"/>
                    <p svgId="connector43pin" layer="copper1"/>
                </pcbView>
            </views>
        </connector>
        <connector type="female" id="connector44" name="E5">
            <description>Digital I/O</description>
            <views>
                <breadboardView>
                    <p svgId="connector44pin" layer="breadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector44pin" layer="schematic" terminalId="connector44terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector44pin" layer="copper0"/>
                    <p svgId="connector44pin" layer="copper1"/>
                </pcbView>
            </views>
        </connector>
        <connector type="female" id="connector45" name="PA0">
            <description>Digital I/O</description>
            <views>
                <breadboardView>
                    <p svgId="connector45pin" layer="breadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector45pin" layer="schematic" terminalId="connector45terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector45pin" layer="copper0"/>
                    <p svgId="connector45pin" layer="copper1"/>
                </pcbView>
            </views>
        </connector>
        <connector type="female" id="connector46" name="PA1">
            <description>Digital I/O</description>
            <views>
                <breadboardView>
                    <p svgId="connector46pin" layer="breadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector46pin" layer="schematic" terminalId="connector46terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector46pin" layer="copper0"/>
                    <p svgId="connector46pin" layer="copper1"/>
                </pcbView>
            </views>
        </connector>
        <connector type="female" id="connector47" name="PA2">
            <description>Digital I/O</description>
            <views>
                <breadboardView>
                    <p svgId="connector47pin" layer="breadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector47pin" layer="schematic" terminalId="connector47terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector47pin" layer="copper0"/>
                    <p svgId="connector47pin" layer="copper1"/>
                </pcbView>
            </views>
        </connector>
        <connector type="female" id="connector48" name="PA3">
            <description>Digital I/O</description>
            <views>
                <breadboardView>
                    <p svgId="connector48pin" layer="breadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector48pin" layer="schematic" terminalId="connector48terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector48pin" layer="copper0"/>
                    <p svgId="connector48pin" layer="copper1"/>
                </pcbView>
            </views>
        </connector>
        <connector type="female" id="connector49" name="PA4">
            <description>Digital I/O</description>
            <views>
                <breadboardView>
                    <p svgId="connector49pin" layer="breadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector49pin" layer="schematic" terminalId="connector49terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector49pin" layer="copper0"/>
                    <p svgId="connector49pin" layer="copper1"/>
                </pcbView>
            </views>
        </connector>
        <connector type="male" id="connector10" name="E0">
            <description>Digital I/O</description>
            <views>
                <breadboardView>
                    <p svgId="connector10pin" layer="breadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector10pin" layer="schematic" terminalId="connector10terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector10pin" layer="copper0"/>
                    <p svgId="connector10pin" layer="copper1"/>
                </pcbView>
            </views>
        </connector>
        <connector type="male" id="connector11" name="E1">
            <description>Digital I/O</description>
            <views>
                <breadboardView>
                    <p svgId="connector11pin" layer="breadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector11pin" layer="schematic" terminalId="connector11terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector11pin" layer="copper0"/>
                    <p svgId="connector11pin" layer="copper1"/>
                </pcbView>
            </views>
        </connector>
        <connector type="male" id="connector12" name="C0">
            <description>Digital I/O</description>
            <views>
                <breadboardView>
                    <p svgId="connector12pin" layer="breadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector12pin" layer="schematic" terminalId="connector12terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector12pin" layer="copper0"/>
                    <p svgId="connector12pin" layer="copper1"/>
                </pcbView>
            </views>
        </connector>
        <connector type="male" id="connector13" name="C1">
            <description>Digital I/O</description>
            <views>
                <breadboardView>
                    <p svgId="connector13pin" layer="breadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector13pin" layer="schematic" terminalId="connector13terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector13pin" layer="copper0"/>
                    <p svgId="connector13pin" layer="copper1"/>
                </pcbView>
            </views>
        </connector>
        <connector type="male" id="connector14" name="C2">
            <description>Digital I/O</description>
            <views>
                <breadboardView>
                    <p svgId="connector14pin" layer="breadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector14pin" layer="schematic" terminalId="connector14terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector14pin" layer="copper0"/>
                    <p svgId="connector14pin" layer="copper1"/>
                </pcbView>
            </views>
        </connector>
        <connector type="male" id="connector15" name="C3">
            <description>Digital I/O</description>
            <views>
                <breadboardView>
                    <p svgId="connector15pin" layer="breadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector15pin" layer="schematic" terminalId="connector15terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector15pin" layer="copper0"/>
                    <p svgId="connector15pin" layer="copper1"/>
                </pcbView>
            </views>
        </connector>
        <connector type="male" id="connector16" name="C4">
            <description>Digital I/O</description>
            <views>
                <breadboardView>
                    <p svgId="connector16pin" layer="breadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector16pin" layer="schematic" terminalId="connector16terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector16pin" layer="copper0"/>
                    <p svgId="connector16pin" layer="copper1"/>
                </pcbView>
            </views>
        </connector>
        <connector type="male" id="connector17" name="C5">
            <description>Digital I/O</description>
            <views>
                <breadboardView>
                    <p svgId="connector17pin" layer="breadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector17pin" layer="schematic" terminalId="connector17terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector17pin" layer="copper0"/>
                    <p svgId="connector17pin" layer="copper1"/>
                </pcbView>
            </views>
        </connector>
        <connector type="male" id="connector18" name="C6">
            <description>Digital I/O</description>
            <views>
                <breadboardView>
                    <p svgId="connector18pin" layer="breadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector18pin" layer="schematic" terminalId="connector18terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector18pin" layer="copper0"/>
                    <p svgId="connector18pin" layer="copper1"/>
                </pcbView>
            </views>
        </connector>
        <connector type="male" id="connector19" name="C7">
            <description>Digital I/O</description>
            <views>
                <breadboardView>
                    <p svgId="connector19pin" layer="breadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector19pin" layer="schematic" terminalId="connector19terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector19pin" layer="copper0"/>
                    <p svgId="connector19pin" layer="copper1"/>
                </pcbView>
            </views>
        </connector>
        <connector type="female" id="connector50" name="PA5">
            <description>Digital I/O</description>
            <views>
                <breadboardView>
                    <p svgId="connector50pin" layer="breadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector50pin" layer="schematic" terminalId="connector50terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector50pin" layer="copper0"/>
                    <p svgId="connector50pin" layer="copper1"/>
                </pcbView>
            </views>
        </connector>
        <connector type="female" id="connector51" name="PA6">
            <description>Digital I/O</description>
            <views>
                <breadboardView>
                    <p svgId="connector51pin" layer="breadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector51pin" layer="schematic" terminalId="connector51terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector51pin" layer="copper0"/>
                    <p svgId="connector51pin" layer="copper1"/>
                </pcbView>
            </views>
        </connector>
        <connector type="female" id="connector52" name="PA7">
            <description>Digital I/O</description>
            <views>
                <breadboardView>
                    <p svgId="connector52pin" layer="breadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector52pin" layer="schematic" terminalId="connector52terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector52pin" layer="copper0"/>
                    <p svgId="connector52pin" layer="copper1"/>
                </pcbView>
            </views>
        </connector>
        <connector type="female" id="connector53" name="ALE">
            <description>ALE</description>
            <views>
                <breadboardView>
                    <p svgId="connector53pin" layer="breadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector53pin" layer="schematic" terminalId="connector53terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector53pin" layer="copper0"/>
                    <p svgId="connector53pin" layer="copper1"/>
                </pcbView>
            </views>
        </connector>
        <connector type="male" id="connector0" name="GND">
            <description>Ground</description>
            <views>
                <breadboardView>
                    <p svgId="connector0pin" layer="breadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector0pin" layer="schematic" terminalId="connector0terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector0pin" layer="copper0"/>
                    <p svgId="connector0pin" layer="copper1"/>
                </pcbView>
            </views>
        </connector>
        <connector type="male" id="connector1" name="B7">
            <description>Digital I/O</description>
            <views>
                <breadboardView>
                    <p svgId="connector1pin" layer="breadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector1pin" layer="schematic" terminalId="connector1terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector1pin" layer="copper0"/>
                    <p svgId="connector1pin" layer="copper1"/>
                </pcbView>
            </views>
        </connector>
        <connector type="male" id="connector2" name="D0">
            <description>Digital I/O</description>
            <views>
                <breadboardView>
                    <p svgId="connector2pin" layer="breadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector2pin" layer="schematic" terminalId="connector2terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector2pin" layer="copper0"/>
                    <p svgId="connector2pin" layer="copper1"/>
                </pcbView>
            </views>
        </connector>
    </connectors>
    <buses>
        <bus id="GND">
            <nodeMember connectorId="connector21"/>
            <nodeMember connectorId="connector0"/>
        </bus>
        <bus id="VCC">
            <nodeMember connectorId="connector20"/>
            <nodeMember connectorId="connector42"/>
        </bus>
    </buses>
</module>
