<?xml version='1.0' encoding='UTF-8'?>
<module fritzingVersion="0.2.2.b.03.04.2550" moduleId="2d505f861194750183f944ba86c13b44_28" referenceFile="generic_female_pin_header_3_100mil.fzp">
 <version>4</version>
 <author>Stefan Hermann</author>
 <title>TSOP312.., 314..</title>
 <label>IR</label>
 <date>Mo. Okt 8 2012</date>
 <tags>
  <tag>ir, infrared, receiver, remote, control</tag>
 </tags>
 <properties>
  <property name="package">THT</property>
  <property name="Row">single</property>
  <property name="Pin Spacing">0.1in (2.54mm)</property>
  <property name="Pins">3</property>
  <property name="part number"></property>
  <property name="family">infrared</property>
 </properties>
 <description>&lt;!DOCTYPE HTML PUBLIC "-//W3C//DTD HTML 4.0//EN" "http://www.w3.org/TR/REC-html40/strict.dtd">
&lt;html>&lt;head>&lt;meta name="qrichtext" content="1" />&lt;style type="text/css">
p, li { white-space: pre-wrap; }
&lt;/style>&lt;/head>&lt;body style=" font-family:'Lucida Grande'; font-size:13pt; font-weight:400; font-style:normal;">
&lt;p style=" margin-top:0px; margin-bottom:0px; margin-left:0px; margin-right:0px; -qt-block-indent:0; text-indent:0px;">The TSOP312.., TSOP314.. series are miniaturized receivers for infrared remote control systems. A PIN diode and a preamplifier are assembled on a lead frame, the epoxy package acts as an IR filter.&lt;/p>
&lt;p style=" margin-top:0px; margin-bottom:0px; margin-left:0px; margin-right:0px; -qt-block-indent:0; text-indent:0px;">The demodulated output signal can be directly decoded by a microprocessor. The TSOP312.. is compatible with all common IR remote control data formats. The TSOP314.. is optimized to suppress almost all spurious pulses from&lt;/p>
&lt;p style=" margin-top:0px; margin-bottom:0px; margin-left:0px; margin-right:0px; -qt-block-indent:0; text-indent:0px;">energy saving fluorescent lamps but will also suppress some data signals. &lt;/p>&lt;/body>&lt;/html></description>
 <views>
  <iconView>
   <layers image="icon/tsop312_icon.svg">
    <layer layerId="icon"/>
   </layers>
  </iconView>
  <breadboardView>
   <layers image="breadboard/tsop312_breadboard.svg">
    <layer layerId="breadboard"/>
   </layers>
  </breadboardView>
  <schematicView fliphorizontal="true">
   <layers image="schematic/tsop312_schematic.svg">
    <layer layerId="schematic"/>
   </layers>
  </schematicView>
  <pcbView>
   <layers image="pcb/tsop312_pcb.svg">
    <layer layerId="copper0"/>
    <layer layerId="silkscreen"/>
    <layer layerId="copper1"/>
   </layers>
  </pcbView>
 </views>
 <connectors>
  <connector type="male" id="connector0" name="GND">
   <description>ground</description>
   <views>
    <breadboardView>
     <p svgId="connector0pin" layer="breadboard" terminalId="connector0terminal"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector0pin" layer="schematic" terminalId="connector0terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector0pin" layer="copper0"/>
     <p svgId="connector0pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector type="male" id="connector1" name="Vs">
   <description>supply voltage</description>
   <views>
    <breadboardView>
     <p svgId="connector1pin" layer="breadboard" terminalId="connector1terminal"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector1pin" layer="schematic" terminalId="connector1terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector1pin" layer="copper0"/>
     <p svgId="connector1pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector type="male" id="connector2" name="Data">
   <description>data</description>
   <views>
    <breadboardView>
     <p svgId="connector2pin" layer="breadboard" terminalId="connector2terminal"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector2pin" layer="schematic" terminalId="connector2terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector2pin" layer="copper0"/>
     <p svgId="connector2pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
 </connectors>
</module>
