<?xml version='1.0' encoding='UTF-8'?>
<module fritzingVersion='0.5.2b.02.18.4756' moduleId='LilyPad Coincell-Battery-v17'>
<date>2013-05-25</date>
<author>f.althaus</author>
<author>SparkFun</author>
<description> If you&apos;re looking for a simple way to add a battery to your LilyPad project, the LilyPad Coin Cell Battery Holder might do the trick. It&apos;s a simple board which holds a 20mm coin cell battery (such as a CR2032) and gives you 4 connection points (two positive and two negative) for sewing into your project.

Note: The LilyPad Coin Cell Battery Holder is a design conceived by Felicia Williams of Boulder, Colorado. Also, a portion of this sale is given back to Dr. Leah Buechley for continued development and education of e-textiles. </description>
<title>LilyPad Coin Cell Battery Holder</title>
<url>http://www.sparkfun.com/products/10730</url>
<tags>
<tag>Lilypad</tag>
<tag>Coin</tag>
<tag>Cell</tag>
<tag>Battery</tag>
</tags>
<properties>
<property name='family'>microcontroller board (lilypad)</property>
<property name='type'>Power Connector</property>
<property name='Connector'>20mm Coin Cell Holder</property>
</properties>
<views>
<breadboardView>
<layers image='breadboard/LilyPad Coincell-Battery-v17_breadboard.svg'>
<layer layerId='breadboardbreadboard'/>
</layers>
</breadboardView>
<schematicView>
<layers image='schematic/LilyPad Coincell-Battery-v17_schematic.svg'>
<layer layerId='schematic'/>
</layers>
</schematicView>
<pcbView>
<layers image='pcb/LilyPad Coincell-Battery-v17_pcb.svg'>
<layer layerId='copper1'/>
<layer layerId='silkscreen'/>
<layer layerId='copper0'/>
</layers>
</pcbView>
<iconView>
<layers image='breadboard/LilyPad Coincell-Battery-v17_breadboard.svg'>
<layer layerId='icon'/>
</layers>
</iconView>
</views>
<connectors>
<connector id='connector5' type='female' name='-'>
<description>-</description><views>
<breadboardView>
<p layer='breadboardbreadboard' svgId='connector5pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector5pin' terminalId='connector5terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector5pad'/><p layer='copper1' svgId='connector5pad'/></pcbView>
</views>
</connector>
<connector id='connector6' type='female' name='+'>
<description>+</description><views>
<breadboardView>
<p layer='breadboardbreadboard' svgId='connector6pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector6pin' terminalId='connector6terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector6pad'/><p layer='copper1' svgId='connector6pad'/></pcbView>
</views>
</connector>
<connector id='connector7' type='female' name='-'>
<description>-</description><views>
<breadboardView>
<p layer='breadboardbreadboard' svgId='connector7pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector7pin' terminalId='connector7terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector7pad'/><p layer='copper1' svgId='connector7pad'/></pcbView>
</views>
</connector>
<connector id='connector8' type='female' name='+'>
<description>+</description><views>
<breadboardView>
<p layer='breadboardbreadboard' svgId='connector8pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector8pin' terminalId='connector8terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector8pad'/><p layer='copper1' svgId='connector8pad'/></pcbView>
</views>
</connector>
</connectors>
<buses>
<bus id='-'>
<nodeMember connectorId='connector5'/>
<nodeMember connectorId='connector7'/>
</bus>
<bus id='+'>
<nodeMember connectorId='connector6'/>
<nodeMember connectorId='connector8'/>
</bus>
</buses>
</module>
