<?xml version='1.0' encoding='UTF-8'?>
<module fritzingVersion='0.9.0b.02.18.4756' moduleId='Bean_revE'>
<version>4</version>
<date>2014-09-16</date>
<author>fabian althaus</author>
<description>The Bean connects your physical devices to the digital world. This is Punch Through Design’s newest addition to the Internet of Things.



We’ve bundled  a microcontroller with our very own Bluetooth Low Energy module to give you a tiny little board that you can program wirelessly from your smartphone or desktop. It runs on a coin cell battery for extended periods of time while in sleep mode —ideal for use as a long-term sensor or data logger. We’ve even built an RGB LED and an accelerometer right into the board!



Zero wires. Infinite uses. What will you build next?</description>
<title>LightBlue Bean</title>
<url>http://punchthrough.com/bean/</url>
<tags>
<tag>microcontroller</tag>
<tag>bluetooth</tag>
<tag>accelerometer</tag>
<tag>wireless</tag>
<tag>app</tag>
<tag>atmega328</tag>
<tag>rev E</tag>
</tags>
<properties>
<property name='family'>microcontroller bean</property>
<property name='type'>rev E</property>
<property name='part name'>LightBlue Bean</property>
</properties>
<views>
<breadboardView>
<layers image='breadboard/Bean_revE_breadboard.svg'>
<layer layerId='breadboard'/>
</layers>
</breadboardView>
<schematicView>
<layers image='schematic/Bean_revE_schematic.svg'>
<layer layerId='schematic'/>
</layers>
</schematicView>
<pcbView>
<layers image='pcb/Bean_revE_pcb.svg'>
<layer layerId='copper1'/>
<layer layerId='silkscreen'/>
<layer layerId='copper0'/>
</layers>
</pcbView>
<iconView>
<layers image='icon/Bean_revE_icon.svg'>
<layer layerId='icon'/>
</layers>
</iconView>
</views>
<connectors>
<connector id='connector71' type='female' name='VCC'>
<description>VCC</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector71pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector71pin' terminalId='connector71terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector71pad'/><p layer='copper1' svgId='connector71pad'/></pcbView>
</views>
</connector>
<connector id='connector72' type='female' name='D5/SCK'>
<description>D5/SCK</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector72pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector72pin' terminalId='connector72terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector72pad'/><p layer='copper1' svgId='connector72pad'/></pcbView>
</views>
</connector>
<connector id='connector73' type='female' name='D4/MISO'>
<description>D4/MISO</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector73pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector73pin' terminalId='connector73terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector73pad'/><p layer='copper1' svgId='connector73pad'/></pcbView>
</views>
</connector>
<connector id='connector74' type='female' name='D3/MOSI'>
<description>D3/MOSI</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector74pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector74pin' terminalId='connector74terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector74pad'/><p layer='copper1' svgId='connector74pad'/></pcbView>
</views>
</connector>
<connector id='connector75' type='female' name='D2'>
<description>D2</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector75pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector75pin' terminalId='connector75terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector75pad'/><p layer='copper1' svgId='connector75pad'/></pcbView>
</views>
</connector>
<connector id='connector76' type='female' name='D1'>
<description>D1</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector76pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector76pin' terminalId='connector76terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector76pad'/><p layer='copper1' svgId='connector76pad'/></pcbView>
</views>
</connector>
<connector id='connector77' type='female' name='D0'>
<description>D0</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector77pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector77pin' terminalId='connector77terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector77pad'/><p layer='copper1' svgId='connector77pad'/></pcbView>
</views>
</connector>
<connector id='connector78' type='female' name='AIN_A1'>
<description>AIN_A1</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector78pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector78pin' terminalId='connector78terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector78pad'/><p layer='copper1' svgId='connector78pad'/></pcbView>
</views>
</connector>
<connector id='connector79' type='female' name='AIN_A0'>
<description>AIN_A0</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector79pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector79pin' terminalId='connector79terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector79pad'/><p layer='copper1' svgId='connector79pad'/></pcbView>
</views>
</connector>
<connector id='connector80' type='female' name='1'>
<description>1</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector80pin'/></breadboardView>
<schematicView>
<p layer='schematic' hybrid='yes' svgId='connector80pin' terminalId='connector80terminal'/></schematicView>
<pcbView>
<p layer='copper0' hybrid='yes' svgId='connector80pad'/><p layer='copper1' hybrid='yes' svgId='connector80pad'/></pcbView>
</views>
</connector>
<connector id='connector81' type='female' name='1'>
<description>1</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector81pin'/></breadboardView>
<schematicView>
<p layer='schematic' hybrid='yes' svgId='connector81pin' terminalId='connector81terminal'hybrid='yes' /></schematicView>
<pcbView>
<p layer='copper0' hybrid='yes' svgId='connector81pad' hybrid='yes' /><p layer='copper1' hybrid='yes' svgId='connector81pad' hybrid='yes' /></pcbView>
</views>
</connector>
<connector id='connector82' type='female' name='1'>
<description>1</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector82pin'/></breadboardView>
<schematicView>
<p layer='schematic' hybrid='yes' svgId='connector82pin' terminalId='connector82terminal'/></schematicView>
<pcbView>
<p layer='copper0' hybrid='yes' svgId='connector82pad'/><p layer='copper1' hybrid='yes' svgId='connector82pad'/></pcbView>
</views>
</connector>
<connector id='connector83' type='female' name='1'>
<description>1</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector83pin'/></breadboardView>
<schematicView>
<p layer='schematic' hybrid='yes' svgId='connector83pin' terminalId='connector83terminal'/></schematicView>
<pcbView>
<p layer='copper0' hybrid='yes' svgId='connector83pad'/><p layer='copper1' hybrid='yes' svgId='connector83pad'/></pcbView>
</views>
</connector>
<connector id='connector84' type='female' name='1'>
<description>1</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector84pin'/></breadboardView>
<schematicView>
<p layer='schematic' hybrid='yes' svgId='connector84pin' terminalId='connector84terminal'/></schematicView>
<pcbView>
<p layer='copper0' hybrid='yes' svgId='connector84pad'/><p layer='copper1' hybrid='yes' svgId='connector84pad'/></pcbView>
</views>
</connector>
<connector id='connector85' type='female' name='1'>
<description>1</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector85pin'/></breadboardView>
<schematicView>
<p layer='schematic' hybrid='yes' svgId='connector85pin' terminalId='connector85terminal'/></schematicView>
<pcbView>
<p layer='copper0' hybrid='yes' svgId='connector85pad'/><p layer='copper1' hybrid='yes' svgId='connector85pad'/></pcbView>
</views>
</connector>
<connector id='connector86' type='female' name='1'>
<description>1</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector86pin'/></breadboardView>
<schematicView>
<p layer='schematic' hybrid='yes' svgId='connector86pin' terminalId='connector86terminal'/></schematicView>
<pcbView>
<p layer='copper0' hybrid='yes' svgId='connector86pad'/><p layer='copper1' hybrid='yes' svgId='connector86pad'/></pcbView>
</views>
</connector>
<connector id='connector87' type='female' name='1'>
<description>1</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector87pin'/></breadboardView>
<schematicView>
<p layer='schematic' hybrid='yes' svgId='connector87pin' terminalId='connector87terminal'/></schematicView>
<pcbView>
<p layer='copper0' hybrid='yes' svgId='connector87pad'/><p layer='copper1' hybrid='yes' svgId='connector87pad'/></pcbView>
</views>
</connector>
<connector id='connector88' type='female' name='1'>
<description>1</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector88pin'/></breadboardView>
<schematicView>
<p layer='schematic' hybrid='yes' svgId='connector88pin' terminalId='connector88terminal'/></schematicView>
<pcbView>
<p layer='copper0' hybrid='yes' svgId='connector88pad'/><p layer='copper1' hybrid='yes' svgId='connector88pad'/></pcbView>
</views>
</connector>
<connector id='connector89' type='female' name='1'>
<description>1</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector89pin'/></breadboardView>
<schematicView>
<p layer='schematic' hybrid='yes' svgId='connector89pin' terminalId='connector89terminal'/></schematicView>
<pcbView>
<p layer='copper0' hybrid='yes' svgId='connector89pad'/><p layer='copper1' hybrid='yes' svgId='connector89pad'/></pcbView>
</views>
</connector>
<connector id='connector90' type='female' name='1'>
<description>1</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector90pin'/></breadboardView>
<schematicView>
<p layer='schematic' hybrid='yes' svgId='connector90pin' terminalId='connector90terminal'/></schematicView>
<pcbView>
<p layer='copper0' hybrid='yes' svgId='connector90pad'/><p layer='copper1' hybrid='yes' svgId='connector90pad'/></pcbView>
</views>
</connector>
<connector id='connector91' type='female' name='1'>
<description>1</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector91pin'/></breadboardView>
<schematicView>
<p layer='schematic' hybrid='yes' svgId='connector91pin' terminalId='connector91terminal'/></schematicView>
<pcbView>
<p layer='copper0' hybrid='yes' svgId='connector91pad'/><p layer='copper1' hybrid='yes' svgId='connector91pad'/></pcbView>
</views>
</connector>
<connector id='connector92' type='female' name='1'>
<description>1</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector92pin'/></breadboardView>
<schematicView>
<p layer='schematic' hybrid='yes' svgId='connector92pin' terminalId='connector92terminal'/></schematicView>
<pcbView>
<p layer='copper0' hybrid='yes' svgId='connector92pad'/><p layer='copper1' hybrid='yes' svgId='connector92pad'/></pcbView>
</views>
</connector>
<connector id='connector93' type='female' name='1'>
<description>1</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector93pin'/></breadboardView>
<schematicView>
<p layer='schematic' hybrid='yes' svgId='connector93pin' terminalId='connector93terminal'/></schematicView>
<pcbView>
<p layer='copper0' hybrid='yes' svgId='connector93pad'/><p layer='copper1' hybrid='yes' svgId='connector93pad'/></pcbView>
</views>
</connector>
<connector id='connector94' type='female' name='1'>
<description>1</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector94pin'/></breadboardView>
<schematicView>
<p layer='schematic' hybrid='yes' svgId='connector94pin' terminalId='connector94terminal'/></schematicView>
<pcbView>
<p layer='copper0' hybrid='yes' svgId='connector94pad'/><p layer='copper1' hybrid='yes' svgId='connector94pad'/></pcbView>
</views>
</connector>
<connector id='connector95' type='female' name='1'>
<description>1</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector95pin'/></breadboardView>
<schematicView>
<p layer='schematic' hybrid='yes' svgId='connector95pin' terminalId='connector95terminal'/></schematicView>
<pcbView>
<p layer='copper0' hybrid='yes' svgId='connector95pad'/><p layer='copper1' hybrid='yes' svgId='connector95pad'/></pcbView>
</views>
</connector>
<connector id='connector96' type='female' name='1'>
<description>1</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector96pin'/></breadboardView>
<schematicView>
<p layer='schematic' hybrid='yes' svgId='connector96pin' terminalId='connector96terminal'/></schematicView>
<pcbView>
<p layer='copper0' hybrid='yes' svgId='connector96pad'/><p layer='copper1' hybrid='yes' svgId='connector96pad'/></pcbView>
</views>
</connector>
<connector id='connector97' type='female' name='1'>
<description>1</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector97pin'/></breadboardView>
<schematicView>
<p layer='schematic' hybrid='yes' svgId='connector97pin' terminalId='connector97terminal'/></schematicView>
<pcbView>
<p layer='copper0' hybrid='yes' svgId='connector97pad'/><p layer='copper1' hybrid='yes' svgId='connector97pad'/></pcbView>
</views>
</connector>
<connector id='connector98' type='female' name='1'>
<description>1</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector98pin'/></breadboardView>
<schematicView>
<p layer='schematic' hybrid='yes' svgId='connector98pin' terminalId='connector98terminal'/></schematicView>
<pcbView>
<p layer='copper0' hybrid='yes' svgId='connector98pad'/><p layer='copper1' hybrid='yes' svgId='connector98pad'/></pcbView>
</views>
</connector>
<connector id='connector99' type='female' name='1'>
<description>1</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector99pin'/></breadboardView>
<schematicView>
<p layer='schematic' hybrid='yes' svgId='connector99pin' terminalId='connector99terminal'/></schematicView>
<pcbView>
<p layer='copper0' hybrid='yes' svgId='connector99pad'/><p layer='copper1' hybrid='yes' svgId='connector99pad'/></pcbView>
</views>
</connector>
<connector id='connector100' type='female' name='1'>
<description>1</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector100pin'/></breadboardView>
<schematicView>
<p layer='schematic' hybrid='yes' svgId='connector100pin' terminalId='connector100terminal'/></schematicView>
<pcbView>
<p layer='copper0' hybrid='yes' svgId='connector100pad'/><p layer='copper1' hybrid='yes' svgId='connector100pad'/></pcbView>
</views>
</connector>
<connector id='connector101' type='female' name='1'>
<description>1</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector101pin'/></breadboardView>
<schematicView>
<p layer='schematic' hybrid='yes' svgId='connector101pin' terminalId='connector101terminal'/></schematicView>
<pcbView>
<p layer='copper0' hybrid='yes' svgId='connector101pad'/><p layer='copper1' hybrid='yes' svgId='connector101pad'/></pcbView>
</views>
</connector>
<connector id='connector102' type='female' name='1'>
<description>1</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector102pin'/></breadboardView>
<schematicView>
<p layer='schematic' hybrid='yes' svgId='connector102pin' terminalId='connector102terminal'/></schematicView>
<pcbView>
<p layer='copper0' hybrid='yes' svgId='connector102pad'/><p layer='copper1' hybrid='yes' svgId='connector102pad'/></pcbView>
</views>
</connector>
<connector id='connector103' type='female' name='1'>
<description>1</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector103pin'/></breadboardView>
<schematicView>
<p layer='schematic' hybrid='yes' svgId='connector103pin' terminalId='connector103terminal'/></schematicView>
<pcbView>
<p layer='copper0' hybrid='yes' svgId='connector103pad'/><p layer='copper1' hybrid='yes' svgId='connector103pad'/></pcbView>
</views>
</connector>
<connector id='connector104' type='female' name='1'>
<description>1</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector104pin'/></breadboardView>
<schematicView>
<p layer='schematic' hybrid='yes' svgId='connector104pin' terminalId='connector104terminal'/></schematicView>
<pcbView>
<p layer='copper0' hybrid='yes' svgId='connector104pad'/><p layer='copper1' hybrid='yes' svgId='connector104pad'/></pcbView>
</views>
</connector>
<connector id='connector105' type='female' name='1'>
<description>1</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector105pin'/></breadboardView>
<schematicView>
<p layer='schematic' hybrid='yes' svgId='connector105pin' terminalId='connector105terminal'/></schematicView>
<pcbView>
<p layer='copper0' hybrid='yes' svgId='connector105pad'/><p layer='copper1' hybrid='yes' svgId='connector105pad'/></pcbView>
</views>
</connector>
<connector id='connector106' type='female' name='1'>
<description>1</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector106pin'/></breadboardView>
<schematicView>
<p layer='schematic' hybrid='yes' svgId='connector106pin' terminalId='connector106terminal'/></schematicView>
<pcbView>
<p layer='copper0' hybrid='yes' svgId='connector106pad'/><p layer='copper1' hybrid='yes' svgId='connector106pad'/></pcbView>
</views>
</connector>
<connector id='connector107' type='female' name='1'>
<description>1</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector107pin'/></breadboardView>
<schematicView>
<p layer='schematic' hybrid='yes' svgId='connector107pin' terminalId='connector107terminal'/></schematicView>
<pcbView>
<p layer='copper0' hybrid='yes' svgId='connector107pad'/><p layer='copper1' hybrid='yes' svgId='connector107pad'/></pcbView>
</views>
</connector>
<connector id='connector108' type='female' name='1'>
<description>1</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector108pin'/></breadboardView>
<schematicView>
<p layer='schematic' hybrid='yes' svgId='connector108pin' terminalId='connector108terminal'/></schematicView>
<pcbView>
<p layer='copper0' hybrid='yes' svgId='connector108pad'/><p layer='copper1' hybrid='yes' svgId='connector108pad'/></pcbView>
</views>
</connector>
<connector id='connector109' type='female' name='1'>
<description>1</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector109pin'/></breadboardView>
<schematicView>
<p layer='schematic' hybrid='yes' svgId='connector109pin' terminalId='connector109terminal'/></schematicView>
<pcbView>
<p layer='copper0' hybrid='yes' svgId='connector109pad'/><p layer='copper1' hybrid='yes' svgId='connector109pad'/></pcbView>
</views>
</connector>
<connector id='connector110' type='female' name='1'>
<description>1</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector110pin'/></breadboardView>
<schematicView>
<p layer='schematic' hybrid='yes' svgId='connector110pin' terminalId='connector110terminal'/></schematicView>
<pcbView>
<p layer='copper0' hybrid='yes' svgId='connector110pad'/><p layer='copper1' hybrid='yes' svgId='connector110pad'/></pcbView>
</views>
</connector>
<connector id='connector111' type='female' name='1'>
<description>1</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector111pin'/></breadboardView>
<schematicView>
<p layer='schematic' hybrid='yes' svgId='connector111pin' terminalId='connector111terminal'/></schematicView>
<pcbView>
<p layer='copper0' hybrid='yes' svgId='connector111pad'/><p layer='copper1' hybrid='yes' svgId='connector111pad'/></pcbView>
</views>
</connector>
<connector id='connector112' type='female' name='1'>
<description>1</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector112pin'/></breadboardView>
<schematicView>
<p layer='schematic' hybrid='yes' svgId='connector112pin' terminalId='connector112terminal'/></schematicView>
<pcbView>
<p layer='copper0' hybrid='yes' svgId='connector112pad'/><p layer='copper1' hybrid='yes' svgId='connector112pad'/></pcbView>
</views>
</connector>
<connector id='connector113' type='female' name='1'>
<description>1</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector113pin'/></breadboardView>
<schematicView>
<p layer='schematic' hybrid='yes' svgId='connector113pin' terminalId='connector113terminal'/></schematicView>
<pcbView>
<p layer='copper0' hybrid='yes' svgId='connector113pad'/><p layer='copper1' hybrid='yes' svgId='connector113pad'/></pcbView>
</views>
</connector>
<connector id='connector114' type='female' name='GND'>
<description>GND</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector114pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector114pin' terminalId='connector114terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector114pad'/><p layer='copper1' svgId='connector114pad'/></pcbView>
</views>
</connector>
<connector id='connector115' type='female' name='Reset'>
<description>Reset</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector115pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector115pin' terminalId='connector115terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector115pad'/><p layer='copper1' svgId='connector115pad'/></pcbView>
</views>
</connector>
<connector id='connector119' type='female' name='BAT'>
<description>BAT</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector119pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector119pin' terminalId='connector119terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector119pad'/><p layer='copper1' svgId='connector119pad'/></pcbView>
</views>
</connector>
<connector id='connector120' type='female' name='GND'>
<description>GND</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector120pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector120pin' terminalId='connector120terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector120pad'/><p layer='copper1' svgId='connector120pad'/></pcbView>
</views>
</connector>
</connectors>
<buses>
<bus id='gnd'>
<nodeMember connectorId='connector114'/>
<nodeMember connectorId='connector120'/>
</bus>
</buses>
</module>
