<?xml version="1.0" encoding="UTF-8"?><module fritzingVersion="0.2.2.b.03.04.2550" moduleId="ws2812b">
    <version>4</version>
    <author>fabian althaus</author>
    <title>ws2812b</title>
    <date>2015-02-23</date>
    <tags>
    <tag>SMD</tag>
    <tag>LED</tag>
    <tag>RGB</tag>
    <tag>Ws2812b</tag>
    </tags>
    <properties>
        <property name="family">rgb Led</property>
        <property name="package">smd 2812b</property>
        <property name="package">THT</property>
   </properties>
    <description>WS2812B 5050 RGB LED with Integrated Driver Chip</description>
    <views>
        <iconView>
            <layers image="breadboard/ws2812b_breadboard.svg">
                <layer layerId="icon"/>
            </layers>
        </iconView>
        <breadboardView>
            <layers image="breadboard/ws2812b_breadboard.svg">
                <layer layerId="breadboard"/>
            </layers>
        </breadboardView>
        <schematicView>
        <layers image="schematic/ws2812b_schematic.svg">
            <layer layerId="schematic"/>
        </layers>
        </schematicView>
        <pcbView>
            <layers image="pcb/ws2812b_pcb.svg">
                <layer layerId="silkscreen"/>
          <layer layerId="copper1"/>
           </layers>
        </pcbView>
    </views>
<connectors>
    <connector id="connector0" name="VDD" type="male">
       <description>pin 1 Vdd</description>
       <views>
        <breadboardView>
         <p layer="breadboard" svgId="connector0pin" terminalId="connector0terminal"/>
        </breadboardView>
        <schematicView>
         <p layer="schematic" svgId="connector0pin" terminalId="connector0terminal"/>
        </schematicView>
        <pcbView>
         
        <p layer="copper1" svgId="connector0pin"/></pcbView>
       </views>
    </connector>
    <connector id="connector1" name="DOUT" type="male">
       <description>pin 2 DOut</description>
       <views>
        <breadboardView>
         <p layer="breadboard" svgId="connector1pin" terminalId="connector1terminal"/>
        </breadboardView>
        <schematicView>
         <p layer="schematic" svgId="connector1pin" terminalId="connector1terminal"/>
        </schematicView>
        <pcbView>
         
        <p layer="copper1" svgId="connector1pin"/></pcbView>
       </views>
    </connector>
    <connector id="connector2" name="VSS" type="male">
       <description>pin 3 Vss</description>
       <views>
        <breadboardView>
         <p layer="breadboard" svgId="connector2pin" terminalId="connector2terminal"/>
        </breadboardView>
        <schematicView>
         <p layer="schematic" svgId="connector2pin" terminalId="connector2terminal"/>
        </schematicView>
        <pcbView>
         
        <p layer="copper1" svgId="connector2pin"/></pcbView>
       </views>
    </connector>
    <connector id="connector3" name="DIN" type="male">
       <description>pin 4 DIn</description>
       <views>
        <breadboardView>
         <p layer="breadboard" svgId="connector3pin" terminalId="connector3terminal"/>
        </breadboardView>
        <schematicView>
         <p layer="schematic" svgId="connector3pin" terminalId="connector3terminal"/>
        </schematicView>
        <pcbView>
         
        <p layer="copper1" svgId="connector3pin"/></pcbView>
       </views>
    </connector>
</connectors>
</module>