<?xml version='1.0' encoding='UTF-8'?>
<module fritzingVersion='0.5.2b.02.18.4756' moduleId='Breadboard Power Supply - SMD v12'>
<version>4</version>
<date>2011-11-16</date>
<author>SparkFun</author>
<description>&lt;p&gt;


	&lt;b&gt;Description: &lt;/b&gt;This is a very simple board that takes a 6-12V input voltage and outputs a selectable 5V or 3.3V regulated voltage. All headers are 0.1&amp;quot; pitch for simple insertion into a breadboard.&lt;/p&gt;


&lt;p&gt;


	Input power can be supplied to either the DC barrel jack or the two pin header labeled + and -. Output power is supplied to the pins labeled GND and VCC. Board has both an On/Off switch and a voltage select switch (3.3V/5V).&amp;nbsp;&lt;/p&gt;


&lt;p&gt;


	The two pairs of GND and VCC pins are spaced such that when connected to our &lt;a classname=&quot;&quot; href=&quot;http://www.sparkfun.com/commerce/product_info.php?products_id=112&quot; name=&quot;&quot; target=&quot;&quot;&gt;Basic Breadboard&lt;/a&gt; both power busses will be powered.&lt;/p&gt;


&lt;p&gt;


	Check out our &lt;a href=&quot;http://www.sparkfun.com/commerce/tutorial_info.php?tutorials_id=103&quot; target=&quot;_blank&quot;&gt;Unregulated Power Supply Tutorial&lt;/a&gt;!&lt;/p&gt;


&lt;p&gt;


	&lt;b&gt;Dimensions:&lt;/b&gt; 2.15x0.65&amp;quot;&lt;/p&gt;


&lt;p&gt;


	&lt;span style=&quot;font-weight: bold;&quot;&gt;Features:&lt;/span&gt;&lt;/p&gt;


&lt;ul&gt;


	&lt;li&gt;


		6-12V input voltage via barrel jack or 2-pin header&lt;/li&gt;


	&lt;li&gt;


		3.3V or 5V regulated output voltage&lt;/li&gt;


	&lt;li&gt;


		ON/OFF switch&lt;/li&gt;


	&lt;li&gt;


		Output voltage select switch&lt;/li&gt;


	&lt;li&gt;


		Power status LED&lt;/li&gt;


	&lt;li&gt;


		PTC fuse protected power&lt;/li&gt;


	&lt;li&gt;


		5.5x2.1mm center positive barrel jack&lt;/li&gt;


&lt;/ul&gt;


&lt;p&gt;


	&lt;b&gt;Documents:&lt;/b&gt;&lt;/p&gt;


&lt;ul&gt;


	&lt;li&gt;


		&lt;a classname=&quot;&quot; href=&quot;http://dlnmh9ip6v2uc.cloudfront.net/datasheets/Prototyping/Breadboard Power Supply - SMD v13.pdf&quot; target=&quot;_blank&quot;&gt;Schematic&lt;/a&gt;&lt;/li&gt;


	&lt;li&gt;


		&lt;a href=&quot;http://dlnmh9ip6v2uc.cloudfront.net/datasheets/Prototyping/Breadboard Power Supply - SMD v13.zip&quot; target=&quot;_blank&quot;&gt;Eagle Files&lt;/a&gt;&lt;/li&gt;


&lt;/ul&gt;


&lt;p&gt;


	&lt;strong&gt;Replaces: &lt;/strong&gt;&lt;a href=&quot;http://www.sparkfun.com/products/9319&quot; target=&quot;_blank&quot;&gt;PRT-09319&lt;/a&gt;&lt;/p&gt;


</description>
<title>Breadboard Power Supply Board SMD</title>
<url>http://www.sparkfun.com/products/10804</url>
<tags>
<tag>Breadboard</tag>
<tag>Power</tag>
<tag>Supply</tag>
</tags>
<properties>
<property name='Input Voltage'>6-12V</property>
<property name='family'>Power Conditioning</property>
<property name='Output Voltage'>3.3V or 5V</property>
<property name='Connector'>0.1 Header</property>
</properties>
<views>
<breadboardView>
<layers image='breadboard/Breadboard Power Supply - SMD v13_breadboard.svg'>
<layer layerId='breadboard'/>
</layers>
</breadboardView>
<schematicView>
<layers image='schematic/Breadboard Power Supply - SMD v13_schematic.svg'>
<layer layerId='schematic'/>
</layers>
</schematicView>
<pcbView>
<layers image='pcb/Breadboard Power Supply - SMD v13_pcb.svg'>
<layer layerId='copper1'/>
<layer layerId='silkscreen'/>
<layer layerId='copper0'/>
</layers>
</pcbView>
<iconView>
<layers image='breadboard/Breadboard Power Supply - SMD v13_breadboard.svg'>
<layer layerId='icon'/>
</layers>
</iconView>
</views>
<connectors>
<connector id='connector14' type='male' name='GND'>
<description>GND</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector14pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector14pin' terminalId='connector14terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector14pad'/><p layer='copper1' svgId='connector14pad'/></pcbView>
</views>
</connector>
<connector id='connector15' type='male' name='VCC'>
<description>VCC</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector15pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector15pin' terminalId='connector15terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector15pad'/><p layer='copper1' svgId='connector15pad'/></pcbView>
</views>
</connector>
<connector id='connector16' type='male' name='VCC'>
<description>VCC</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector16pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector16pin' terminalId='connector16terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector16pad'/><p layer='copper1' svgId='connector16pad'/></pcbView>
</views>
</connector>
<connector id='connector17' type='male' name='GND'>
<description>GND</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector17pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector17pin' terminalId='connector17terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector17pad'/><p layer='copper1' svgId='connector17pad'/></pcbView>
</views>
</connector>
<connector id='connector18' type='male' name='VIN'>
<description>VIN</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector18pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector18pin' terminalId='connector18terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector18pad'/><p layer='copper1' svgId='connector18pad'/></pcbView>
</views>
</connector>
<connector id='connector19' type='male' name='GND'>
<description>GND</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector19pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector19pin' terminalId='connector19terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector19pad'/><p layer='copper1' svgId='connector19pad'/></pcbView>
</views>
</connector>
</connectors>
<buses>
<bus id='vcc'>
<nodeMember connectorId='connector15'/>
<nodeMember connectorId='connector16'/>
</bus>
<bus id='gnd'>
<nodeMember connectorId='connector14'/>
<nodeMember connectorId='connector17'/>
<nodeMember connectorId='connector19'/>
</bus>
</buses>
</module>
