<?xml version='1.0' encoding='UTF-8'?>
<module fritzingVersion="0.6.2b.07.11.5217" moduleId="b7c86ac27f1d86eafa64253206dff603">
    <author>Brett Hagman, Rogue Robotics, bhagman@roguerobotics.com, http://www.roguerobotics.com/</author>
    <title>Wiring S</title>
    <label>WiringS</label>
    <date>2011-07-20</date>
    <tags>
        <tag>microcontroller</tag>
        <tag>wiring</tag>
        <tag>brain board</tag>
    </tags>
    <properties>
        <property name="Hardware PWM pins">6</property>
        <property name="I/O pins">32</property>
        <property name="CAN Bus ports">0</property>
        <property name="family">Microcontroller Board (Wiring)</property>
        <property name="I2C/TWI ports">1</property>
        <property name="SPI ports">1</property>
        <property name="series">Wiring</property>
        <property name="Analog input pins">8</property>
        <property name="fritzpart version">1.0</property>
        <property name="processor">Atmel ATmega644P(A)</property>
        <property name="URL">http://wiring.org.co/</property>
        <property name="Regulated voltages">5V, 3.3V</property>
        <property name="Serial ports">2</property>
        <property name="Supply voltage">7.5 to 12 VDC, or USB 5V</property>
        <property name="part number">Wiring S</property>
        <property name="variant">S</property>
    </properties>
    <description>An open source hardware platform based on the Atmel ATmega644P(A) microcontroller.  Programmable and powered via USB.  Can also be powered by external power supply.
http://wiring.org.co/</description>
    <views>
        <iconView>
            <layers image="icon/Wiring_Sa99.svg">
                <layer layerId="icon"/>
            </layers>
        </iconView>
        <breadboardView>
            <layers image="breadboard/Wiring_Sa99.svg">
                <layer layerId="breadboardbreadboard"/>
            </layers>
        </breadboardView>
        <schematicView>
            <layers image="schematic/Wiring_Sa99.svg">
                <layer layerId="schematic"/>
            </layers>
        </schematicView>
        <pcbView>
            <layers image="pcb/Wiring_Sa99.svg">
                <layer layerId="copper0"/>
                <layer layerId="copper1"/>
            </layers>
        </pcbView>
    </views>
    <connectors>
        <connector type="female" id="connector3" name="D3/TX1">
            <description>Digital I/O 3, Serial Transmit 1</description>
            <views>
                <breadboardView>
                    <p svgId="connector3pin" layer="breadboardbreadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector3" layer="schematic" terminalId="connector3terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector3" layer="copper0"/>
                    <p svgId="connector3" layer="copper1"/>
                </pcbView>
            </views>
        </connector>
        <connector type="female" id="connector20" name="D20">
            <description>Digital I/O 20, SPI SS (Slave)</description>
            <views>
                <breadboardView>
                    <p svgId="connector20pin" layer="breadboardbreadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector20" layer="schematic" terminalId="connector20terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector20" layer="copper0"/>
                    <p svgId="connector20" layer="copper1"/>
                </pcbView>
            </views>
        </connector>
        <connector type="female" id="connector4" name="D4">
            <description>Digital I/O 4, PWM</description>
            <views>
                <breadboardView>
                    <p svgId="connector4pin" layer="breadboardbreadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector4" layer="schematic" terminalId="connector4terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector4" layer="copper0"/>
                    <p svgId="connector4" layer="copper1"/>
                </pcbView>
            </views>
        </connector>
        <connector type="female" id="connector21" name="D21">
            <description>Digital I/O 21, SPI MOSI</description>
            <views>
                <breadboardView>
                    <p svgId="connector21pin" layer="breadboardbreadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector21" layer="schematic" terminalId="connector21terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector21" layer="copper0"/>
                    <p svgId="connector21" layer="copper1"/>
                </pcbView>
            </views>
        </connector>
        <connector type="female" id="connector5" name="D5">
            <description>Digital I/O 5, PWM</description>
            <views>
                <breadboardView>
                    <p svgId="connector5pin" layer="breadboardbreadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector5" layer="schematic" terminalId="connector5terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector5" layer="copper0"/>
                    <p svgId="connector5" layer="copper1"/>
                </pcbView>
            </views>
        </connector>
        <connector type="female" id="connector22" name="D22">
            <description>Digital I/O 22, SPI MISO</description>
            <views>
                <breadboardView>
                    <p svgId="connector22pin" layer="breadboardbreadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector22" layer="schematic" terminalId="connector22terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector22" layer="copper0"/>
                    <p svgId="connector22" layer="copper1"/>
                </pcbView>
            </views>
        </connector>
        <connector type="female" id="connector6" name="D6">
            <description>Digital I/O 6, PWM</description>
            <views>
                <breadboardView>
                    <p svgId="connector6pin" layer="breadboardbreadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector6" layer="schematic" terminalId="connector6terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector6" layer="copper0"/>
                    <p svgId="connector6" layer="copper1"/>
                </pcbView>
            </views>
        </connector>
        <connector type="female" id="connector7" name="D7">
            <description>Digital I/O 7, PWM</description>
            <views>
                <breadboardView>
                    <p svgId="connector7pin" layer="breadboardbreadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector7" layer="schematic" terminalId="connector7terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector7" layer="copper0"/>
                    <p svgId="connector7" layer="copper1"/>
                </pcbView>
            </views>
        </connector>
        <connector type="female" id="connector23" name="D23">
            <description>Digital I/O 23, SPI SCK</description>
            <views>
                <breadboardView>
                    <p svgId="connector23pin" layer="breadboardbreadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector23" layer="schematic" terminalId="connector23terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector23" layer="copper0"/>
                    <p svgId="connector23" layer="copper1"/>
                </pcbView>
            </views>
        </connector>
        <connector type="female" id="connector8" name="D8">
            <description>Digital I/O 8, I2C/TWI SCL</description>
            <views>
                <breadboardView>
                    <p svgId="connector8pin" layer="breadboardbreadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector8" layer="schematic" terminalId="connector8terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector8" layer="copper0"/>
                    <p svgId="connector8" layer="copper1"/>
                </pcbView>
            </views>
        </connector>
        <connector type="female" id="connector24" name="D24">
            <description>Digital I/O 24, Analog Input 0</description>
            <views>
                <breadboardView>
                    <p svgId="connector24pin" layer="breadboardbreadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector24" layer="schematic" terminalId="connector24terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector24" layer="copper0"/>
                    <p svgId="connector24" layer="copper1"/>
                </pcbView>
            </views>
        </connector>
        <connector type="female" id="connector9" name="D9">
            <description>Digital I/O 9, I2C/TWI SDA</description>
            <views>
                <breadboardView>
                    <p svgId="connector9pin" layer="breadboardbreadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector9" layer="schematic" terminalId="connector9terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector9" layer="copper0"/>
                    <p svgId="connector9" layer="copper1"/>
                </pcbView>
            </views>
        </connector>
        <connector type="female" id="connector25" name="D25">
            <description>Digital I/O 25, Analog Input 1</description>
            <views>
                <breadboardView>
                    <p svgId="connector25pin" layer="breadboardbreadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector25" layer="schematic" terminalId="connector25terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector25" layer="copper0"/>
                    <p svgId="connector25" layer="copper1"/>
                </pcbView>
            </views>
        </connector>
        <connector type="female" id="connector26" name="D26">
            <description>Digital I/O 26, Analog Input 2</description>
            <views>
                <breadboardView>
                    <p svgId="connector26pin" layer="breadboardbreadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector26" layer="schematic" terminalId="connector26terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector26" layer="copper0"/>
                    <p svgId="connector26" layer="copper1"/>
                </pcbView>
            </views>
        </connector>
        <connector type="female" id="connector27" name="D27">
            <description>Digital I/O 27, Analog Input 3</description>
            <views>
                <breadboardView>
                    <p svgId="connector27pin" layer="breadboardbreadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector27" layer="schematic" terminalId="connector27terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector27" layer="copper0"/>
                    <p svgId="connector27" layer="copper1"/>
                </pcbView>
            </views>
        </connector>
        <connector type="female" id="connector28" name="D28">
            <description>Digital I/O 28, Analog Input 4</description>
            <views>
                <breadboardView>
                    <p svgId="connector28pin" layer="breadboardbreadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector28" layer="schematic" terminalId="connector28terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector28" layer="copper0"/>
                    <p svgId="connector28" layer="copper1"/>
                </pcbView>
            </views>
        </connector>
        <connector type="female" id="connector29" name="D29">
            <description>Digital I/O 29, Analog Input 5</description>
            <views>
                <breadboardView>
                    <p svgId="connector29pin" layer="breadboardbreadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector29" layer="schematic" terminalId="connector29terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector29" layer="copper0"/>
                    <p svgId="connector29" layer="copper1"/>
                </pcbView>
            </views>
        </connector>
        <connector type="female" id="connector30" name="D30">
            <description>Digital I/O 30, Analog Input 6</description>
            <views>
                <breadboardView>
                    <p svgId="connector30pin" layer="breadboardbreadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector30" layer="schematic" terminalId="connector30terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector30" layer="copper0"/>
                    <p svgId="connector30" layer="copper1"/>
                </pcbView>
            </views>
        </connector>
        <connector type="female" id="connector31" name="D31">
            <description>Digital I/O 31, Analog Input 7</description>
            <views>
                <breadboardView>
                    <p svgId="connector31pin" layer="breadboardbreadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector31" layer="schematic" terminalId="connector31terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector31" layer="copper0"/>
                    <p svgId="connector31" layer="copper1"/>
                </pcbView>
            </views>
        </connector>
        <connector type="female" id="connector32" name="RESET">
            <description>Reset</description>
            <views>
                <breadboardView>
                    <p svgId="connector32pin" layer="breadboardbreadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector32" layer="schematic" terminalId="connector32terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector32" layer="copper0"/>
                    <p svgId="connector32" layer="copper1"/>
                </pcbView>
            </views>
        </connector>
        <connector type="female" id="connector33" name="AREF">
            <description>Analog Input External Voltage Reference</description>
            <views>
                <breadboardView>
                    <p svgId="connector33pin" layer="breadboardbreadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector33" layer="schematic" terminalId="connector33terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector33" layer="copper0"/>
                    <p svgId="connector33" layer="copper1"/>
                </pcbView>
            </views>
        </connector>
        <connector type="female" id="connector34" name="3.3V">
            <description>3.3 Volt Power Supply</description>
            <views>
                <breadboardView>
                    <p svgId="connector34pin" layer="breadboardbreadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector34" layer="schematic" terminalId="connector34terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector34" layer="copper0"/>
                    <p svgId="connector34" layer="copper1"/>
                </pcbView>
            </views>
        </connector>
        <connector type="female" id="connector35" name="3.3V">
            <description>3.3 Volt Power Supply</description>
            <views>
                <breadboardView>
                    <p svgId="connector35pin" layer="breadboardbreadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector35" layer="schematic" terminalId="connector35terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector35" layer="copper0"/>
                    <p svgId="connector35" layer="copper1"/>
                </pcbView>
            </views>
        </connector>
        <connector type="female" id="connector36" name="GND">
            <description>Ground</description>
            <views>
                <breadboardView>
                    <p svgId="connector36pin" layer="breadboardbreadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector36" layer="schematic" terminalId="connector36terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector36" layer="copper0"/>
                    <p svgId="connector36" layer="copper1"/>
                </pcbView>
            </views>
        </connector>
        <connector type="female" id="connector37" name="GND">
            <description>Ground</description>
            <views>
                <breadboardView>
                    <p svgId="connector37pin" layer="breadboardbreadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector37" layer="schematic" terminalId="connector37terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector37" layer="copper0"/>
                    <p svgId="connector37" layer="copper1"/>
                </pcbView>
            </views>
        </connector>
        <connector type="female" id="connector38" name="5V">
            <description>5 Volt Power Supply</description>
            <views>
                <breadboardView>
                    <p svgId="connector38pin" layer="breadboardbreadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector38" layer="schematic" terminalId="connector38terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector38" layer="copper0"/>
                    <p svgId="connector38" layer="copper1"/>
                </pcbView>
            </views>
        </connector>
        <connector type="female" id="connector39" name="5V">
            <description>5 Volt Power Supply</description>
            <views>
                <breadboardView>
                    <p svgId="connector39pin" layer="breadboardbreadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector39" layer="schematic" terminalId="connector39terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector39" layer="copper0"/>
                    <p svgId="connector39" layer="copper1"/>
                </pcbView>
            </views>
        </connector>
        <connector type="female" id="connector10" name="D10">
            <description>Digital I/O 10</description>
            <views>
                <breadboardView>
                    <p svgId="connector10pin" layer="breadboardbreadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector10" layer="schematic" terminalId="connector10terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector10" layer="copper0"/>
                    <p svgId="connector10" layer="copper1"/>
                </pcbView>
            </views>
        </connector>
        <connector type="female" id="connector11" name="D11">
            <description>Digital I/O 11</description>
            <views>
                <breadboardView>
                    <p svgId="connector11pin" layer="breadboardbreadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector11" layer="schematic" terminalId="connector11terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector11" layer="copper0"/>
                    <p svgId="connector11" layer="copper1"/>
                </pcbView>
            </views>
        </connector>
        <connector type="female" id="connector12" name="D12">
            <description>Digital I/O 12</description>
            <views>
                <breadboardView>
                    <p svgId="connector12pin" layer="breadboardbreadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector12" layer="schematic" terminalId="connector12terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector12" layer="copper0"/>
                    <p svgId="connector12" layer="copper1"/>
                </pcbView>
            </views>
        </connector>
        <connector type="female" id="connector13" name="D13">
            <description>Digital I/O 13</description>
            <views>
                <breadboardView>
                    <p svgId="connector13pin" layer="breadboardbreadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector13" layer="schematic" terminalId="connector13terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector13" layer="copper0"/>
                    <p svgId="connector13" layer="copper1"/>
                </pcbView>
            </views>
        </connector>
        <connector type="female" id="connector14" name="D14">
            <description>Digital I/O 14</description>
            <views>
                <breadboardView>
                    <p svgId="connector14pin" layer="breadboardbreadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector14" layer="schematic" terminalId="connector14terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector14" layer="copper0"/>
                    <p svgId="connector14" layer="copper1"/>
                </pcbView>
            </views>
        </connector>
        <connector type="female" id="connector15" name="D15">
            <description>Digital I/O 15</description>
            <views>
                <breadboardView>
                    <p svgId="connector15pin" layer="breadboardbreadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector15" layer="schematic" terminalId="connector15terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector15" layer="copper0"/>
                    <p svgId="connector15" layer="copper1"/>
                </pcbView>
            </views>
        </connector>
        <connector type="female" id="connector16" name="D16">
            <description>Digital I/O 16</description>
            <views>
                <breadboardView>
                    <p svgId="connector16pin" layer="breadboardbreadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector16" layer="schematic" terminalId="connector16terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector16" layer="copper0"/>
                    <p svgId="connector16" layer="copper1"/>
                </pcbView>
            </views>
        </connector>
        <connector type="female" id="connector17" name="D17">
            <description>Digital I/O 17</description>
            <views>
                <breadboardView>
                    <p svgId="connector17pin" layer="breadboardbreadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector17" layer="schematic" terminalId="connector17terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector17" layer="copper0"/>
                    <p svgId="connector17" layer="copper1"/>
                </pcbView>
            </views>
        </connector>
        <connector type="female" id="connector18" name="D18">
            <description>Digital I/O 18</description>
            <views>
                <breadboardView>
                    <p svgId="connector18pin" layer="breadboardbreadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector18" layer="schematic" terminalId="connector18terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector18" layer="copper0"/>
                    <p svgId="connector18" layer="copper1"/>
                </pcbView>
            </views>
        </connector>
        <connector type="female" id="connector19" name="D19">
            <description>Digital I/O 19</description>
            <views>
                <breadboardView>
                    <p svgId="connector19pin" layer="breadboardbreadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector19" layer="schematic" terminalId="connector19terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector19" layer="copper0"/>
                    <p svgId="connector19" layer="copper1"/>
                </pcbView>
            </views>
        </connector>
        <connector type="female" id="connector0" name="D0/RX0">
            <description>Digital I/O 0, Serial Receive 0</description>
            <views>
                <breadboardView>
                    <p svgId="connector0pin" layer="breadboardbreadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector0" layer="schematic" terminalId="connector0terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector0" layer="copper0"/>
                    <p svgId="connector0" layer="copper1"/>
                </pcbView>
            </views>
        </connector>
        <connector type="female" id="connector1" name="D1/TX0">
            <description>Digital I/O 1, Serial Transmit 0</description>
            <views>
                <breadboardView>
                    <p svgId="connector1pin" layer="breadboardbreadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector1" layer="schematic" terminalId="connector1terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector1" layer="copper0"/>
                    <p svgId="connector1" layer="copper1"/>
                </pcbView>
            </views>
        </connector>
        <connector type="female" id="connector2" name="D2/RX1">
            <description>Digital I/O 2, Serial Receive 1</description>
            <views>
                <breadboardView>
                    <p svgId="connector2pin" layer="breadboardbreadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector2" layer="schematic" terminalId="connector2terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector2" layer="copper0"/>
                    <p svgId="connector2" layer="copper1"/>
                </pcbView>
            </views>
        </connector>
    </connectors>
</module>
