<?xml version='1.0' encoding='UTF-8'?>
<module moduleId="chipkit_MX4" referenceFile="chipkit_MX4.fzp">
 <version>4</version>
 <author>Amber Mear/Digilent Inc.</author>
 <title>chipKIT™Pro MX4</title>
 <label>MX4</label>
 <date>Fri Feb 21 2014</date>
 <tags>
  <tag>DIP</tag>
  <tag>fritzing core</tag>
 </tags>
 <properties>
  <property name="family">chipKIT</property>
  <property name="package">MX4</property>
  <property name="variant">variant 3</property>
 </properties>
 <taxonomy>part.dip.108.pins</taxonomy>
 <description>&lt;!DOCTYPE HTML PUBLIC "-//W3C//DTD HTML 4.0//EN" "http://www.w3.org/TR/REC-html40/strict.dtd">
&lt;html>&lt;head>&lt;meta name="qrichtext" content="1" />&lt;style type="text/css">
p, li { white-space: pre-wrap; }
&lt;/style>&lt;/head>&lt;body style=" font-family:'MS Shell Dlg 2'; font-size:8.25pt; font-weight:400; font-style:normal;">
&lt;p style=" margin-top:0px; margin-bottom:0px; margin-left:0px; margin-right:0px; -qt-block-indent:0; text-indent:0px;">&lt;span style=" font-family:'Arial,Geneva,Verdana,Helvetica'; font-size:14px; color:#000000; background-color:#fffffd;">The chipKIT™ Pro MX4 is a microcontroller development board based on the Microchip PIC32MX460F512L, a member of the 32-bit PIC32 microcontroller family. It is compatible with Digilent’s line of Pmod™ peripheral modules, and is suitable for use with the Microchip MPLAB® IDE tools. The chipKIT Pro MX4 is also compatible for use with the chipKIT™ MPIDE development environment. ChipKIT and MPIDE is a PIC32 based system compatible with many existing Arduino™ code examples, reference materials and other resources.  The chipKIT Pro MX4 is designed to be easy to use and suitable for use by anyone from beginners to advanced users for experimenting with electronics and embedded control systems. A built in programming/debugging circuit compatible with the Microchip MPLAB® IDE is provided on the board, so no additional hardware is required for use with MPLAB. The kit contains everything needed to start developing embedded applications using either the MPLAB® IDE or the MPIDE.  The chipKIT Pro MX4 provides 74 I/O pins that support a number of peripheral functions, such as USB controller, UART, SPI and I2C™ ports as well as five pulse width modulated outputs and five external interrupt inputs. Fifteen of the I/O pins can be used as analog inputs in addition to their use as digital inputs and outputs..  The chipKIT Pro MX4 can be powered via USB, or an external power supply that may be either an AC-DC power adapter, or batteries.&lt;/span>&lt;/p>&lt;/body>&lt;/html></description>
 <views>
  <iconView>
   <layers image="icon/chipkit_MX4_icon.svg">
    <layer layerId="icon"/>
   </layers>
  </iconView>
  <breadboardView>
   <layers image="breadboard/chipkit_MX4_breadboard.svg">
    <layer layerId="breadboard"/>
   </layers>
  </breadboardView>
  <schematicView>
   <layers image="schematic/chipkit_MX4_schematic.svg">
    <layer layerId="schematic"/>
   </layers>
  </schematicView>
  <pcbView>
   <layers image="pcb/chipkit_MX4_pcb.svg">
    <layer layerId="silkscreen"/>
    <layer layerId="copper0"/>
    <layer layerId="copper1"/>
   </layers>
  </pcbView>
 </views>
 <connectors>
  <connector type="female" id="connector0" name="VDD">
   <description>pin 1</description>
   <views>
    <breadboardView>
     <p svgId="connector0pin" layer="breadboard" terminalId="connector0terminal"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector0pin" layer="schematic" terminalId="connector0terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector0pin" layer="copper0"/>
     <p svgId="connector0pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector type="female" id="connector1" name="GND">
   <description>pin 2</description>
   <views>
    <breadboardView>
     <p svgId="connector1pin" layer="breadboard" terminalId="connector1terminal"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector1pin" layer="schematic" terminalId="connector1terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector1pin" layer="copper0"/>
     <p svgId="connector1pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector type="female" id="connector2" name="RC4">
   <description>pin 3</description>
   <views>
    <breadboardView>
     <p svgId="connector2pin" layer="breadboard" terminalId="connector2terminal"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector2pin" layer="schematic" terminalId="connector2terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector2pin" layer="copper0"/>
     <p svgId="connector2pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector type="female" id="connector3" name="RD12">
   <description>pin 4</description>
   <views>
    <breadboardView>
     <p svgId="connector3pin" layer="breadboard" terminalId="connector3terminal"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector3pin" layer="schematic" terminalId="connector3terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector3pin" layer="copper0"/>
     <p svgId="connector3pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector type="female" id="connector4" name="RA10">
   <description>pin 5</description>
   <views>
    <breadboardView>
     <p svgId="connector4pin" layer="breadboard" terminalId="connector4terminal"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector4pin" layer="schematic" terminalId="connector4terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector4pin" layer="copper0"/>
     <p svgId="connector4pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector type="female" id="connector5" name="RA9">
   <description>pin 6</description>
   <views>
    <breadboardView>
     <p svgId="connector5pin" layer="breadboard" terminalId="connector5terminal"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector5pin" layer="schematic" terminalId="connector5terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector5pin" layer="copper0"/>
     <p svgId="connector5pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector type="female" id="connector6" name="VDD">
   <description>pin 7</description>
   <views>
    <breadboardView>
     <p svgId="connector6pin" layer="breadboard" terminalId="connector6terminal"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector6pin" layer="schematic" terminalId="connector6terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector6pin" layer="copper0"/>
     <p svgId="connector6pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector type="female" id="connector7" name="GND">
   <description>pin 8</description>
   <views>
    <breadboardView>
     <p svgId="connector7pin" layer="breadboard" terminalId="connector7terminal"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector7pin" layer="schematic" terminalId="connector7terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector7pin" layer="copper0"/>
     <p svgId="connector7pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector type="female" id="connector8" name="RB13">
   <description>pin 9</description>
   <views>
    <breadboardView>
     <p svgId="connector8pin" layer="breadboard" terminalId="connector8terminal"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector8pin" layer="schematic" terminalId="connector8terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector8pin" layer="copper0"/>
     <p svgId="connector8pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector type="female" id="connector9" name="RB12">
   <description>pin 10</description>
   <views>
    <breadboardView>
     <p svgId="connector9pin" layer="breadboard" terminalId="connector9terminal"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector9pin" layer="schematic" terminalId="connector9terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector9pin" layer="copper0"/>
     <p svgId="connector9pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector type="female" id="connector10" name="RB11">
   <description>pin 11</description>
   <views>
    <breadboardView>
     <p svgId="connector10pin" layer="breadboard" terminalId="connector10terminal"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector10pin" layer="schematic" terminalId="connector10terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector10pin" layer="copper0"/>
     <p svgId="connector10pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector type="female" id="connector11" name="RB10">
   <description>pin 12</description>
   <views>
    <breadboardView>
     <p svgId="connector11pin" layer="breadboard" terminalId="connector11terminal"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector11pin" layer="schematic" terminalId="connector11terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector11pin" layer="copper0"/>
     <p svgId="connector11pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector type="female" id="connector12" name="VDD">
   <description>pin 13</description>
   <views>
    <breadboardView>
     <p svgId="connector12pin" layer="breadboard" terminalId="connector12terminal"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector12pin" layer="schematic" terminalId="connector12terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector12pin" layer="copper0"/>
     <p svgId="connector12pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector type="female" id="connector13" name="GND">
   <description>pin 14</description>
   <views>
    <breadboardView>
     <p svgId="connector13pin" layer="breadboard" terminalId="connector13terminal"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector13pin" layer="schematic" terminalId="connector13terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector13pin" layer="copper0"/>
     <p svgId="connector13pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector type="female" id="connector14" name="RB9">
   <description>pin 15</description>
   <views>
    <breadboardView>
     <p svgId="connector14pin" layer="breadboard" terminalId="connector14terminal"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector14pin" layer="schematic" terminalId="connector14terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector14pin" layer="copper0"/>
     <p svgId="connector14pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector type="female" id="connector15" name="RB8">
   <description>pin 16</description>
   <views>
    <breadboardView>
     <p svgId="connector15pin" layer="breadboard" terminalId="connector15terminal"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector15pin" layer="schematic" terminalId="connector15terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector15pin" layer="copper0"/>
     <p svgId="connector15pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector type="female" id="connector16" name="RB5">
   <description>pin 17</description>
   <views>
    <breadboardView>
     <p svgId="connector16pin" layer="breadboard" terminalId="connector16terminal"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector16pin" layer="schematic" terminalId="connector16terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector16pin" layer="copper0"/>
     <p svgId="connector16pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector type="female" id="connector17" name="RB4">
   <description>pin 18</description>
   <views>
    <breadboardView>
     <p svgId="connector17pin" layer="breadboard" terminalId="connector17terminal"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector17pin" layer="schematic" terminalId="connector17terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector17pin" layer="copper0"/>
     <p svgId="connector17pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector type="female" id="connector18" name="VDD">
   <description>pin 19</description>
   <views>
    <breadboardView>
     <p svgId="connector18pin" layer="breadboard" terminalId="connector18terminal"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector18pin" layer="schematic" terminalId="connector18terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector18pin" layer="copper0"/>
     <p svgId="connector18pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector type="female" id="connector19" name="GND">
   <description>pin 20</description>
   <views>
    <breadboardView>
     <p svgId="connector19pin" layer="breadboard" terminalId="connector19terminal"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector19pin" layer="schematic" terminalId="connector19terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector19pin" layer="copper0"/>
     <p svgId="connector19pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector type="female" id="connector20" name="RB3">
   <description>pin 21</description>
   <views>
    <breadboardView>
     <p svgId="connector20pin" layer="breadboard" terminalId="connector20terminal"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector20pin" layer="schematic" terminalId="connector20terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector20pin" layer="copper0"/>
     <p svgId="connector20pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector type="female" id="connector21" name="RB2">
   <description>pin 22</description>
   <views>
    <breadboardView>
     <p svgId="connector21pin" layer="breadboard" terminalId="connector21terminal"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector21pin" layer="schematic" terminalId="connector21terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector21pin" layer="copper0"/>
     <p svgId="connector21pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector type="female" id="connector22" name="RB1">
   <description>pin 23</description>
   <views>
    <breadboardView>
     <p svgId="connector22pin" layer="breadboard" terminalId="connector22terminal"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector22pin" layer="schematic" terminalId="connector22terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector22pin" layer="copper0"/>
     <p svgId="connector22pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector type="female" id="connector23" name="RB0">
   <description>pin 24</description>
   <views>
    <breadboardView>
     <p svgId="connector23pin" layer="breadboard" terminalId="connector23terminal"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector23pin" layer="schematic" terminalId="connector23terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector23pin" layer="copper0"/>
     <p svgId="connector23pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector type="female" id="connector24" name="VDD">
   <description>pin 25</description>
   <views>
    <breadboardView>
     <p svgId="connector24pin" layer="breadboard" terminalId="connector24terminal"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector24pin" layer="schematic" terminalId="connector24terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector24pin" layer="copper0"/>
     <p svgId="connector24pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector type="female" id="connector25" name="GND">
   <description>pin 26</description>
   <views>
    <breadboardView>
     <p svgId="connector25pin" layer="breadboard" terminalId="connector25terminal"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector25pin" layer="schematic" terminalId="connector25terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector25pin" layer="copper0"/>
     <p svgId="connector25pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector type="female" id="connector26" name="RD13">
   <description>pin 27</description>
   <views>
    <breadboardView>
     <p svgId="connector26pin" layer="breadboard" terminalId="connector26terminal"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector26pin" layer="schematic" terminalId="connector26terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector26pin" layer="copper0"/>
     <p svgId="connector26pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector type="female" id="connector27" name="RD8">
   <description>pin 28</description>
   <views>
    <breadboardView>
     <p svgId="connector27pin" layer="breadboard" terminalId="connector27terminal"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector27pin" layer="schematic" terminalId="connector27terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector27pin" layer="copper0"/>
     <p svgId="connector27pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector type="female" id="connector28" name="RD0">
   <description>pin 29</description>
   <views>
    <breadboardView>
     <p svgId="connector28pin" layer="breadboard" terminalId="connector28terminal"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector28pin" layer="schematic" terminalId="connector28terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector28pin" layer="copper0"/>
     <p svgId="connector28pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector type="female" id="connector29" name="RE8">
   <description>pin 30</description>
   <views>
    <breadboardView>
     <p svgId="connector29pin" layer="breadboard" terminalId="connector29terminal"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector29pin" layer="schematic" terminalId="connector29terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector29pin" layer="copper0"/>
     <p svgId="connector29pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector type="female" id="connector30" name="VDD">
   <description>pin 31</description>
   <views>
    <breadboardView>
     <p svgId="connector30pin" layer="breadboard" terminalId="connector30terminal"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector30pin" layer="schematic" terminalId="connector30terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector30pin" layer="copper0"/>
     <p svgId="connector30pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector type="female" id="connector31" name="GND">
   <description>pin 32</description>
   <views>
    <breadboardView>
     <p svgId="connector31pin" layer="breadboard" terminalId="connector31terminal"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector31pin" layer="schematic" terminalId="connector31terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector31pin" layer="copper0"/>
     <p svgId="connector31pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector type="female" id="connector32" name="RF13">
   <description>pin 33</description>
   <views>
    <breadboardView>
     <p svgId="connector32pin" layer="breadboard" terminalId="connector32terminal"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector32pin" layer="schematic" terminalId="connector32terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector32pin" layer="copper0"/>
     <p svgId="connector32pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector type="female" id="connector33" name="RF4">
   <description>pin 34</description>
   <views>
    <breadboardView>
     <p svgId="connector33pin" layer="breadboard" terminalId="connector33terminal"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector33pin" layer="schematic" terminalId="connector33terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector33pin" layer="copper0"/>
     <p svgId="connector33pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector type="female" id="connector34" name="RF5">
   <description>pin 35</description>
   <views>
    <breadboardView>
     <p svgId="connector34pin" layer="breadboard" terminalId="connector34terminal"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector34pin" layer="schematic" terminalId="connector34terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector34pin" layer="copper0"/>
     <p svgId="connector34pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector type="female" id="connector35" name="RF12">
   <description>pin 36</description>
   <views>
    <breadboardView>
     <p svgId="connector35pin" layer="breadboard" terminalId="connector35terminal"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector35pin" layer="schematic" terminalId="connector35terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector35pin" layer="copper0"/>
     <p svgId="connector35pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector type="female" id="connector36" name="RE0">
   <description>pin 37</description>
   <views>
    <breadboardView>
     <p svgId="connector36pin" layer="breadboard" terminalId="connector36terminal"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector36pin" layer="schematic" terminalId="connector36terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector36pin" layer="copper0"/>
     <p svgId="connector36pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector type="female" id="connector37" name="RE1">
   <description>pin 38</description>
   <views>
    <breadboardView>
     <p svgId="connector37pin" layer="breadboard" terminalId="connector37terminal"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector37pin" layer="schematic" terminalId="connector37terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector37pin" layer="copper0"/>
     <p svgId="connector37pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector type="female" id="connector38" name="RE2">
   <description>pin 39</description>
   <views>
    <breadboardView>
     <p svgId="connector38pin" layer="breadboard" terminalId="connector38terminal"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector38pin" layer="schematic" terminalId="connector38terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector38pin" layer="copper0"/>
     <p svgId="connector38pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector type="female" id="connector39" name="RE3">
   <description>pin 40</description>
   <views>
    <breadboardView>
     <p svgId="connector39pin" layer="breadboard" terminalId="connector39terminal"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector39pin" layer="schematic" terminalId="connector39terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector39pin" layer="copper0"/>
     <p svgId="connector39pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector type="female" id="connector40" name="GND">
   <description>pin 41</description>
   <views>
    <breadboardView>
     <p svgId="connector40pin" layer="breadboard" terminalId="connector40terminal"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector40pin" layer="schematic" terminalId="connector40terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector40pin" layer="copper0"/>
     <p svgId="connector40pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector type="female" id="connector41" name="VDD">
   <description>pin 42</description>
   <views>
    <breadboardView>
     <p svgId="connector41pin" layer="breadboard" terminalId="connector41terminal"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector41pin" layer="schematic" terminalId="connector41terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector41pin" layer="copper0"/>
     <p svgId="connector41pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector type="female" id="connector42" name="RE4">
   <description>pin 43</description>
   <views>
    <breadboardView>
     <p svgId="connector42pin" layer="breadboard" terminalId="connector42terminal"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector42pin" layer="schematic" terminalId="connector42terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector42pin" layer="copper0"/>
     <p svgId="connector42pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector type="female" id="connector43" name="RE5">
   <description>pin 44</description>
   <views>
    <breadboardView>
     <p svgId="connector43pin" layer="breadboard" terminalId="connector43terminal"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector43pin" layer="schematic" terminalId="connector43terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector43pin" layer="copper0"/>
     <p svgId="connector43pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector type="male" id="connector44" name="RE6">
   <description>pin 45</description>
   <views>
    <breadboardView>
     <p svgId="connector44pin" layer="breadboard" terminalId="connector44terminal"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector44pin" layer="schematic" terminalId="connector44terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector44pin" layer="copper0"/>
     <p svgId="connector44pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector type="female" id="connector45" name="RE7">
   <description>pin 46</description>
   <views>
    <breadboardView>
     <p svgId="connector45pin" layer="breadboard" terminalId="connector45terminal"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector45pin" layer="schematic" terminalId="connector45terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector45pin" layer="copper0"/>
     <p svgId="connector45pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector type="female" id="connector46" name="GND">
   <description>pin 47</description>
   <views>
    <breadboardView>
     <p svgId="connector46pin" layer="breadboard" terminalId="connector46terminal"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector46pin" layer="schematic" terminalId="connector46terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector46pin" layer="copper0"/>
     <p svgId="connector46pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector type="female" id="connector47" name="VDD">
   <description>pin 48</description>
   <views>
    <breadboardView>
     <p svgId="connector47pin" layer="breadboard" terminalId="connector47terminal"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector47pin" layer="schematic" terminalId="connector47terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector47pin" layer="copper0"/>
     <p svgId="connector47pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector type="female" id="connector48" name="RG9">
   <description>pin 49</description>
   <views>
    <breadboardView>
     <p svgId="connector48pin" layer="breadboard" terminalId="connector48terminal"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector48pin" layer="schematic" terminalId="connector48terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector48pin" layer="copper0"/>
     <p svgId="connector48pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector type="female" id="connector49" name="RG8">
   <description>pin 50</description>
   <views>
    <breadboardView>
     <p svgId="connector49pin" layer="breadboard" terminalId="connector49terminal"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector49pin" layer="schematic" terminalId="connector49terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector49pin" layer="copper0"/>
     <p svgId="connector49pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector type="female" id="connector50" name="RG7">
   <description>pin 51</description>
   <views>
    <breadboardView>
     <p svgId="connector50pin" layer="breadboard" terminalId="connector50terminal"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector50pin" layer="schematic" terminalId="connector50terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector50pin" layer="copper0"/>
     <p svgId="connector50pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector type="female" id="connector51" name="RG6">
   <description>pin 52</description>
   <views>
    <breadboardView>
     <p svgId="connector51pin" layer="breadboard" terminalId="connector51terminal"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector51pin" layer="schematic" terminalId="connector51terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector51pin" layer="copper0"/>
     <p svgId="connector51pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector type="female" id="connector52" name="GND">
   <description>pin 53</description>
   <views>
    <breadboardView>
     <p svgId="connector52pin" layer="breadboard" terminalId="connector52terminal"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector52pin" layer="schematic" terminalId="connector52terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector52pin" layer="copper0"/>
     <p svgId="connector52pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector type="female" id="connector53" name="VDD">
   <description>pin 54</description>
   <views>
    <breadboardView>
     <p svgId="connector53pin" layer="breadboard" terminalId="connector53terminal"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector53pin" layer="schematic" terminalId="connector53terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector53pin" layer="copper0"/>
     <p svgId="connector53pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector type="female" id="connector54" name="RB15">
   <description>pin 55</description>
   <views>
    <breadboardView>
     <p svgId="connector54pin" layer="breadboard" terminalId="connector54terminal"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector54pin" layer="schematic" terminalId="connector54terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector54pin" layer="copper0"/>
     <p svgId="connector54pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector type="female" id="connector55" name="RD5">
   <description>pin 56</description>
   <views>
    <breadboardView>
     <p svgId="connector55pin" layer="breadboard" terminalId="connector55terminal"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector55pin" layer="schematic" terminalId="connector55terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector55pin" layer="copper0"/>
     <p svgId="connector55pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector type="female" id="connector56" name="RD4">
   <description>pin 57</description>
   <views>
    <breadboardView>
     <p svgId="connector56pin" layer="breadboard" terminalId="connector56terminal"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector56pin" layer="schematic" terminalId="connector56terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector56pin" layer="copper0"/>
     <p svgId="connector56pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector type="female" id="connector57" name="RB14">
   <description>pin 58</description>
   <views>
    <breadboardView>
     <p svgId="connector57pin" layer="breadboard" terminalId="connector57terminal"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector57pin" layer="schematic" terminalId="connector57terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector57pin" layer="copper0"/>
     <p svgId="connector57pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector type="female" id="connector58" name="GND">
   <description>pin 59</description>
   <views>
    <breadboardView>
     <p svgId="connector58pin" layer="breadboard" terminalId="connector58terminal"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector58pin" layer="schematic" terminalId="connector58terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector58pin" layer="copper0"/>
     <p svgId="connector58pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector type="female" id="connector59" name="VDD">
   <description>pin 60</description>
   <views>
    <breadboardView>
     <p svgId="connector59pin" layer="breadboard" terminalId="connector59terminal"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector59pin" layer="schematic" terminalId="connector59terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector59pin" layer="copper0"/>
     <p svgId="connector59pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector type="female" id="connector60" name="RG12">
   <description>pin 61</description>
   <views>
    <breadboardView>
     <p svgId="connector60pin" layer="breadboard" terminalId="connector60terminal"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector60pin" layer="schematic" terminalId="connector60terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector60pin" layer="copper0"/>
     <p svgId="connector60pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector type="female" id="connector61" name="RG13">
   <description>pin 62</description>
   <views>
    <breadboardView>
     <p svgId="connector61pin" layer="breadboard" terminalId="connector61terminal"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector61pin" layer="schematic" terminalId="connector61terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector61pin" layer="copper0"/>
     <p svgId="connector61pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector type="female" id="connector62" name="RG14">
   <description>pin 63</description>
   <views>
    <breadboardView>
     <p svgId="connector62pin" layer="breadboard" terminalId="connector62terminal"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector62pin" layer="schematic" terminalId="connector62terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector62pin" layer="copper0"/>
     <p svgId="connector62pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector type="female" id="connector63" name="RG15">
   <description>pin 64</description>
   <views>
    <breadboardView>
     <p svgId="connector63pin" layer="breadboard" terminalId="connector63terminal"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector63pin" layer="schematic" terminalId="connector63terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector63pin" layer="copper0"/>
     <p svgId="connector63pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector type="female" id="connector64" name="GND">
   <description>pin 65</description>
   <views>
    <breadboardView>
     <p svgId="connector64pin" layer="breadboard" terminalId="connector64terminal"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector64pin" layer="schematic" terminalId="connector64terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector64pin" layer="copper0"/>
     <p svgId="connector64pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector type="female" id="connector65" name="VDD">
   <description>pin 66</description>
   <views>
    <breadboardView>
     <p svgId="connector65pin" layer="breadboard" terminalId="connector65terminal"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector65pin" layer="schematic" terminalId="connector65terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector65pin" layer="copper0"/>
     <p svgId="connector65pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector type="female" id="connector66" name="RG0">
   <description>pin 67</description>
   <views>
    <breadboardView>
     <p svgId="connector66pin" layer="breadboard" terminalId="connector66terminal"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector66pin" layer="schematic" terminalId="connector66terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector66pin" layer="copper0"/>
     <p svgId="connector66pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector type="female" id="connector67" name="RG1">
   <description>pin 68</description>
   <views>
    <breadboardView>
     <p svgId="connector67pin" layer="breadboard" terminalId="connector67terminal"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector67pin" layer="schematic" terminalId="connector67terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector67pin" layer="copper0"/>
     <p svgId="connector67pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector type="female" id="connector68" name="RF0">
   <description>pin 69</description>
   <views>
    <breadboardView>
     <p svgId="connector68pin" layer="breadboard" terminalId="connector68terminal"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector68pin" layer="schematic" terminalId="connector68terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector68pin" layer="copper0"/>
     <p svgId="connector68pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector type="female" id="connector69" name="RF1">
   <description>pin 70</description>
   <views>
    <breadboardView>
     <p svgId="connector69pin" layer="breadboard" terminalId="connector69terminal"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector69pin" layer="schematic" terminalId="connector69terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector69pin" layer="copper0"/>
     <p svgId="connector69pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector type="female" id="connector70" name="GND">
   <description>pin 71</description>
   <views>
    <breadboardView>
     <p svgId="connector70pin" layer="breadboard" terminalId="connector70terminal"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector70pin" layer="schematic" terminalId="connector70terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector70pin" layer="copper0"/>
     <p svgId="connector70pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector type="female" id="connector71" name="VDD">
   <description>pin 72</description>
   <views>
    <breadboardView>
     <p svgId="connector71pin" layer="breadboard" terminalId="connector71terminal"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector71pin" layer="schematic" terminalId="connector71terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector71pin" layer="copper0"/>
     <p svgId="connector71pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector type="female" id="connector72" name="RD7">
   <description>pin 73</description>
   <views>
    <breadboardView>
     <p svgId="connector72pin" layer="breadboard" terminalId="connector72terminal"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector72pin" layer="schematic" terminalId="connector72terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector72pin" layer="copper0"/>
     <p svgId="connector72pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector type="female" id="connector73" name="RD1">
   <description>pin 74</description>
   <views>
    <breadboardView>
     <p svgId="connector73pin" layer="breadboard" terminalId="connector73terminal"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector73pin" layer="schematic" terminalId="connector73terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector73pin" layer="copper0"/>
     <p svgId="connector73pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector type="female" id="connector74" name="RD9">
   <description>pin 75</description>
   <views>
    <breadboardView>
     <p svgId="connector74pin" layer="breadboard" terminalId="connector74terminal"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector74pin" layer="schematic" terminalId="connector74terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector74pin" layer="copper0"/>
     <p svgId="connector74pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector type="female" id="connector75" name="RC1">
   <description>pin 76</description>
   <views>
    <breadboardView>
     <p svgId="connector75pin" layer="breadboard" terminalId="connector75terminal"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector75pin" layer="schematic" terminalId="connector75terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector75pin" layer="copper0"/>
     <p svgId="connector75pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector type="female" id="connector76" name="GND">
   <description>pin 77</description>
   <views>
    <breadboardView>
     <p svgId="connector76pin" layer="breadboard" terminalId="connector76terminal"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector76pin" layer="schematic" terminalId="connector76terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector76pin" layer="copper0"/>
     <p svgId="connector76pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector type="female" id="connector77" name="VDD">
   <description>pin 78</description>
   <views>
    <breadboardView>
     <p svgId="connector77pin" layer="breadboard" terminalId="connector77terminal"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector77pin" layer="schematic" terminalId="connector77terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector77pin" layer="copper0"/>
     <p svgId="connector77pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector type="female" id="connector78" name="RD6">
   <description>pin 79</description>
   <views>
    <breadboardView>
     <p svgId="connector78pin" layer="breadboard" terminalId="connector78terminal"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector78pin" layer="schematic" terminalId="connector78terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector78pin" layer="copper0"/>
     <p svgId="connector78pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector type="female" id="connector79" name="RD2">
   <description>pin 80</description>
   <views>
    <breadboardView>
     <p svgId="connector79pin" layer="breadboard" terminalId="connector79terminal"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector79pin" layer="schematic" terminalId="connector79terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector79pin" layer="copper0"/>
     <p svgId="connector79pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector type="female" id="connector80" name="RD10">
   <description>pin 81</description>
   <views>
    <breadboardView>
     <p svgId="connector80pin" layer="breadboard" terminalId="connector80terminal"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector80pin" layer="schematic" terminalId="connector80terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector80pin" layer="copper0"/>
     <p svgId="connector80pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector type="female" id="connector81" name="RC2">
   <description>pin 82</description>
   <views>
    <breadboardView>
     <p svgId="connector81pin" layer="breadboard" terminalId="connector81terminal"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector81pin" layer="schematic" terminalId="connector81terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector81pin" layer="copper0"/>
     <p svgId="connector81pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector type="female" id="connector82" name="GND">
   <description>pin 83</description>
   <views>
    <breadboardView>
     <p svgId="connector82pin" layer="breadboard" terminalId="connector82terminal"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector82pin" layer="schematic" terminalId="connector82terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector82pin" layer="copper0"/>
     <p svgId="connector82pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector type="female" id="connector83" name="VDD">
   <description>pin 84</description>
   <views>
    <breadboardView>
     <p svgId="connector83pin" layer="breadboard" terminalId="connector83terminal"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector83pin" layer="schematic" terminalId="connector83terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector83pin" layer="copper0"/>
     <p svgId="connector83pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector type="female" id="connector84" name="VDD">
   <description>pin 85</description>
   <views>
    <breadboardView>
     <p svgId="connector84pin" layer="breadboard" terminalId="connector84terminal"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector84pin" layer="schematic" terminalId="connector84terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector84pin" layer="copper0"/>
     <p svgId="connector84pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector type="female" id="connector85" name="GND">
   <description>pin 86</description>
   <views>
    <breadboardView>
     <p svgId="connector85pin" layer="breadboard" terminalId="connector85terminal"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector85pin" layer="schematic" terminalId="connector85terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector85pin" layer="copper0"/>
     <p svgId="connector85pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector type="female" id="connector86" name="RC3">
   <description>pin 87</description>
   <views>
    <breadboardView>
     <p svgId="connector86pin" layer="breadboard" terminalId="connector86terminal"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector86pin" layer="schematic" terminalId="connector86terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector86pin" layer="copper0"/>
     <p svgId="connector86pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector type="female" id="connector87" name="RD11">
   <description>pin 88</description>
   <views>
    <breadboardView>
     <p svgId="connector87pin" layer="breadboard" terminalId="connector87terminal"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector87pin" layer="schematic" terminalId="connector87terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector87pin" layer="copper0"/>
     <p svgId="connector87pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector type="female" id="connector88" name="RD3">
   <description>pin 89</description>
   <views>
    <breadboardView>
     <p svgId="connector88pin" layer="breadboard" terminalId="connector88terminal"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector88pin" layer="schematic" terminalId="connector88terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector88pin" layer="copper0"/>
     <p svgId="connector88pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector type="female" id="connector89" name="RE9">
   <description>pin 90</description>
   <views>
    <breadboardView>
     <p svgId="connector89pin" layer="breadboard" terminalId="connector89terminal"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector89pin" layer="schematic" terminalId="connector89terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector89pin" layer="copper0"/>
     <p svgId="connector89pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector type="female" id="connector90" name="VDD">
   <description>pin 91</description>
   <views>
    <breadboardView>
     <p svgId="connector90pin" layer="breadboard" terminalId="connector90terminal"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector90pin" layer="schematic" terminalId="connector90terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector90pin" layer="copper0"/>
     <p svgId="connector90pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector type="female" id="connector91" name="GND">
   <description>pin 92</description>
   <views>
    <breadboardView>
     <p svgId="connector91pin" layer="breadboard" terminalId="connector91terminal"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector91pin" layer="schematic" terminalId="connector91terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector91pin" layer="copper0"/>
     <p svgId="connector91pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector type="female" id="connector92" name="RD15">
   <description>pin 93</description>
   <views>
    <breadboardView>
     <p svgId="connector92pin" layer="breadboard" terminalId="connector92terminal"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector92pin" layer="schematic" terminalId="connector92terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector92pin" layer="copper0"/>
     <p svgId="connector92pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector type="female" id="connector93" name="RF2">
   <description>pin 94</description>
   <views>
    <breadboardView>
     <p svgId="connector93pin" layer="breadboard" terminalId="connector93terminal"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector93pin" layer="schematic" terminalId="connector93terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector93pin" layer="copper0"/>
     <p svgId="connector93pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector type="female" id="connector94" name="RF8">
   <description>pin 95</description>
   <views>
    <breadboardView>
     <p svgId="connector94pin" layer="breadboard" terminalId="connector94terminal"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector94pin" layer="schematic" terminalId="connector94terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector94pin" layer="copper0"/>
     <p svgId="connector94pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector type="female" id="connector95" name="RD14">
   <description>pin 96</description>
   <views>
    <breadboardView>
     <p svgId="connector95pin" layer="breadboard" terminalId="connector95terminal"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector95pin" layer="schematic" terminalId="connector95terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector95pin" layer="copper0"/>
     <p svgId="connector95pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector type="female" id="connector96" name="VDD">
   <description>pin 97</description>
   <views>
    <breadboardView>
     <p svgId="connector96pin" layer="breadboard" terminalId="connector96terminal"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector96pin" layer="schematic" terminalId="connector96terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector96pin" layer="copper0"/>
     <p svgId="connector96pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector type="female" id="connector97" name="GND">
   <description>pin 98</description>
   <views>
    <breadboardView>
     <p svgId="connector97pin" layer="breadboard" terminalId="connector97terminal"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector97pin" layer="schematic" terminalId="connector97terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector97pin" layer="copper0"/>
     <p svgId="connector97pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector type="female" id="connector98" name="RA5">
   <description>pin 99</description>
   <views>
    <breadboardView>
     <p svgId="connector98pin" layer="breadboard" terminalId="connector98terminal"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector98pin" layer="schematic" terminalId="connector98terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector98pin" layer="copper0"/>
     <p svgId="connector98pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector type="female" id="connector99" name="RA4">
   <description>pin 100</description>
   <views>
    <breadboardView>
     <p svgId="connector99pin" layer="breadboard" terminalId="connector99terminal"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector99pin" layer="schematic" terminalId="connector99terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector99pin" layer="copper0"/>
     <p svgId="connector99pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector type="female" id="connector100" name="RA1">
   <description>pin 101</description>
   <views>
    <breadboardView>
     <p svgId="connector100pin" layer="breadboard" terminalId="connector100terminal"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector100pin" layer="schematic" terminalId="connector100terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector100pin" layer="copper0"/>
     <p svgId="connector100pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector type="female" id="connector101" name="RA0">
   <description>pin 102</description>
   <views>
    <breadboardView>
     <p svgId="connector101pin" layer="breadboard" terminalId="connector101terminal"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector101pin" layer="schematic" terminalId="connector101terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector101pin" layer="copper0"/>
     <p svgId="connector101pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector type="female" id="connector102" name="VDD">
   <description>pin 103</description>
   <views>
    <breadboardView>
     <p svgId="connector102pin" layer="breadboard" terminalId="connector102terminal"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector102pin" layer="schematic" terminalId="connector102terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector102pin" layer="copper0"/>
     <p svgId="connector102pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector type="female" id="connector103" name="GND">
   <description>pin 104</description>
   <views>
    <breadboardView>
     <p svgId="connector103pin" layer="breadboard" terminalId="connector103terminal"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector103pin" layer="schematic" terminalId="connector103terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector103pin" layer="copper0"/>
     <p svgId="connector103pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector type="female" id="connector104" name="RA7">
   <description>pin 105</description>
   <views>
    <breadboardView>
     <p svgId="connector104pin" layer="breadboard" terminalId="connector104terminal"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector104pin" layer="schematic" terminalId="connector104terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector104pin" layer="copper0"/>
     <p svgId="connector104pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector type="female" id="connector105" name="RA6">
   <description>pin 106</description>
   <views>
    <breadboardView>
     <p svgId="connector105pin" layer="breadboard" terminalId="connector105terminal"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector105pin" layer="schematic" terminalId="connector105terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector105pin" layer="copper0"/>
     <p svgId="connector105pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector type="female" id="connector106" name="RA15">
   <description>pin 107</description>
   <views>
    <breadboardView>
     <p svgId="connector106pin" layer="breadboard" terminalId="connector106terminal"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector106pin" layer="schematic" terminalId="connector106terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector106pin" layer="copper0"/>
     <p svgId="connector106pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector type="female" id="connector107" name="RA14">
   <description>pin 108</description>
   <views>
    <breadboardView>
     <p svgId="connector107pin" layer="breadboard" terminalId="connector107terminal"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector107pin" layer="schematic" terminalId="connector107terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector107pin" layer="copper0"/>
     <p svgId="connector107pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
 </connectors>
 <url>http://digilentinc.com/Products/Detail.cfm?NavPath=2,892,1218&amp;Prod=CHIPKIT-PRO-MX4</url>
</module>
