<?xml version="1.0" encoding="UTF-8"?><module moduleId="generic_sip_2_300mil">
 <version>4</version>
 <author>Fritzing Part-o-matic</author>
 <title>SIP - 2 pins</title>
 <label>U</label>
 <date>2009-10-20</date>
 <tags>
  <tag>SIP</tag>
  <tag>fritzing core</tag>
 </tags>
 <properties>
  <property name="family">Generic IC</property>
  <property name="package">SIP (Single Inline) [THT]</property>
  <property name="pins">2</property>
  <property name="spacing">300mil</property>
  <property name="chip label">IC</property>
    <property name="hole size"></property>

<property name='editable pin labels'>true</property>
</properties>
 <taxonomy>part.sip.2pins</taxonomy>
 <description>A SIP stand-in part for whatever you want.  With 2 pins on a 300 mil single inline package (SIP) footprint.</description>
 <views>
  <iconView>
   <layers image="icon/dip_icon.svg">
    <layer layerId="icon"/>
   </layers>
  </iconView>
  <breadboardView>
   <layers image="breadboard/generic_sip_2_300mil_bread.svg">
    <layer layerId="breadboard"/>
   </layers>
  </breadboardView>
  <schematicView>
   <layers image="schematic/generic_sip_2_300mil_schem.svg">
    <layer layerId="schematic"/>
   </layers>
  </schematicView>
  <pcbView>
   <layers image="pcb/jumper_2_100mil_pcb.svg">
    <layer layerId="silkscreen"/>
    <layer layerId="copper0"/>
   <layer layerId="copper1"/></layers>
  </pcbView>
 </views>
 <connectors>
  <connector id="connector0" name="pin1" type="male">
   <description>pin 1</description>
   <views>
    <breadboardView>
     <p layer="breadboard" svgId="connector0pin" terminalId="connector0terminal"/>
    </breadboardView>
    <schematicView>
     <p layer="schematic" svgId="connector0pin" terminalId="connector0terminal"/>
    </schematicView>
    <pcbView>
     <p layer="copper0" svgId="connector0pin"/>
    <p layer="copper1" svgId="connector0pin"/></pcbView>
   </views>
  </connector>
  <connector id="connector1" name="pin2" type="male">
   <description>pin 2</description>
   <views>
    <breadboardView>
     <p layer="breadboard" svgId="connector1pin" terminalId="connector1terminal"/>
    </breadboardView>
    <schematicView>
     <p layer="schematic" svgId="connector1pin" terminalId="connector1terminal"/>
    </schematicView>
    <pcbView>
     <p layer="copper0" svgId="connector1pin"/>
    <p layer="copper1" svgId="connector1pin"/></pcbView>
   </views>
  </connector>
 </connectors>
</module>