<?xml version="1.0" encoding="UTF-8"?><module fritzingVersion="0.7.2b" moduleId="SparkFun-Connectors-DB9-MALE">
<!-- generated from Sparkfun Eagle Library 'SparkFun-Connectors' DB9 MALE -->
<version>4</version>
<date>2013-02-13</date>
<label>X</label>
<author>www.fritzing.org</author>
<description>&lt;b&gt;DB9 Connector&lt;/b&gt;
Standard DB9 (D-Sub 9) serial connector. Can be used for CAN bus as well as RS485 and RS232. Footprint production proven. Spark Fun Electronics SKU : PRT-00429</description>
<title>DB9 Connector</title>
<tags>
<tag>DB9</tag>
<tag>DB9_MALE</tag>
<tag>MALE</tag>
</tags>
<properties>
<property name="package">db9</property>
<property name="family">sparkfun DB Connector</property>
<property name="gender">male</property>
</properties>
<views>
<breadboardView>
<layers image="breadboard/sparkfun-connectors_db9_male_breadboard.svg">
<layer layerId="breadboard"/>
</layers>
</breadboardView>
<schematicView>
<layers image="schematic/sparkfun-connectors_f09g_schematic.svg">
<layer layerId="schematic"/>
</layers>
</schematicView>
<pcbView>
<layers image="pcb/sparkfun-connectors_db9_male_pcb.svg">
<layer layerId="copper1"/>
<layer layerId="silkscreen"/>
<layer layerId="copper0"/>
</layers>
</pcbView>
<iconView>
<layers image="icon/DB9_MALE.svg">
<layer layerId="icon"/>
</layers>
</iconView>
</views>
<connectors>
<connector id="connector1" name="1" type="male">
<description>1</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector1pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector0pin" terminalId="connector0terminal"/>
</schematicView>
<pcbView>
<p layer="copper0" svgId="connector1pad"/>
<p layer="copper1" svgId="connector1pad"/>
</pcbView>
</views>
</connector>
<connector id="connector3" name="2" type="male">
<description>2</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector3pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector3pin" terminalId="connector3terminal"/>
</schematicView>
<pcbView>
<p layer="copper0" svgId="connector3pad"/>
<p layer="copper1" svgId="connector3pad"/>
</pcbView>
</views>
</connector>
<connector id="connector4" name="3" type="male">
<description>3</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector4pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector4pin" terminalId="connector4terminal"/>
</schematicView>
<pcbView>
<p layer="copper0" svgId="connector4pad"/>
<p layer="copper1" svgId="connector4pad"/>
</pcbView>
</views>
</connector>
<connector id="connector5" name="4" type="male">
<description>4</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector5pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector5pin" terminalId="connector5terminal"/>
</schematicView>
<pcbView>
<p layer="copper0" svgId="connector5pad"/>
<p layer="copper1" svgId="connector5pad"/>
</pcbView>
</views>
</connector>
<connector id="connector6" name="5" type="male">
<description>5</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector6pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector6pin" terminalId="connector6terminal"/>
</schematicView>
<pcbView>
<p layer="copper0" svgId="connector6pad"/>
<p layer="copper1" svgId="connector6pad"/>
</pcbView>
</views>
</connector>
<connector id="connector7" name="6" type="male">
<description>6</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector7pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector7pin" terminalId="connector7terminal"/>
</schematicView>
<pcbView>
<p layer="copper0" svgId="connector7pad"/>
<p layer="copper1" svgId="connector7pad"/>
</pcbView>
</views>
</connector>
<connector id="connector8" name="7" type="male">
<description>7</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector8pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector8pin" terminalId="connector8terminal"/>
</schematicView>
<pcbView>
<p layer="copper0" svgId="connector8pad"/>
<p layer="copper1" svgId="connector8pad"/>
</pcbView>
</views>
</connector>
<connector id="connector9" name="8" type="male">
<description>8</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector9pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector9pin" terminalId="connector9terminal"/>
</schematicView>
<pcbView>
<p layer="copper0" svgId="connector9pad"/>
<p layer="copper1" svgId="connector9pad"/>
</pcbView>
</views>
</connector>
<connector id="connector10" name="9" type="male">
<description>9</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector10pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector10pin" terminalId="connector10terminal"/>
</schematicView>
<pcbView>
<p layer="copper0" svgId="connector10pad"/>
<p layer="copper1" svgId="connector10pad"/>
</pcbView>
</views>
</connector>
</connectors>
<buses>
</buses>
</module>