<?xml version="1.0" encoding="UTF-8"?><module fritzingVersion="0.3.15b.02.03.3943" moduleId="cee49c7a6b94e1759bb995959b72f50cPotentiometerModuleID">
    <version replacedby="e55c4e524988a0331c383c6d9b004770_8">4</version>
    <author>Lionel Michel</author>
    <title>Rotary Potentiometer (Small)</title>
    <label>R</label>
    <date>2010-02-10</date>
    <tags>
        <tag>potentiometer</tag>
        <tag>poti</tag>
        <tag>adjustable</tag>
        <tag>resistor</tag>
				<tag>fritzing core</tag>
    </tags>
    <properties>
        <property name="family">/obsolete/Potentiometer</property>
        <property name="track">Linear</property>
        <property name="type">Rotary Shaft Potentiometer</property>
        <property name="size">Rotary - 9mm</property>
	<property name="power" showInLabel="yes"></property>
        <property name="Maximum Resistance" showInLabel="yes">100k&#937;</property>
    </properties>
    <description>A rotary adjustable resistor (potentiometer).</description>
    <views>
        <iconView>
            <layers image="icon/pot-small.svg">
                <layer layerId="icon"/>
            </layers>
        </iconView>
        <schematicView>
            <layers image="schematic/basic_poti.svg">
                <layer layerId="schematic"/>
            </layers>
        </schematicView>
        <pcbView>
            <layers image="pcb/jumper_3_100mil_pcb.svg">
                <layer layerId="copper0"/>
                <layer layerId="silkscreen"/>
                <layer layerId="keepout"/>
                <layer layerId="soldermask"/>
                <layer layerId="outline"/>
            <layer layerId="copper1"/></layers>
        </pcbView>
        <breadboardView>
            <layers image="breadboard/pot-small.svg">
                <layer layerId="breadboard"/>
            </layers>
        </breadboardView>
    </views>
    <connectors>
        <connector id="connector0" name="leg1" type="male">
            <description>leg1</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector0pin"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector0pin" terminalId="connector0terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper0" svgId="connector0pin"/>
                <p layer="copper1" svgId="connector0pin"/></pcbView>
            </views>
        </connector>
        <connector id="connector1" name="wiper" type="male">
            <description>wiper</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector1pin"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector1pin" terminalId="connector1terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper0" svgId="connector1pin"/>
                <p layer="copper1" svgId="connector1pin"/></pcbView>
            </views>
        </connector>
        <connector id="connector2" name="leg2" type="male">
            <description>leg2</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector2pin"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector2pin" terminalId="connector2terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper0" svgId="connector2pin"/>
                <p layer="copper1" svgId="connector2pin"/></pcbView>
            </views>
        </connector>
    </connectors>
</module>