<?xml version='1.0' encoding='UTF-8'?>
<module fritzingVersion='0.5.2b.02.18.4756' moduleId='canbus_shield-v12'>
<version>4</version>
<date>2011-07-08</date>
<author>SparkFun</author>
<description>&lt;div&gt;


	&lt;strong&gt;Description:&lt;/strong&gt; This shield gives the Arduino CAN-Bus capability. It uses the Microchip MCP2515 CAN controller with MCP2551 CAN transceiver. CAN connection is via a standard 9-way sub-D for use with&amp;nbsp;OBDII cable. Ideal for automative CAN application. The shield also has a uSD card holder, serial LCD connector and connector for an&amp;nbsp;EM406 GPS module. Making this shield ideal for data logging application.&lt;/div&gt;


&lt;div&gt;


	&lt;strong&gt;Features&lt;/strong&gt;&lt;/div&gt;


&lt;div&gt;


	&lt;ul&gt;


		&lt;li&gt;


			CAN v2.0B upto 1 Mb/s&lt;/li&gt;


		&lt;li&gt;


			High speed SPI Interface (10 MHz)&lt;/li&gt;


		&lt;li&gt;


			Standard and extened data and remote frames&lt;/li&gt;


		&lt;li&gt;


			CAN connection via standard 9-way sub-D connector&lt;/li&gt;


		&lt;li&gt;


			9-way sub-D standard&amp;nbsp;OBDII connection cable&lt;/li&gt;


		&lt;li&gt;


			Power can supply to Arduino by sub-D via resettable fuse and reverse polarity protection.&lt;/li&gt;


		&lt;li&gt;


			Socket for&amp;nbsp;EM406 GPS module&lt;/li&gt;


		&lt;li&gt;


			Micro SD card holder&lt;/li&gt;


		&lt;li&gt;


			Connector for&amp;nbsp;serial LCD&lt;/li&gt;


		&lt;li&gt;


			Reset button&lt;/li&gt;


		&lt;li&gt;


			Joystick control menu navigation control&lt;/li&gt;


		&lt;li&gt;


			Two LED indicator&lt;/li&gt;


	&lt;/ul&gt;


	&lt;p&gt;


		&lt;strong&gt;Documents:&lt;/strong&gt;&lt;/p&gt;


	&lt;ul&gt;


		&lt;li&gt;


			&lt;a href=&quot;http://www.sparkfun.com/datasheets/DevTools/Arduino/canbus_shield-v12.pdf&quot; target=&quot;_blank&quot;&gt;Schematic&lt;/a&gt;&lt;/li&gt;


		&lt;li&gt;


			&lt;a href=&quot;http://www.sparkfun.com/datasheets/DevTools/Arduino/canbus_shield-v12.zip&quot; target=&quot;_blank&quot;&gt;Eagle Files&lt;/a&gt;&lt;/li&gt;


		&lt;li&gt;


			&lt;a href=&quot;http://www.sparkfun.com/datasheets/DevTools/Arduino/MCP2515.pdf&quot; target=&quot;_blank&quot;&gt;Datasheet &lt;/a&gt;(MCP2515)&lt;/li&gt;


		&lt;li&gt;


			&lt;a href=&quot;http://www.sparkfun.com/datasheets/DevTools/Arduino/MCP2551.pdf&quot; target=&quot;_blank&quot;&gt;Datasheet &lt;/a&gt;(MCP2551)&lt;/li&gt;


	&lt;/ul&gt;


&lt;/div&gt;</description>
<title>Arduino Can-Bus Shield</title>
<url>http://www.sparkfun.com/products/10039</url>
<tags>
<tag>Can</tag>
<tag>Bus</tag>
<tag>Automobile</tag>
<tag>OBD</tag>
</tags>
<properties>
<property name='family'>CAN Shield</property>
</properties>
<views>
<breadboardView>
<layers image='breadboard/canbus_shield-v12_breadboard.svg'>
<layer layerId='breadboard'/>
</layers>
</breadboardView>
<schematicView>
<layers image='schematic/canbus_shield-v12_schematic.svg'>
<layer layerId='schematic'/>
</layers>
</schematicView>
<pcbView>
<layers image='pcb/canbus_shield-v12_pcb.svg'>
<layer layerId='copper1'/>
<layer layerId='silkscreen'/>
<layer layerId='copper0'/>
</layers>
</pcbView>
<iconView>
<layers image='breadboard/canbus_shield-v12_breadboard.svg'>
<layer layerId='icon'/>
</layers>
</iconView>
</views>
<connectors>
<connector id='connector22' type='male' name='VCC'>
<description>VCC</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector22pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector22pin' terminalId='connector22terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector22pad'/><p layer='copper1' svgId='connector22pad'/></pcbView>
</views>
</connector>
<connector id='connector23' type='male' name='GND'>
<description>GND</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector23pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector23pin' terminalId='connector23terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector23pad'/><p layer='copper1' svgId='connector23pad'/></pcbView>
</views>
</connector>
<connector id='connector24' type='male' name='LCD'>
<description>LCD</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector24pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector24pin' terminalId='connector24terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector24pad'/><p layer='copper1' svgId='connector24pad'/></pcbView>
</views>
</connector>
<connector id='connector27' type='female' name='VCC'>
<description>VCC</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector27pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector27pin' terminalId='connector27terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector27pad'/><p layer='copper1' svgId='connector27pad'/></pcbView>
</views>
</connector>
<connector id='connector28' type='female' name='GND'>
<description>GND</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector28pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector28pin' terminalId='connector28terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector28pad'/><p layer='copper1' svgId='connector28pad'/></pcbView>
</views>
</connector>
<connector id='connector29' type='female' name='CANH'>
<description>CANH</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector29pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector29pin' terminalId='connector29terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector29pad'/><p layer='copper1' svgId='connector29pad'/></pcbView>
</views>
</connector>
<connector id='connector30' type='female' name='CANL'>
<description>CANL</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector30pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector30pin' terminalId='connector30terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector30pad'/><p layer='copper1' svgId='connector30pad'/></pcbView>
</views>
</connector>
<connector id='connector75' type='female' name='3.3V'>
<description>3.3V</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector75pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector75pin' terminalId='connector75terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector75pad'/><p layer='copper1' svgId='connector75pad'/></pcbView>
</views>
</connector>
<connector id='connector76' type='female' name='VCC'>
<description>VCC</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector76pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector76pin' terminalId='connector76terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector76pad'/><p layer='copper1' svgId='connector76pad'/></pcbView>
</views>
</connector>
<connector id='connector77' type='female' name='A0'>
<description>A0</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector77pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector77pin' terminalId='connector77terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector77pad'/><p layer='copper1' svgId='connector77pad'/></pcbView>
</views>
</connector>
<connector id='connector78' type='female' name='JOY-UP'>
<description>JOY-UP</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector78pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector78pin' terminalId='connector78terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector78pad'/><p layer='copper1' svgId='connector78pad'/></pcbView>
</views>
</connector>
<connector id='connector79' type='female' name='JOY-LEFT'>
<description>JOY-LEFT</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector79pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector79pin' terminalId='connector79terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector79pad'/><p layer='copper1' svgId='connector79pad'/></pcbView>
</views>
</connector>
<connector id='connector80' type='female' name='JOY-DOWN'>
<description>JOY-DOWN</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector80pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector80pin' terminalId='connector80terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector80pad'/><p layer='copper1' svgId='connector80pad'/></pcbView>
</views>
</connector>
<connector id='connector81' type='female' name='JOY-CLICK'>
<description>JOY-CLICK</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector81pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector81pin' terminalId='connector81terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector81pad'/><p layer='copper1' svgId='connector81pad'/></pcbView>
</views>
</connector>
<connector id='connector82' type='female' name='JOY-RIGHT'>
<description>JOY-RIGHT</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector82pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector82pin' terminalId='connector82terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector82pad'/><p layer='copper1' svgId='connector82pad'/></pcbView>
</views>
</connector>
<connector id='connector83' type='female' name='AREF'>
<description>AREF</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector83pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector83pin' terminalId='connector83terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector83pad'/><p layer='copper1' svgId='connector83pad'/></pcbView>
</views>
</connector>
<connector id='connector84' type='female' name='CAN_INT'>
<description>CAN_INT</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector84pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector84pin' terminalId='connector84terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector84pad'/><p layer='copper1' svgId='connector84pad'/></pcbView>
</views>
</connector>
<connector id='connector85' type='female' name='D3'>
<description>D3</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector85pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector85pin' terminalId='connector85terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector85pad'/><p layer='copper1' svgId='connector85pad'/></pcbView>
</views>
</connector>
<connector id='connector86' type='female' name='D4'>
<description>D4</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector86pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector86pin' terminalId='connector86terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector86pad'/><p layer='copper1' svgId='connector86pad'/></pcbView>
</views>
</connector>
<connector id='connector87' type='female' name='D5'>
<description>D5</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector87pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector87pin' terminalId='connector87terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector87pad'/><p layer='copper1' svgId='connector87pad'/></pcbView>
</views>
</connector>
<connector id='connector88' type='female' name='LCD'>
<description>LCD</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector88pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector88pin' terminalId='connector88terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector88pad'/><p layer='copper1' svgId='connector88pad'/></pcbView>
</views>
</connector>
<connector id='connector89' type='female' name='LED2'>
<description>LED2</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector89pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector89pin' terminalId='connector89terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector89pad'/><p layer='copper1' svgId='connector89pad'/></pcbView>
</views>
</connector>
<connector id='connector90' type='female' name='LED1'>
<description>LED1</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector90pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector90pin' terminalId='connector90terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector90pad'/><p layer='copper1' svgId='connector90pad'/></pcbView>
</views>
</connector>
<connector id='connector91' type='female' name='SD_CS'>
<description>SD_CS</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector91pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector91pin' terminalId='connector91terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector91pad'/><p layer='copper1' svgId='connector91pad'/></pcbView>
</views>
</connector>
<connector id='connector92' type='female' name='CAN_CS'>
<description>CAN_CS</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector92pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector92pin' terminalId='connector92terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector92pad'/><p layer='copper1' svgId='connector92pad'/></pcbView>
</views>
</connector>
<connector id='connector93' type='female' name='MOSI'>
<description>MOSI</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector93pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector93pin' terminalId='connector93terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector93pad'/><p layer='copper1' svgId='connector93pad'/></pcbView>
</views>
</connector>
<connector id='connector94' type='female' name='MISO'>
<description>MISO</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector94pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector94pin' terminalId='connector94terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector94pad'/><p layer='copper1' svgId='connector94pad'/></pcbView>
</views>
</connector>
<connector id='connector95' type='female' name='SCK'>
<description>SCK</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector95pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector95pin' terminalId='connector95terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector95pad'/><p layer='copper1' svgId='connector95pad'/></pcbView>
</views>
</connector>
<connector id='connector96' type='female' name='GND'>
<description>GND</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector96pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector96pin' terminalId='connector96terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector96pad'/><p layer='copper1' svgId='connector96pad'/></pcbView>
</views>
</connector>
<connector id='connector97' type='female' name='GND'>
<description>GND</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector97pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector97pin' terminalId='connector97terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector97pad'/><p layer='copper1' svgId='connector97pad'/></pcbView>
</views>
</connector>
<connector id='connector98' type='female' name='GND'>
<description>GND</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector98pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector98pin' terminalId='connector98terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector98pad'/><p layer='copper1' svgId='connector98pad'/></pcbView>
</views>
</connector>
<connector id='connector99' type='female' name='RS'>
<description>RS</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector99pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector99pin' terminalId='connector99terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector99pad'/><p layer='copper1' svgId='connector99pad'/></pcbView>
</views>
</connector>
<connector id='connector100' type='female' name='RX'>
<description>RX</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector100pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector100pin' terminalId='connector100terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector100pad'/><p layer='copper1' svgId='connector100pad'/></pcbView>
</views>
</connector>
<connector id='connector101' type='female' name='TX'>
<description>TX</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector101pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector101pin' terminalId='connector101terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector101pad'/><p layer='copper1' svgId='connector101pad'/></pcbView>
</views>
</connector>
<connector id='connector102' type='female' name='+12V'>
<description>+12V</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector102pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector102pin' terminalId='connector102terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector102pad'/><p layer='copper1' svgId='connector102pad'/></pcbView>
</views>
</connector>
</connectors>
<buses>
<bus id='vcc'>
<nodeMember connectorId='connector22'/>
<nodeMember connectorId='connector27'/>
<nodeMember connectorId='connector76'/>
</bus>
<bus id='gnd'>
<nodeMember connectorId='connector23'/>
<nodeMember connectorId='connector28'/>
<nodeMember connectorId='connector96'/>
<nodeMember connectorId='connector97'/>
<nodeMember connectorId='connector98'/>
</bus>
<bus id='lcd'>
<nodeMember connectorId='connector24'/>
<nodeMember connectorId='connector88'/>
</bus>
</buses>
</module>
