<?xml version='1.0' encoding='UTF-8'?>
<module fritzingVersion='0.5.2b.02.18.4756' moduleId='Arduino-Pro-Mini-v11'>
<version replacedby='Arduino-Pro-Mini-v13'>4</version>
<date>2011-07-08</date>
<author>SparkFun</author>
<description>&lt;p&gt;


	&lt;span style=&quot;font-weight: bold;&quot;&gt;Description:&lt;/span&gt; It&amp;#39;s blue! It&amp;#39;s thin (0.8mm)! It&amp;#39;s the Arduino Pro Mini! SparkFun&amp;#39;s minimal design approach to Arduino. This is a 3.3V Arduino running the 8MHz bootloader (select &amp;#39;Arduino Duemilanove w/ 328&amp;#39; within the Arduino software). Arduino Pro Mini does not come with connectors populated so that you can solder in any connector or wire with any orientation you need. We recommend first time Arduino users start with the Duemilanove. It&amp;#39;s a great board that will get you up and running quickly. The Arduino Pro series is meant for users that understand the limitations of system voltage (3.3V), lack of connectors, and USB off board.&lt;/p&gt;


&lt;p&gt;


	We really wanted to minimize the cost of an Arduino. The Arduino Pro Mini is like the Arduino Mini (same pin out) but to keep the cost low, we used all SMD components, made it two layer, etc. This board connects directly to the FTDI Basic Breakout board and supports auto-reset. The Arduino Pro Mini also works with the FTDI cable but the FTDI cable does not bring out the DTR pin so the auto-reset feature will not work.&lt;/p&gt;


&lt;p&gt;


	Can&amp;#39;t decide which Arduino is right for you? &lt;a classname=&quot;&quot; href=&quot;http://www.sparkfun.com/commerce/tutorial_info.php?tutorials_id=148&quot; name=&quot;&quot; target=&quot;&quot;&gt;Arduino buying guide&lt;/a&gt;!&lt;/p&gt;


&lt;p&gt;


	&lt;span style=&quot;font-weight: bold;&quot;&gt;Features:&lt;/span&gt;&lt;/p&gt;


&lt;ul&gt;


	&lt;li&gt;


		ATmega328 running at 8MHz with external resonator (0.5% tolerance)&lt;/li&gt;


	&lt;li&gt;


		Low-voltage board needs no interfacing circuitry to popular 3.3V devices and modules (GPS, accelerometers, sensors, etc)&lt;/li&gt;


	&lt;li&gt;


		USB connection off board&lt;/li&gt;


	&lt;li&gt;


		Supports auto-reset&lt;/li&gt;


	&lt;li&gt;


		3.3V regulator&lt;/li&gt;


	&lt;li&gt;


		Max 150mA output&lt;/li&gt;


	&lt;li&gt;


		Over current protected&lt;/li&gt;


	&lt;li&gt;


		Reverse polarity protected&lt;/li&gt;


	&lt;li&gt;


		DC input 3.3V up to 12V&lt;/li&gt;


	&lt;li&gt;


		On board Power and Status LEDs&lt;/li&gt;


&lt;/ul&gt;


&lt;p&gt;


	&lt;span style=&quot;font-weight: bold;&quot;&gt;Dimensions:&lt;/span&gt;&lt;/p&gt;


&lt;ul&gt;


	&lt;li&gt;


		0.7x1.3&amp;quot; (18x33mm)&lt;/li&gt;


	&lt;li&gt;


		Less than 2 grams&lt;/li&gt;


&lt;/ul&gt;


&lt;p&gt;


	&lt;span style=&quot;font-weight: bold;&quot;&gt;Documents: &lt;/span&gt;&lt;/p&gt;


&lt;ul&gt;


	&lt;li&gt;


		&lt;a classname=&quot;&quot; href=&quot;http://dlnmh9ip6v2uc.cloudfront.net/datasheets/Dev/Arduino/Boards/Arduino-Pro-Mini-v12.pdf&quot; target=&quot;_blank&quot;&gt;Schematic&lt;/a&gt;&lt;/li&gt;


	&lt;li&gt;


		&lt;a classname=&quot;&quot; href=&quot;http://dlnmh9ip6v2uc.cloudfront.net/datasheets/Dev/Arduino/Boards/Arduino-Pro-Mini-v12.zip&quot; target=&quot;_blank&quot;&gt;Eagle Files&lt;/a&gt;&lt;/li&gt;


	&lt;li&gt;


		&lt;a classname=&quot;&quot; href=&quot;http://www.arduino.cc/en/Main/ArduinoBoardProMini&quot; name=&quot;&quot; target=&quot;_blank&quot;&gt;Arduino Pro Mini Homepage&lt;/a&gt;&lt;/li&gt;


	&lt;li&gt;


		&lt;a classname=&quot;&quot; href=&quot;http://www.arduino.cc/en/Guide/ArduinoProMini&quot; name=&quot;&quot; target=&quot;_blank&quot;&gt;Getting Started Tutorial&lt;/a&gt;&lt;/li&gt;


&lt;/ul&gt;</description>
<title>Arduino Pro Mini 3.3V</title>
<url>http://www.sparkfun.com/products/9220</url>
<tags>
<tag>Arduino</tag>
<tag>Pro</tag>
</tags>
<properties>
<property name="family">/obsolete/Microcontroller Board (Arduino)</property>
<property name='Voltage'>3.3V</property>
<property name='Digital Pins'>14</property>
<property name='Analog Pins'>4</property>
</properties>
<views>
<breadboardView>
<layers image='breadboard/Arduino-Pro-Mini-v11_breadboard.svg'>
<layer layerId='breadboard'/>
</layers>
</breadboardView>
<schematicView>
<layers image='schematic/Arduino-Pro-Mini-v11_schematic.svg'>
<layer layerId='schematic'/>
</layers>
</schematicView>
<pcbView>
<layers image='pcb/Arduino-Pro-Mini-v11_pcb.svg'>
<layer layerId='copper1'/>
<layer layerId='silkscreen'/>
<layer layerId='copper0'/>
</layers>
</pcbView>
<iconView>
<layers image='breadboard/Arduino-Pro-Mini-v11_breadboard.svg'>
<layer layerId='icon'/>
</layers>
</iconView>
</views>
<connectors>
<connector id='connector14' type='male' name='DTR' replacedby='DTR'>
<description>DTR</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector14pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector14pin' terminalId='connector14terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector14pad'/><p layer='copper1' svgId='connector14pad'/></pcbView>
</views>
<erc ignore='ifUnconnected'/></connector>
<connector id='connector15' type='male' name='TXO' replacedby='D0/TX'>
<description>TXO</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector15pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector15pin' terminalId='connector15terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector15pad'/><p layer='copper1' svgId='connector15pad'/></pcbView>
</views>
<erc ignore='ifUnconnected'/></connector>
<connector id='connector16' type='male' name='RXI' replacedby='D1/RX'>
<description>RXI</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector16pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector16pin' terminalId='connector16terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector16pad'/><p layer='copper1' svgId='connector16pad'/></pcbView>
</views>
<erc ignore='ifUnconnected'/></connector>
<connector id='connector17' type='male' name='VCC' replacedby='VCC'>
<description>VCC</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector17pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector17pin' terminalId='connector17terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector17pad'/><p layer='copper1' svgId='connector17pad'/></pcbView>
</views>
<erc ignore='ifUnconnected'/></connector>
<connector id='connector18' type='male' name='GND' replacedby='GND'>
<description>GND</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector18pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector18pin' terminalId='connector18terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector18pad'/><p layer='copper1' svgId='connector18pad'/></pcbView>
</views>
<erc ignore='ifUnconnected'/></connector>
<connector id='connector19' type='male' name='GND' replacedby='GND'>
<description>GND</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector19pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector19pin' terminalId='connector19terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector19pad'/><p layer='copper1' svgId='connector19pad'/></pcbView>
</views>
<erc ignore='ifUnconnected'/></connector>
<connector id='connector20' type='male' name='A4' replacedby='A4'>
<description>A4</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector20pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector20pin' terminalId='connector20terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector20pad'/><p layer='copper1' svgId='connector20pad'/></pcbView>
</views>
<erc ignore='ifUnconnected'/></connector>
<connector id='connector21' type='male' name='A5' replacedby='A5'>
<description>A5</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector21pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector21pin' terminalId='connector21terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector21pad'/><p layer='copper1' svgId='connector21pad'/></pcbView>
</views>
<erc ignore='ifUnconnected'/></connector>
<connector id='connector22' type='male' name='RAW' replacedby='RAW'>
<description>RAW</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector22pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector22pin' terminalId='connector22terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector22pad'/><p layer='copper1' svgId='connector22pad'/></pcbView>
</views>
<erc ignore='ifUnconnected'/></connector>
<connector id='connector23' type='male' name='GND' replacedby='GND'>
<description>GND</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector23pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector23pin' terminalId='connector23terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector23pad'/><p layer='copper1' svgId='connector23pad'/></pcbView>
</views>
<erc ignore='ifUnconnected'/></connector>
<connector id='connector24' type='male' name='RESET' replacedby='RESET'>
<description>RESET</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector24pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector24pin' terminalId='connector24terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector24pad'/><p layer='copper1' svgId='connector24pad'/></pcbView>
</views>
<erc ignore='ifUnconnected'/></connector>
<connector id='connector25' type='male' name='VCC' replacedby='VCC'>
<description>VCC</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector25pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector25pin' terminalId='connector25terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector25pad'/><p layer='copper1' svgId='connector25pad'/></pcbView>
</views>
<erc ignore='ifUnconnected'/></connector>
<connector id='connector26' type='male' name='A3' replacedby='A3'>
<description>A3</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector26pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector26pin' terminalId='connector26terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector26pad'/><p layer='copper1' svgId='connector26pad'/></pcbView>
</views>
<erc ignore='ifUnconnected'/></connector>
<connector id='connector27' type='male' name='A2' replacedby='A2'>
<description>A2</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector27pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector27pin' terminalId='connector27terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector27pad'/><p layer='copper1' svgId='connector27pad'/></pcbView>
</views>
<erc ignore='ifUnconnected'/></connector>
<connector id='connector28' type='male' name='A1' replacedby='A1'>
<description>A1</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector28pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector28pin' terminalId='connector28terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector28pad'/><p layer='copper1' svgId='connector28pad'/></pcbView>
</views>
<erc ignore='ifUnconnected'/></connector>
<connector id='connector29' type='male' name='A0' replacedby='A0'>
<description>A0</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector29pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector29pin' terminalId='connector29terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector29pad'/><p layer='copper1' svgId='connector29pad'/></pcbView>
</views>
<erc ignore='ifUnconnected'/></connector>
<connector id='connector30' type='male' name='SCK' replacedby='D13/SCK'>
<description>SCK</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector30pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector30pin' terminalId='connector30terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector30pad'/><p layer='copper1' svgId='connector30pad'/></pcbView>
</views>
<erc ignore='ifUnconnected'/></connector>
<connector id='connector31' type='male' name='MISO' replacedby='D12/MISO'>
<description>MISO</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector31pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector31pin' terminalId='connector31terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector31pad'/><p layer='copper1' svgId='connector31pad'/></pcbView>
</views>
<erc ignore='ifUnconnected'/></connector>
<connector id='connector32' type='male' name='MOSI' replacedby='D11 PWM/MOSI'>
<description>MOSI</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector32pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector32pin' terminalId='connector32terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector32pad'/><p layer='copper1' svgId='connector32pad'/></pcbView>
</views>
<erc ignore='ifUnconnected'/></connector>
<connector id='connector33' type='male' name='D10' replacedby='D10 PWM/SS'>
<description>D10</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector33pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector33pin' terminalId='connector33terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector33pad'/><p layer='copper1' svgId='connector33pad'/></pcbView>
</views>
<erc ignore='ifUnconnected'/></connector>
<connector id='connector34' type='male' name='D9' replacedby='D9 PWM'>
<description>D9</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector34pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector34pin' terminalId='connector34terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector34pad'/><p layer='copper1' svgId='connector34pad'/></pcbView>
</views>
<erc ignore='ifUnconnected'/></connector>
<connector id='connector35' type='male' name='D8' replacedby='D8'>
<description>D8</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector35pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector35pin' terminalId='connector35terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector35pad'/><p layer='copper1' svgId='connector35pad'/></pcbView>
</views>
<erc ignore='ifUnconnected'/></connector>
<connector id='connector36' type='male' name='D7' replacedby='D7'>
<description>D7</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector36pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector36pin' terminalId='connector36terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector36pad'/><p layer='copper1' svgId='connector36pad'/></pcbView>
</views>
<erc ignore='ifUnconnected'/></connector>
<connector id='connector37' type='male' name='D6' replacedby='D6 PWM'>
<description>D6</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector37pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector37pin' terminalId='connector37terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector37pad'/><p layer='copper1' svgId='connector37pad'/></pcbView>
</views>
<erc ignore='ifUnconnected'/></connector>
<connector id='connector38' type='male' name='D5' replacedby='D5 PWM'>
<description>D5</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector38pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector38pin' terminalId='connector38terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector38pad'/><p layer='copper1' svgId='connector38pad'/></pcbView>
</views>
<erc ignore='ifUnconnected'/></connector>
<connector id='connector39' type='male' name='D4' replacedby='D4'>
<description>D4</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector39pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector39pin' terminalId='connector39terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector39pad'/><p layer='copper1' svgId='connector39pad'/></pcbView>
</views>
<erc ignore='ifUnconnected'/></connector>
<connector id='connector40' type='male' name='D3' replacedby='D3 PWM'>
<description>D3</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector40pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector40pin' terminalId='connector40terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector40pad'/><p layer='copper1' svgId='connector40pad'/></pcbView>
</views>
<erc ignore='ifUnconnected'/></connector>
<connector id='connector41' type='male' name='D2' replacedby='D2'>
<description>D2</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector41pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector41pin' terminalId='connector41terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector41pad'/><p layer='copper1' svgId='connector41pad'/></pcbView>
</views>
<erc ignore='ifUnconnected'/></connector>
<connector id='connector42' type='male' name='GND' replacedby='GND'>
<description>GND</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector42pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector42pin' terminalId='connector42terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector42pad'/><p layer='copper1' svgId='connector42pad'/></pcbView>
</views>
<erc ignore='ifUnconnected'/></connector>
<connector id='connector43' type='male' name='RESET' replacedby='RESET'>
<description>RESET</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector43pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector43pin' terminalId='connector43terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector43pad'/><p layer='copper1' svgId='connector43pad'/></pcbView>
</views>
<erc ignore='ifUnconnected'/></connector>
<connector id='connector44' type='male' name='RXI' replacedby='D1/RX'>
<description>RXI</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector44pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector44pin' terminalId='connector44terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector44pad'/><p layer='copper1' svgId='connector44pad'/></pcbView>
</views>
<erc ignore='ifUnconnected'/></connector>
<connector id='connector45' type='male' name='TXO' replacedby='D0/TX'>
<description>TXO</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector45pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector45pin' terminalId='connector45terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector45pad'/><p layer='copper1' svgId='connector45pad'/></pcbView>
</views>
<erc ignore='ifUnconnected'/></connector>
</connectors>
<buses>
<bus id='gnd'>
<nodeMember connectorId='connector18'/>
<nodeMember connectorId='connector19'/>
<nodeMember connectorId='connector23'/>
<nodeMember connectorId='connector42'/>
</bus>
<bus id='vcc'>
<nodeMember connectorId='connector17'/>
<nodeMember connectorId='connector25'/>
</bus>
<bus id='reset'>
<nodeMember connectorId='connector24'/>
<nodeMember connectorId='connector43'/>
</bus>
<bus id='rxi'>
<nodeMember connectorId='connector16'/>
<nodeMember connectorId='connector44'/>
</bus>
<bus id='txo'>
<nodeMember connectorId='connector15'/>
<nodeMember connectorId='connector45'/>
</bus>
</buses>
</module>
