<?xml version='1.0' encoding='UTF-8'?>
<module moduleId="Button-LED-Breakout-v10" referenceFile="Button-LED-Breakout-v10.fzp" fritzingVersion="0.5.2b.02.18.4756">
 <version>4</version>
 <date>Mon Nov 3 2014</date>
 <author>SFE and Fritzing</author>
 <description>This simple breakout board makes it easy to use our LED tactile switches in a breadboard, or your next project.</description>
 <title>LED Tactile Button Breakout v10</title>
 <url>https://www.sparkfun.com/products/10467</url>
 <tags>
  <tag>SparkFun</tag>
 </tags>
 <properties>
  <property name="layer"></property>
  <property name="family">LED Tactile Button Breakout</property>
  <property name="variant">variant 1</property>
  <property name="part number">BOB-10467</property>
 </properties>
 <views>
  <breadboardView>
   <layers image="breadboard/prefix0000_SFE-10467-v10_2.svg">
    <layer layerId="breadboard"/>
   </layers>
  </breadboardView>
  <schematicView>
   <layers image="schematic/prefix0000_SFE-10467-v10_2.svg">
    <layer layerId="schematic"/>
   </layers>
  </schematicView>
  <pcbView>
   <layers image="pcb/prefix0000_SFE-10467-v10_2.svg">
    <layer layerId="copper1"/>
    <layer layerId="silkscreen"/>
    <layer layerId="copper0"/>
   </layers>
  </pcbView>
  <iconView>
   <layers image="icon/prefix0000_SFE-10467-v10_2.svg">
    <layer layerId="icon"/>
   </layers>
  </iconView>
 </views>
 <connectors>
  <connector type="female" id="connector0" name="1">
   <description>1</description>
   <views>
    <breadboardView>
     <p svgId="connector0pin" layer="breadboard"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector0pin" layer="schematic" terminalId="connector0terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector0pad" layer="copper0"/>
     <p svgId="connector0pad" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector type="female" id="connector1" name="2">
   <description>2</description>
   <views>
    <breadboardView>
     <p svgId="connector1pin" layer="breadboard"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector1pin" layer="schematic" terminalId="connector1terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector1pad" layer="copper0"/>
     <p svgId="connector1pad" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector type="female" id="connector2" name="3">
   <description>3</description>
   <views>
    <breadboardView>
     <p svgId="connector2pin" layer="breadboard"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector2pin" layer="schematic" terminalId="connector2terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector2pad" layer="copper0"/>
     <p svgId="connector2pad" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector type="female" id="connector3" name="4">
   <description>4</description>
   <views>
    <breadboardView>
     <p svgId="connector3pin" layer="breadboard"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector3pin" layer="schematic" terminalId="connector3terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector3pad" layer="copper0"/>
     <p svgId="connector3pad" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
 </connectors>
 <buses/>
</module>
