<?xml version='1.0' encoding='UTF-8'?>
<module fritzingVersion='0.5.2b.02.18.4756' moduleId='TEMT6000_Breakout-v12'>
<version>4</version>
<date>2011-07-08</date>
<author>SparkFun</author>
<description>&lt;p&gt;


	&lt;span style=&quot;font-weight: bold;&quot;&gt;Description:&lt;/span&gt; Basic breakout board for the TEMT6000 Ambient Light Sensor. Only what you need, nothing you don&amp;#39;t. Sensor acts like a transistor - the greater the incoming light, the higher the analog voltage on the signal pin.&lt;br /&gt;


	&lt;br /&gt;


	&lt;span style=&quot;font-weight: bold;&quot;&gt;Documents:&lt;/span&gt;&lt;/p&gt;


&lt;ul&gt;


	&lt;li&gt;


		&lt;a classname=&quot;&quot; href=&quot;http://www.sparkfun.com/datasheets/Sensors/Imaging/TEMT6000.pdf&quot; name=&quot;&quot; target=&quot;_blank&quot;&gt;Datasheet&lt;/a&gt;&lt;/li&gt;


	&lt;li&gt;


		&lt;a classname=&quot;&quot; href=&quot;http://wiring.org.co/learning/basics/ambientlighttemt6000.html&quot; name=&quot;&quot; target=&quot;_blank&quot;&gt;Wiring Example&lt;/a&gt;&lt;/li&gt;


&lt;/ul&gt;</description>
<title>Ambient Light Sensor (TEMT6000 Breakout Board)</title>
<url>http://www.sparkfun.com/products/8688</url>
<tags>
<tag>Ambient</tag>
<tag>Light</tag>
<tag>TEMT6000</tag>
</tags>
<properties>
<property name='family'>Light Sensor Breakout</property>
<property name='Lilypad'>No</property>
</properties>
<views>
<breadboardView>
<layers image='breadboard/TEMT6000_Breakout-v12_breadboard.svg'>
<layer layerId='breadboard'/>
</layers>
</breadboardView>
<schematicView>
<layers image='schematic/TEMT6000_Breakout-v12_schematic.svg'>
<layer layerId='schematic'/>
</layers>
</schematicView>
<pcbView>
<layers image='pcb/TEMT6000_Breakout-v12_pcb.svg'>
<layer layerId='copper1'/>
<layer layerId='silkscreen'/>
<layer layerId='copper0'/>
</layers>
</pcbView>
<iconView>
<layers image='breadboard/TEMT6000_Breakout-v12_breadboard.svg'>
<layer layerId='icon'/>
</layers>
</iconView>
</views>
<connectors>
<connector id='connector2' type='male' name='VCC'>
<description>VCC</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector2pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector2pin' terminalId='connector2terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector2pad'/><p layer='copper1' svgId='connector2pad'/></pcbView>
</views>
</connector>
<connector id='connector3' type='male' name='GND'>
<description>GND</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector3pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector3pin' terminalId='connector3terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector3pad'/><p layer='copper1' svgId='connector3pad'/></pcbView>
</views>
</connector>
<connector id='connector4' type='male' name='S'>
<description>S</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector4pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector4pin' terminalId='connector4terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector4pad'/><p layer='copper1' svgId='connector4pad'/></pcbView>
</views>
</connector>
</connectors>
<buses>
</buses>
</module>
