<?xml version="1.0" encoding="UTF-8"?><module fritzingVersion="0.7.2b" moduleId="SparkFun-Sensors-HMC1052L-">
<!-- generated from Sparkfun Eagle Library 'SparkFun-Sensors' HMC1052L  -->
<version>4</version>
<date>2013-02-13</date>
<label>U</label>
<author>www.fritzing.org</author>
<description>&lt;b&gt;HMC1052L&lt;/b&gt;
Dual axis magnetic sensor. Used for compass and magnetometer applications. Schematic and footprint are not tested and probably need fixing. Spark Fun Electronics SKU : COM-00708</description>
<title>HMC1052L</title>
<tags>
<tag>16LPCC</tag>
<tag>HMC1052L</tag>
</tags>
<properties>
<property name="package">16lpcc</property>
<property name="family">sparkfun Magnetic Sensor</property>
<property name="axis">2</property>
</properties>
<views>
<breadboardView>
<layers image="breadboard/sparkfun-sensors_16lpcc_breadboard.svg">
<layer layerId="breadboard"/>
</layers>
</breadboardView>
<schematicView>
<layers image="schematic/sparkfun-sensors_hmc1052l_schematic.svg">
<layer layerId="schematic"/>
</layers>
</schematicView>
<pcbView>
<layers image="pcb/sparkfun-sensors_16lpcc_pcb.svg">
<layer layerId="copper1"/>
<layer layerId="silkscreen"/>
</layers>
</pcbView>
<iconView>
<layers image="breadboard/sparkfun-sensors_16lpcc_breadboard.svg">
<layer layerId="icon"/>
</layers>
</iconView>
</views>
<connectors>
<connector id="connector12" name="GND1A" type="male">
<description>GND1A</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector12pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector12pin" terminalId="connector12terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector12pad"/>
</pcbView>
</views>
</connector>
<connector id="connector14" name="GND1B" type="male">
<description>GND1B</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector14pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector14pin" terminalId="connector14terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector14pad"/>
</pcbView>
</views>
</connector>
<connector id="connector0" name="GND2A" type="male">
<description>GND2A</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector0pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector0pin" terminalId="connector0terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector0pad"/>
</pcbView>
</views>
</connector>
<connector id="connector6" name="GND2B" type="male">
<description>GND2B</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector6pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector6pin" terminalId="connector6terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector6pad"/>
</pcbView>
</views>
</connector>
<connector id="connector4" name="NC" type="male">
<description>NC</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector4pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector4pin" terminalId="connector4terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector4pad"/>
</pcbView>
</views>
</connector>
<connector id="connector8" name="NC2" type="male">
<description>NC2</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector8pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector8pin" terminalId="connector8terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector8pad"/>
</pcbView>
</views>
</connector>
<connector id="connector11" name="NC3" type="male">
<description>NC3</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector11pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector11pin" terminalId="connector11terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector11pad"/>
</pcbView>
</views>
</connector>
<connector id="connector1" name="OFF+" type="male">
<description>OFF+</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector1pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector1pin" terminalId="connector1terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector1pad"/>
</pcbView>
</views>
</connector>
<connector id="connector5" name="OFF-" type="male">
<description>OFF-</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector5pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector5pin" terminalId="connector5terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector5pad"/>
</pcbView>
</views>
</connector>
<connector id="connector2" name="OUT+A" type="male">
<description>OUT+A</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector2pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector2pin" terminalId="connector2terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector2pad"/>
</pcbView>
</views>
</connector>
<connector id="connector15" name="OUT+B" type="male">
<description>OUT+B</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector15pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector15pin" terminalId="connector15terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector15pad"/>
</pcbView>
</views>
</connector>
<connector id="connector13" name="OUT-A" type="male">
<description>OUT-A</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector13pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector13pin" terminalId="connector13terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector13pad"/>
</pcbView>
</views>
</connector>
<connector id="connector9" name="OUT-B" type="male">
<description>OUT-B</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector9pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector9pin" terminalId="connector9terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector9pad"/>
</pcbView>
</views>
</connector>
<connector id="connector7" name="S_R+" type="male">
<description>S_R+</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector7pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector7pin" terminalId="connector7terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector7pad"/>
</pcbView>
</views>
</connector>
<connector id="connector10" name="S_R-" type="male">
<description>S_R-</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector10pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector10pin" terminalId="connector10terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector10pad"/>
</pcbView>
</views>
</connector>
<connector id="connector3" name="VB" type="male">
<description>VB</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector3pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector3pin" terminalId="connector3terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector3pad"/>
</pcbView>
</views>
</connector>
</connectors>
<buses>
</buses>
</module>