<?xml version='1.0' encoding='UTF-8'?>
<module fritzingVersion="0.4.1b.07.17.4356" moduleId="atlas-sientific_Conductivity Circuit" referenceFile="atlas-sientific_Conductivity Circuit.fzp">
 <author>Atlas Scientific </author>
 <title>Conductivity Circuit</title>
 <label>Conductivity Circuit</label>
 <date>Fri Jul 19 2013</date>
 <tags/>
 <properties>
  <property name="family">Conductivity</property>
  <property name="variant">V3</property>
 </properties>
 <description>&lt;!DOCTYPE HTML PUBLIC "-//W3C//DTD HTML 4.0//EN" "http://www.w3.org/TR/REC-html40/strict.dtd">
&lt;html>&lt;head>&lt;meta name="qrichtext" content="1" />&lt;style type="text/css">
p, li { white-space: pre-wrap; }
&lt;/style>&lt;/head>&lt;body style=" font-family:'MS Shell Dlg 2'; font-size:8.25pt; font-weight:400; font-style:normal;">
&lt;p style=" margin-top:0px; margin-bottom:0px; margin-left:0px; margin-right:0px; -qt-block-indent:0; text-indent:0px;">&lt;span style=" font-size:8pt;">There was a time when manufacturing custom scientific equipment for a project was only available to the elite; a time when environmental data was only available to governments and subject to the political pressures of the day. Atlas Scientific is working hard to end those days. We are the new scientists, all of us. Reading the Electrical Conductivity (E.C.), total dissolved solids and salinity of water, was notoriously hard to do. With little information available on the subject, many engineers had to abandon their goal of adding a conductivity circuit to their design. Atlas Scientific has finally put an end to this problem.&lt;/span>&lt;/p>
&lt;p style="-qt-paragraph-type:empty; margin-top:0px; margin-bottom:0px; margin-left:0px; margin-right:0px; -qt-block-indent:0; text-indent:0px; font-size:8pt;">&lt;br />&lt;/p>
&lt;p style=" margin-top:0px; margin-bottom:0px; margin-left:0px; margin-right:0px; -qt-block-indent:0; text-indent:0px;">&lt;span style=" font-size:8pt;">The Atlas Scientific Conductivity Circuit is small, modularized, and designed specifically to read the conductivity, total dissolved solids and salinity of water.&lt;/span>&lt;/p>
&lt;p style="-qt-paragraph-type:empty; margin-top:0px; margin-bottom:0px; margin-left:0px; margin-right:0px; -qt-block-indent:0; text-indent:0px; font-size:8pt;">&lt;br />&lt;/p>
&lt;p style=" margin-top:0px; margin-bottom:0px; margin-left:0px; margin-right:0px; -qt-block-indent:0; text-indent:0px;">&lt;span style=" font-size:8pt;">The Atlas Scientific Conductivity Circuit is designed for both continuous and intermittent readings. After calibration, the Conductivity Sensor can be immersed in a liquid and operate continuously for 12 months before recalibration is recommended.&lt;/span>&lt;/p>
&lt;p style="-qt-paragraph-type:empty; margin-top:0px; margin-bottom:0px; margin-left:0px; margin-right:0px; -qt-block-indent:0; text-indent:0px; font-size:8pt;">&lt;br />&lt;/p>
&lt;p style=" margin-top:0px; margin-bottom:0px; margin-left:0px; margin-right:0px; -qt-block-indent:0; text-indent:0px;">&lt;span style=" font-size:8pt;">• Conductivity readings +/- 5μs&lt;/span>&lt;/p>
&lt;p style=" margin-top:0px; margin-bottom:0px; margin-left:0px; margin-right:0px; -qt-block-indent:0; text-indent:0px;">&lt;span style=" font-size:8pt;">• Full Conductivity capability from 11μs to 92,000μs&lt;/span>&lt;/p>
&lt;p style=" margin-top:0px; margin-bottom:0px; margin-left:0px; margin-right:0px; -qt-block-indent:0; text-indent:0px;">&lt;span style=" font-size:8pt;">• Temperature dependent or temperature independent readings&lt;/span>&lt;/p>
&lt;p style=" margin-top:0px; margin-bottom:0px; margin-left:0px; margin-right:0px; -qt-block-indent:0; text-indent:0px;">&lt;span style=" font-size:8pt;">• Total dissolved solids (TDS) referenced to KCL&lt;/span>&lt;/p>
&lt;p style=" margin-top:0px; margin-bottom:0px; margin-left:0px; margin-right:0px; -qt-block-indent:0; text-indent:0px;">&lt;span style=" font-size:8pt;">• Salinity is derived from the Practical Salinity Scale (PSS-78)&lt;/span>&lt;/p>
&lt;p style=" margin-top:0px; margin-bottom:0px; margin-left:0px; margin-right:0px; -qt-block-indent:0; text-indent:0px;">&lt;span style=" font-size:8pt;">• Data output is a comma separated string: μs, TDS, Salinity&lt;/span>&lt;/p>
&lt;p style=" margin-top:0px; margin-bottom:0px; margin-left:0px; margin-right:0px; -qt-block-indent:0; text-indent:0px;">&lt;span style=" font-size:8pt;">• Single reading or continuous reading modes&lt;/span>&lt;/p>
&lt;p style=" margin-top:0px; margin-bottom:0px; margin-left:0px; margin-right:0px; -qt-block-indent:0; text-indent:0px;">&lt;span style=" font-size:8pt;">• Simple asynchronous serial connectivity (voltage swing 0-5v)&lt;/span>&lt;/p>
&lt;p style=" margin-top:0px; margin-bottom:0px; margin-left:0px; margin-right:0px; -qt-block-indent:0; text-indent:0px;">&lt;span style=" font-size:8pt;">• Simple instruction set consisting of only 6 (not including   calibration) commands&lt;/span>&lt;/p>
&lt;p style=" margin-top:0px; margin-bottom:0px; margin-left:0px; margin-right:0px; -qt-block-indent:0; text-indent:0px;">&lt;span style=" font-size:8pt;">• Micro footprint circuitry&lt;/span>&lt;/p>
&lt;p style=" margin-top:0px; margin-bottom:0px; margin-left:0px; margin-right:0px; -qt-block-indent:0; text-indent:0px;">&lt;span style=" font-size:8pt;">• Debugging LED's&lt;/span>&lt;/p>
&lt;p style=" margin-top:0px; margin-bottom:0px; margin-left:0px; margin-right:0px; -qt-block-indent:0; text-indent:0px;">&lt;span style=" font-size:8pt;">• 5V operational voltage&lt;/span>&lt;/p>
&lt;p style=" margin-top:0px; margin-bottom:0px; margin-left:0px; margin-right:0px; -qt-block-indent:0; text-indent:0px;">&lt;span style=" font-size:8pt;">• Dimensions: 18.4mm X 20.56mm (0.72&amp;quot; X0.80&amp;quot;)&lt;/span>&lt;/p>&lt;/body>&lt;/html></description>
 <views>
  <iconView>
   <layers image="icon/atlas-sientific_Conductivity Circuit_icon.svg">
    <layer layerId="icon"/>
   </layers>
  </iconView>
  <schematicView>
   <layers image="schematic/atlas-sientific_Conductivity Circuit_schematic.svg">
    <layer layerId="schematic"/>
   </layers>
  </schematicView>
  <breadboardView>
   <layers image="breadboard/atlas-sientific_Conductivity Circuit_breadboard.svg">
    <layer layerId="breadboard"/>
   </layers>
  </breadboardView>
  <pcbView>
   <layers image="pcb/atlas-sientific_Conductivity Circuit_pcb.svg">
    <layer layerId="copper0"/>
    <layer layerId="silkscreen"/>
    <layer layerId="copper1"/>
   </layers>
  </pcbView>
 </views>
 <connectors>
  <connector type="male" id="connector0" name="GND">
   <description>Supply Ground</description>
   <views>
    <breadboardView>
     <p svgId="connector0pin" layer="breadboard"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector0pin" layer="schematic" terminalId="connector0terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector0pin" layer="copper1"/>
     <p svgId="connector0pin" layer="copper0"/>
    </pcbView>
   </views>
  </connector>
  <connector type="male" id="connector1" name="TX">
   <description>Data Out</description>
   <views>
    <breadboardView>
     <p svgId="connector1pin" layer="breadboard"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector1pin" layer="schematic" terminalId="connector1terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector1pin" layer="copper1"/>
     <p svgId="connector1pin" layer="copper0"/>
    </pcbView>
   </views>
  </connector>
  <connector type="male" id="connector2" name="RX">
   <description>Data In</description>
   <views>
    <breadboardView>
     <p svgId="connector2pin" layer="breadboard"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector2pin" layer="schematic" terminalId="connector2terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector2pin" layer="copper1"/>
     <p svgId="connector2pin" layer="copper0"/>
    </pcbView>
   </views>
  </connector>
  <connector type="male" id="connector3" name="Vcc">
   <description>Supply Voltage</description>
   <views>
    <breadboardView>
     <p svgId="connector3pin" layer="breadboard"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector3pin" layer="schematic"/>
    </schematicView>
    <pcbView>
     <p svgId="connector3pin" layer="copper1"/>
     <p svgId="connector3pin" layer="copper0"/>
    </pcbView>
   </views>
  </connector>
  <connector type="male" id="connector4" name="PRB">
   <description>Probe (Sensor)</description>
   <views>
    <breadboardView>
     <p svgId="connector4pin" layer="breadboard"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector4pin" layer="schematic"/>
    </schematicView>
    <pcbView>
     <p svgId="connector4pin" layer="copper1"/>
     <p svgId="connector4pin" layer="copper0"/>
    </pcbView>
   </views>
  </connector>
  <connector type="male" id="connector5" name="GND">
   <description>Supply Ground</description>
   <views>
    <breadboardView>
     <p svgId="connector5pin" layer="breadboard"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector5pin" layer="schematic"/>
    </schematicView>
    <pcbView>
     <p svgId="connector5pin" layer="copper1"/>
     <p svgId="connector5pin" layer="copper0"/>
    </pcbView>
   </views>
  </connector>
 </connectors>
 <url>https://www.atlas-scientific.com/product_pages/embedded/ec.html</url>
</module>
