<?xml version="1.0" encoding="UTF-8"?><module fritzingVersion="0.7.2b" moduleId="SparkFun-RF-MN5010HS-SMD">
<!-- generated from Sparkfun Eagle Library 'SparkFun-RF' MN5010HS SMD -->
<version>4</version>
<date>2013-02-13</date>
<label>U</label>
<author>www.fritzing.org</author>
<description>MN5010HS GPS Receiver Module. Packagse GR-10 and MN5010HS are NOT tested with this device.</description>
<title>MN5010HS</title>
<tags>
<tag>MN5010HS</tag>
<tag>SMD</tag>
</tags>
<properties>
<property name="package">mn5010hs</property>
<property name="family">sparkfun GPS Reveiver</property>
<property name="chip">MN5010HS</property>
<property name="variant">smd</property>
</properties>
<views>
<breadboardView>
<layers image="breadboard/sparkfun-rf_mn5010hs_breadboard.svg">
<layer layerId="breadboard"/>
</layers>
</breadboardView>
<schematicView>
<layers image="schematic/sparkfun-rf_mn5010hs_schematic.svg">
<layer layerId="schematic"/>
</layers>
</schematicView>
<pcbView>
<layers image="pcb/sparkfun-rf_mn5010hs_pcb.svg">
<layer layerId="copper1"/>
<layer layerId="silkscreen"/>
</layers>
</pcbView>
<iconView>
<layers image="icon/MN5010HS.svg">
<layer layerId="icon"/>
</layers>
</iconView>
</views>
<connectors>
</connectors>
</module>