<?xml version="1.0" encoding="UTF-8"?><module fritzingVersion="0.1.1255" moduleId="2244EBEC21">
 <version replacedby="2244EBEC21e">4</version>
 <author>Stefan Hermann</author>
 <title>PNP-Transistor</title>
 <label>Q</label>
 <date>2008-10-10</date>
 <tags>
  <tag>pnp</tag>
  <tag>transistor</tag>
  <tag>signal transistor</tag>
  <tag>amplifier</tag>
  <tag>fritzing core</tag>
 </tags>
 <properties>
  <property name="package">TO92 [THT]</property>
  <property name="family">//obsolete// Bipolar Transistor</property>
  <property name="type">PNP</property>
 </properties>
 <description>A standard PNP signal transistor</description>
 <views>
  <iconView>
   <layers image="icon/basic_transistor_pnpicon.svg">
    <layer layerId="icon"/>
   </layers>
  </iconView>
  <breadboardView>
   <layers image="breadboard/transistor_pnp.svg">
    <layer layerId="breadboard"/>
   </layers>
  </breadboardView>
 <schematicView fliphorizontal="true" flipvertical="true">
   <layers image="schematic/basic_transistor_pnp.svg">
    <layer layerId="schematic"/>
   </layers>
  </schematicView>
  <pcbView>
   <layers image="pcb/TO92_3_100mil_pcb.svg">
    <layer layerId="copper0"/>
    <layer layerId="silkscreen"/>
   <layer layerId="copper1"/></layers>
  </pcbView>
 </views>
 <connectors>
  <connector id="connector0" name="E" type="male">
   <description>Emitter</description>
   <views>
    <breadboardView>
     <p layer="breadboard" svgId="connector0pin"  legId="connector0leg"/>
    </breadboardView>
    <schematicView>
     <p layer="schematic" svgId="connector2pin" terminalId="connector2terminal"/>
    </schematicView>
    <pcbView>
     <p layer="copper0" svgId="connector2pin"/>
    <p layer="copper1" svgId="connector2pin"/></pcbView>
   </views>
  </connector>
  <connector id="connector1" name="B" type="male">
   <description>Base</description>
   <views>
    <breadboardView>
     <p layer="breadboard" svgId="connector1pin"  legId="connector1leg"/>
    </breadboardView>
    <schematicView>
     <p layer="schematic" svgId="connector0pin" terminalId="connector0terminal"/>
    </schematicView>
    <pcbView>
     <p layer="copper0" svgId="connector1pin"/>
    <p layer="copper1" svgId="connector1pin"/></pcbView>
   </views>
  </connector>
  <connector id="connector2" name="C" type="male">
   <description>Collector</description>
   <views>
    <breadboardView>
     <p layer="breadboard" svgId="connector2pin"  legId="connector2leg"/>
    </breadboardView>
    <schematicView>
     <p layer="schematic" svgId="connector1pin" terminalId="connector1terminal"/>
    </schematicView>
    <pcbView>
     <p layer="copper0" svgId="connector0pin"/>
    <p layer="copper1" svgId="connector0pin"/></pcbView>
   </views>
  </connector>
 </connectors>
</module>
