<?xml version="1.0" encoding="UTF-8"?>
<module fritzingVersion="0.7.0b.02.01.5801" moduleId="M5450_LED_Driver">
    <version>4</version>
    <author>Christopher Mann</author>
    <title>M5450 LED Driver</title>
    <label>M5450</label>
    <date>2012-03-04</date>
    <tags>
        <tag>DIP</tag>
        <tag>user part</tag>
        <tag>shift register</tag>
        <tag>LED driver</tag>
        <tag>74HC595</tag>
    </tags>
    <properties>
        <property name="package">DIP (Dual Inline) [THT]</property>
        <property name="family">IC</property>
        <property name="editable pin labels">true</property>
        <property name="chip label">IC</property>
        <property name="part number"></property>
        <property name="pins">40</property>
        <property name="spacing">600mil</property>
    </properties>
    <description>The M5450 is a monolithic MOS integrated circuit produced with an N-channel silicon gate technology.  A single pin controls the LED display brightness by setting a reference current through a variable resistor connected to Vdd or to a separate supply of 13.2V maximum.</description>
    <views>
        <iconView>
            <layers image="icon/M5450_LED_Driver_icon.svg">
                <layer layerId="icon"/>
            </layers>
        </iconView>
        <breadboardView>
            <layers image="breadboard/M5450_LED_Driver_breadboard.svg">
                <layer layerId="breadboard"/>
            </layers>
        </breadboardView>
        <schematicView>
            <layers image="schematic/M5450_LED_Driver_schematic.svg">
                <layer layerId="schematic"/>
            </layers>
        </schematicView>
        <pcbView>
            <layers image="pcb/M5450_LED_Driver_pcb.svg">
                <layer layerId="copper0"/>
                <layer layerId="silkscreen"/>
                <layer layerId="copper1"/>
            </layers>
        </pcbView>
    </views>
    <connectors>
        <connector id="connector3" type="male" name="out 15">
            <description>output 15</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector3pin" terminalId="connector3terminal"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector3pin" terminalId="connector3terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper1" svgId="connector3pin"/>
                    <p layer="copper0" svgId="connector3pin"/>
                </pcbView>
            </views>
        </connector>
        <connector id="connector20" type="male" name="clock in">
            <description>clock in</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector20pin" terminalId="connector20terminal"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector20pin" terminalId="connector20terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper1" svgId="connector20pin"/>
                    <p layer="copper0" svgId="connector20pin"/>
                </pcbView>
            </views>
        </connector>
        <connector id="connector4" type="male" name="out 14">
            <description>output 14</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector4pin" terminalId="connector4terminal"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector4pin" terminalId="connector4terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper1" svgId="connector4pin"/>
                    <p layer="copper0" svgId="connector4pin"/>
                </pcbView>
            </views>
        </connector>
        <connector id="connector21" type="male" name="data in">
            <description>data in</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector21pin" terminalId="connector21terminal"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector21pin" terminalId="connector21terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper1" svgId="connector21pin"/>
                    <p layer="copper0" svgId="connector21pin"/>
                </pcbView>
            </views>
        </connector>
        <connector id="connector5" type="male" name="out 13">
            <description>output 13</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector5pin" terminalId="connector5terminal"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector5pin" terminalId="connector5terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper1" svgId="connector5pin"/>
                    <p layer="copper0" svgId="connector5pin"/>
                </pcbView>
            </views>
        </connector>
        <connector id="connector22" type="male" name="data enable">
            <description>data enable</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector22pin" terminalId="connector22terminal"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector22pin" terminalId="connector22terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper1" svgId="connector22pin"/>
                    <p layer="copper0" svgId="connector22pin"/>
                </pcbView>
            </views>
        </connector>
        <connector id="connector6" type="male" name="out 12">
            <description>output 12</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector6pin" terminalId="connector6terminal"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector6pin" terminalId="connector6terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper1" svgId="connector6pin"/>
                    <p layer="copper0" svgId="connector6pin"/>
                </pcbView>
            </views>
        </connector>
        <connector id="connector7" type="male" name="out 11">
            <description>output 11</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector7pin" terminalId="connector7terminal"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector7pin" terminalId="connector7terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper1" svgId="connector7pin"/>
                    <p layer="copper0" svgId="connector7pin"/>
                </pcbView>
            </views>
        </connector>
        <connector id="connector23" type="male" name="out 34">
            <description>output 34</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector23pin" terminalId="connector23terminal"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector23pin" terminalId="connector23terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper1" svgId="connector23pin"/>
                    <p layer="copper0" svgId="connector23pin"/>
                </pcbView>
            </views>
        </connector>
        <connector id="connector8" type="male" name="out 10">
            <description>output 10</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector8pin" terminalId="connector8terminal"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector8pin" terminalId="connector8terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper1" svgId="connector8pin"/>
                    <p layer="copper0" svgId="connector8pin"/>
                </pcbView>
            </views>
        </connector>
        <connector id="connector24" type="male" name="out 33">
            <description>output 33</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector24pin" terminalId="connector24terminal"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector24pin" terminalId="connector24terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper1" svgId="connector24pin"/>
                    <p layer="copper0" svgId="connector24pin"/>
                </pcbView>
            </views>
        </connector>
        <connector id="connector9" type="male" name="out 9">
            <description>output 9</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector9pin" terminalId="connector9terminal"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector9pin" terminalId="connector9terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper1" svgId="connector9pin"/>
                    <p layer="copper0" svgId="connector9pin"/>
                </pcbView>
            </views>
        </connector>
        <connector id="connector25" type="male" name="out 32">
            <description>output 32</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector25pin" terminalId="connector25terminal"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector25pin" terminalId="connector25terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper1" svgId="connector25pin"/>
                    <p layer="copper0" svgId="connector25pin"/>
                </pcbView>
            </views>
        </connector>
        <connector id="connector26" type="male" name="out 31">
            <description>output 31</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector26pin" terminalId="connector26terminal"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector26pin" terminalId="connector26terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper1" svgId="connector26pin"/>
                    <p layer="copper0" svgId="connector26pin"/>
                </pcbView>
            </views>
        </connector>
        <connector id="connector27" type="male" name="out 30">
            <description>output 30</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector27pin" terminalId="connector27terminal"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector27pin" terminalId="connector27terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper1" svgId="connector27pin"/>
                    <p layer="copper0" svgId="connector27pin"/>
                </pcbView>
            </views>
        </connector>
        <connector id="connector28" type="male" name="out 29">
            <description>output 29</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector28pin" terminalId="connector28terminal"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector28pin" terminalId="connector28terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper1" svgId="connector28pin"/>
                    <p layer="copper0" svgId="connector28pin"/>
                </pcbView>
            </views>
        </connector>
        <connector id="connector29" type="male" name="out 28">
            <description>output 28</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector29pin" terminalId="connector29terminal"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector29pin" terminalId="connector29terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper1" svgId="connector29pin"/>
                    <p layer="copper0" svgId="connector29pin"/>
                </pcbView>
            </views>
        </connector>
        <connector id="connector30" type="male" name="out 27">
            <description>output 27</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector30pin" terminalId="connector30terminal"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector30pin" terminalId="connector30terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper1" svgId="connector30pin"/>
                    <p layer="copper0" svgId="connector30pin"/>
                </pcbView>
            </views>
        </connector>
        <connector id="connector31" type="male" name="out 26">
            <description>output 26</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector31pin" terminalId="connector31terminal"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector31pin" terminalId="connector31terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper1" svgId="connector31pin"/>
                    <p layer="copper0" svgId="connector31pin"/>
                </pcbView>
            </views>
        </connector>
        <connector id="connector32" type="male" name="out 25">
            <description>output 25</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector32pin" terminalId="connector32terminal"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector32pin" terminalId="connector32terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper1" svgId="connector32pin"/>
                    <p layer="copper0" svgId="connector32pin"/>
                </pcbView>
            </views>
        </connector>
        <connector id="connector33" type="male" name="out 24">
            <description>output 24</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector33pin" terminalId="connector33terminal"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector33pin" terminalId="connector33terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper1" svgId="connector33pin"/>
                    <p layer="copper0" svgId="connector33pin"/>
                </pcbView>
            </views>
        </connector>
        <connector id="connector34" type="male" name="out 23">
            <description>output 23</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector34pin" terminalId="connector34terminal"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector34pin" terminalId="connector34terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper1" svgId="connector34pin"/>
                    <p layer="copper0" svgId="connector34pin"/>
                </pcbView>
            </views>
        </connector>
        <connector id="connector35" type="male" name="out 22">
            <description>output 22</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector35pin" terminalId="connector35terminal"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector35pin" terminalId="connector35terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper1" svgId="connector35pin"/>
                    <p layer="copper0" svgId="connector35pin"/>
                </pcbView>
            </views>
        </connector>
        <connector id="connector36" type="male" name="out 21">
            <description>output 21</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector36pin" terminalId="connector36terminal"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector36pin" terminalId="connector36terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper1" svgId="connector36pin"/>
                    <p layer="copper0" svgId="connector36pin"/>
                </pcbView>
            </views>
        </connector>
        <connector id="connector37" type="male" name="out 20">
            <description>output 20</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector37pin" terminalId="connector37terminal"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector37pin" terminalId="connector37terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper1" svgId="connector37pin"/>
                    <p layer="copper0" svgId="connector37pin"/>
                </pcbView>
            </views>
        </connector>
        <connector id="connector38" type="male" name="out 19">
            <description>output 19</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector38pin" terminalId="connector38terminal"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector38pin" terminalId="connector38terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper1" svgId="connector38pin"/>
                    <p layer="copper0" svgId="connector38pin"/>
                </pcbView>
            </views>
        </connector>
        <connector id="connector39" type="male" name="out 18">
            <description>output 18</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector39pin" terminalId="connector39terminal"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector39pin" terminalId="connector39terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper1" svgId="connector39pin"/>
                    <p layer="copper0" svgId="connector39pin"/>
                </pcbView>
            </views>
        </connector>
        <connector id="connector10" type="male" name="out 8">
            <description>output 8</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector10pin" terminalId="connector10terminal"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector10pin" terminalId="connector10terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper1" svgId="connector10pin"/>
                    <p layer="copper0" svgId="connector10pin"/>
                </pcbView>
            </views>
        </connector>
        <connector id="connector11" type="male" name="out 7">
            <description>output 7</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector11pin" terminalId="connector11terminal"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector11pin" terminalId="connector11terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper1" svgId="connector11pin"/>
                    <p layer="copper0" svgId="connector11pin"/>
                </pcbView>
            </views>
        </connector>
        <connector id="connector12" type="male" name="out 6">
            <description>output 6</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector12pin" terminalId="connector12terminal"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector12pin" terminalId="connector12terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper1" svgId="connector12pin"/>
                    <p layer="copper0" svgId="connector12pin"/>
                </pcbView>
            </views>
        </connector>
        <connector id="connector13" type="male" name="out 5">
            <description>output 5</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector13pin" terminalId="connector13terminal"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector13pin" terminalId="connector13terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper1" svgId="connector13pin"/>
                    <p layer="copper0" svgId="connector13pin"/>
                </pcbView>
            </views>
        </connector>
        <connector id="connector14" type="male" name="out 4">
            <description>output 4</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector14pin" terminalId="connector14terminal"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector14pin" terminalId="connector14terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper1" svgId="connector14pin"/>
                    <p layer="copper0" svgId="connector14pin"/>
                </pcbView>
            </views>
        </connector>
        <connector id="connector15" type="male" name="out 3">
            <description>output 3</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector15pin" terminalId="connector15terminal"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector15pin" terminalId="connector15terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper1" svgId="connector15pin"/>
                    <p layer="copper0" svgId="connector15pin"/>
                </pcbView>
            </views>
        </connector>
        <connector id="connector16" type="male" name="out 2">
            <description>output 2</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector16pin" terminalId="connector16terminal"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector16pin" terminalId="connector16terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper1" svgId="connector16pin"/>
                    <p layer="copper0" svgId="connector16pin"/>
                </pcbView>
            </views>
        </connector>
        <connector id="connector17" type="male" name="out 1">
            <description>output 1</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector17pin" terminalId="connector17terminal"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector17pin" terminalId="connector17terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper1" svgId="connector17pin"/>
                    <p layer="copper0" svgId="connector17pin"/>
                </pcbView>
            </views>
        </connector>
        <connector id="connector18" type="male" name="brightness">
            <description>brightness</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector18pin" terminalId="connector18terminal"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector18pin" terminalId="connector18terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper1" svgId="connector18pin"/>
                    <p layer="copper0" svgId="connector18pin"/>
                </pcbView>
            </views>
        </connector>
        <connector id="connector19" type="male" name="Vdd">
            <description>Vdd</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector19pin" terminalId="connector19terminal"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector19pin" terminalId="connector19terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper1" svgId="connector19pin"/>
                    <p layer="copper0" svgId="connector19pin"/>
                </pcbView>
            </views>
        </connector>
        <connector id="connector0" type="male" name="Vss">
            <description>Vss</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector0pin" terminalId="connector0terminal"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector0pin" terminalId="connector0terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper1" svgId="connector0pin"/>
                    <p layer="copper0" svgId="connector0pin"/>
                </pcbView>
            </views>
        </connector>
        <connector id="connector1" type="male" name="out 17">
            <description>output 17</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector1pin" terminalId="connector1terminal"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector1pin" terminalId="connector1terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper1" svgId="connector1pin"/>
                    <p layer="copper0" svgId="connector1pin"/>
                </pcbView>
            </views>
        </connector>
        <connector id="connector2" type="male" name="out 16">
            <description>output 16</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector2pin" terminalId="connector2terminal"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector2pin" terminalId="connector2terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper1" svgId="connector2pin"/>
                    <p layer="copper0" svgId="connector2pin"/>
                </pcbView>
            </views>
        </connector>
    </connectors>
</module>
