<?xml version='1.0' encoding='UTF-8'?>
<module fritzingVersion='0.5.2b.02.18.4756' moduleId='Arduino-Mini-v5'>
<version>5</version>
<date>2013-04-03</date>
<author>althaus</author>
<description>The Arduino Mini is a small microcontroller board originally based on the ATmega168, but now supplied with the 328.(datasheet), intended for use on breadboards and when space is at a premium. It has 14 digital input/output pins (of which 6 can be used as PWM outputs), 8 analog inputs, and a 16 MHz crystal oscillator. It can be programmed with the USB Serial adapter or other USB or RS232 to TTL serial adapter.



The new Mini (revision 05) has a new package for the ATmega328, which enables all components to be on the top of the board. It also has an onboard reset button. The new version has the same pin configuration as revision 04.



Warning: Don&apos;t power the Arduino mini with more than 9 volts, or plug the power in backwards: you&apos;ll probably kill it. 

</description>
<title>Arduino Mini (Rev5)</title>   
<label>Arduino</label>
<url>http://arduino.cc/en/Main/ArduinoBoardMini</url>
<tags>
<tag>arduino</tag>
<tag>mini</tag>
<tag>ATmega328</tag>
</tags>
<properties>
<property name='family'>microcontroller board (arduino)</property>
<property name='type'>Arduino Mini (Rev5)</property>
</properties>
<views>
<breadboardView>
<layers image='breadboard/Arduino-Mini-v5_breadboard.svg'>
<layer layerId='breadboardbreadboard'/>
</layers>
</breadboardView>
<schematicView>
<layers image='schematic/Arduino-Mini-v5_schematic.svg'>
<layer layerId='schematic'/>
</layers>
</schematicView>
<pcbView>
<layers image='pcb/Arduino-Mini-v5_pcb.svg'>
<layer layerId='copper1'/>
<layer layerId='silkscreen'/>
<layer layerId='copper0'/>
</layers>
</pcbView>
<iconView>
<layers image='breadboard/Arduino-Mini-v5_breadboard.svg'>
<layer layerId='icon'/>
</layers>
</iconView>
</views>
<connectors>
<connector id='connector25' type='male' name='D0/TX'>
<description>D0/TX</description><views>
<breadboardView>
<p layer='breadboardbreadboard' svgId='connector25pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector25pin' terminalId='connector25terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector25pad'/><p layer='copper1' svgId='connector25pad'/></pcbView>
</views>
</connector>
<connector id='connector26' type='male' name='D1/RX'>
<description>D1/RX</description><views>
<breadboardView>
<p layer='breadboardbreadboard' svgId='connector26pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector26pin' terminalId='connector26terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector26pad'/><p layer='copper1' svgId='connector26pad'/></pcbView>
</views>
</connector>
<connector id='connector27' type='male' name='RESET'>
<description>RESET</description><views>
<breadboardView>
<p layer='breadboardbreadboard' svgId='connector27pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector27pin' terminalId='connector27terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector27pad'/><p layer='copper1' svgId='connector27pad'/></pcbView>
</views>
</connector>
<connector id='connector28' type='male' name='GND'>
<description>GND</description><views>
<breadboardView>
<p layer='breadboardbreadboard' svgId='connector28pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector28pin' terminalId='connector28terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector28pad'/><p layer='copper1' svgId='connector28pad'/></pcbView>
</views>
</connector>
<connector id='connector29' type='male' name='D2'>
<description>D2</description><views>
<breadboardView>
<p layer='breadboardbreadboard' svgId='connector29pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector29pin' terminalId='connector29terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector29pad'/><p layer='copper1' svgId='connector29pad'/></pcbView>
</views>
</connector>
<connector id='connector30' type='male' name='D3 PWM'>
<description>D3 PWM</description><views>
<breadboardView>
<p layer='breadboardbreadboard' svgId='connector30pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector30pin' terminalId='connector30terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector30pad'/><p layer='copper1' svgId='connector30pad'/></pcbView>
</views>
</connector>
<connector id='connector31' type='male' name='D4'>
<description>D4</description><views>
<breadboardView>
<p layer='breadboardbreadboard' svgId='connector31pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector31pin' terminalId='connector31terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector31pad'/><p layer='copper1' svgId='connector31pad'/></pcbView>
</views>
</connector>
<connector id='connector32' type='male' name='D5 PWM'>
<description>D5 PWM</description><views>
<breadboardView>
<p layer='breadboardbreadboard' svgId='connector32pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector32pin' terminalId='connector32terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector32pad'/><p layer='copper1' svgId='connector32pad'/></pcbView>
</views>
</connector>
<connector id='connector33' type='male' name='D6 PWM'>
<description>D6 PWM</description><views>
<breadboardView>
<p layer='breadboardbreadboard' svgId='connector33pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector33pin' terminalId='connector33terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector33pad'/><p layer='copper1' svgId='connector33pad'/></pcbView>
</views>
</connector>
<connector id='connector34' type='male' name='D7'>
<description>D7</description><views>
<breadboardView>
<p layer='breadboardbreadboard' svgId='connector34pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector34pin' terminalId='connector34terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector34pad'/><p layer='copper1' svgId='connector34pad'/></pcbView>
</views>
</connector>
<connector id='connector35' type='male' name='D8'>
<description>D8</description><views>
<breadboardView>
<p layer='breadboardbreadboard' svgId='connector35pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector35pin' terminalId='connector35terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector35pad'/><p layer='copper1' svgId='connector35pad'/></pcbView>
</views>
</connector>
<connector id='connector36' type='male' name='D9 PWM'>
<description>D9 PWM</description><views>
<breadboardView>
<p layer='breadboardbreadboard' svgId='connector36pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector36pin' terminalId='connector36terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector36pad'/><p layer='copper1' svgId='connector36pad'/></pcbView>
</views>
</connector>
<connector id='connector37' type='male' name='VCC'>
<description>VCC</description><views>
<breadboardView>
<p layer='breadboardbreadboard' svgId='connector37pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector37pin' terminalId='connector37terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector37pad'/><p layer='copper1' svgId='connector37pad'/></pcbView>
</views>
</connector>
<connector id='connector38' type='male' name='GND'>
<description>GND</description><views>
<breadboardView>
<p layer='breadboardbreadboard' svgId='connector38pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector38pin' terminalId='connector38terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector38pad'/><p layer='copper1' svgId='connector38pad'/></pcbView>
</views>
</connector>
<connector id='connector39' type='male' name='RESET'>
<description>RESET</description><views>
<breadboardView>
<p layer='breadboardbreadboard' svgId='connector39pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector39pin' terminalId='connector39terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector39pad'/><p layer='copper1' svgId='connector39pad'/></pcbView>
</views>
</connector>
<connector id='connector40' type='male' name='5V'>
<description>5V</description><views>
<breadboardView>
<p layer='breadboardbreadboard' svgId='connector40pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector40pin' terminalId='connector40terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector40pad'/><p layer='copper1' svgId='connector40pad'/></pcbView>
</views>
</connector>
<connector id='connector41' type='male' name='A3'>
<description>A3</description><views>
<breadboardView>
<p layer='breadboardbreadboard' svgId='connector41pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector41pin' terminalId='connector41terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector41pad'/><p layer='copper1' svgId='connector41pad'/></pcbView>
</views>
</connector>
<connector id='connector42' type='male' name='A2'>
<description>A2</description><views>
<breadboardView>
<p layer='breadboardbreadboard' svgId='connector42pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector42pin' terminalId='connector42terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector42pad'/><p layer='copper1' svgId='connector42pad'/></pcbView>
</views>
</connector>
<connector id='connector43' type='male' name='A1'>
<description>A1</description><views>
<breadboardView>
<p layer='breadboardbreadboard' svgId='connector43pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector43pin' terminalId='connector43terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector43pad'/><p layer='copper1' svgId='connector43pad'/></pcbView>
</views>
</connector>
<connector id='connector44' type='male' name='A0'>
<description>A0</description><views>
<breadboardView>
<p layer='breadboardbreadboard' svgId='connector44pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector44pin' terminalId='connector44terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector44pad'/><p layer='copper1' svgId='connector44pad'/></pcbView>
</views>
</connector>
<connector id='connector45' type='male' name='D13'>
<description>D13</description><views>
<breadboardView>
<p layer='breadboardbreadboard' svgId='connector45pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector45pin' terminalId='connector45terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector45pad'/><p layer='copper1' svgId='connector45pad'/></pcbView>
</views>
</connector>
<connector id='connector46' type='male' name='D12'>
<description>D12</description><views>
<breadboardView>
<p layer='breadboardbreadboard' svgId='connector46pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector46pin' terminalId='connector46terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector46pad'/><p layer='copper1' svgId='connector46pad'/></pcbView>
</views>
</connector>
<connector id='connector47' type='male' name='D11 PWM'>
<description>D11 PWM</description><views>
<breadboardView>
<p layer='breadboardbreadboard' svgId='connector47pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector47pin' terminalId='connector47terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector47pad'/><p layer='copper1' svgId='connector47pad'/></pcbView>
</views>
</connector>
<connector id='connector48' type='male' name='D10 PWM'>
<description>D10 PWM</description><views>
<breadboardView>
<p layer='breadboardbreadboard' svgId='connector48pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector48pin' terminalId='connector48terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector48pad'/><p layer='copper1' svgId='connector48pad'/></pcbView>
</views>
</connector>
<connector id='connector49' type='female' name='A6'>
<description>A6</description><views>
<breadboardView>
<p layer='breadboardbreadboard' svgId='connector49pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector49pin' terminalId='connector49terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector49pad'/><p layer='copper1' svgId='connector49pad'/></pcbView>
</views>
</connector>
<connector id='connector50' type='female' name='A4'>
<description>A4</description><views>
<breadboardView>
<p layer='breadboardbreadboard' svgId='connector50pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector50pin' terminalId='connector50terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector50pad'/><p layer='copper1' svgId='connector50pad'/></pcbView>
</views>
</connector>
<connector id='connector51' type='female' name='A7'>
<description>A7</description><views>
<breadboardView>
<p layer='breadboardbreadboard' svgId='connector51pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector51pin' terminalId='connector51terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector51pad'/><p layer='copper1' svgId='connector51pad'/></pcbView>
</views>
</connector>
<connector id='connector52' type='female' name='A5'>
<description>A5</description><views>
<breadboardView>
<p layer='breadboardbreadboard' svgId='connector52pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector52pin' terminalId='connector52terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector52pad'/><p layer='copper1' svgId='connector52pad'/></pcbView>
</views>
</connector>
<connector id='connector53' type='female' name='RESET'>
<description>RESET</description><views>
<breadboardView>
<p layer='breadboardbreadboard' svgId='connector53pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector53pin' terminalId='connector53terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector53pad'/><p layer='copper1' svgId='connector53pad'/></pcbView>
</views>
</connector>
<connector id='connector54' type='female' name='TX'>
<description>TX</description><views>
<breadboardView>
<p layer='breadboardbreadboard' svgId='connector54pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector54pin' terminalId='connector54terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector54pad'/><p layer='copper1' svgId='connector54pad'/></pcbView>
</views>
</connector>
<connector id='connector55' type='female' name='RX'>
<description>RX</description><views>
<breadboardView>
<p layer='breadboardbreadboard' svgId='connector55pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector55pin' terminalId='connector55terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector55pad'/><p layer='copper1' svgId='connector55pad'/></pcbView>
</views>
</connector>
<connector id='connector56' type='female' name='5V'>
<description>5V</description><views>
<breadboardView>
<p layer='breadboardbreadboard' svgId='connector56pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector56pin' terminalId='connector56terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector56pad'/><p layer='copper1' svgId='connector56pad'/></pcbView>
</views>
</connector>
<connector id='connector57' type='female' name='GND'>
<description>GND</description><views>
<breadboardView>
<p layer='breadboardbreadboard' svgId='connector57pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector57pin' terminalId='connector57terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector57pad'/><p layer='copper1' svgId='connector57pad'/></pcbView>
</views>
</connector>
<connector id='connector58' type='female' name='GND'>
<description>GND</description><views>
<breadboardView>
<p layer='breadboardbreadboard' svgId='connector58pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector58pin' terminalId='connector58terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector58pad'/><p layer='copper1' svgId='connector58pad'/></pcbView>
</views>
</connector>
<connector id='connector59' type='female' name='5V'>
<description>5V</description><views>
<breadboardView>
<p layer='breadboardbreadboard' svgId='connector59pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector59pin' terminalId='connector59terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector59pad'/><p layer='copper1' svgId='connector59pad'/></pcbView>
</views>
</connector>
</connectors>
<buses>
<bus id='gnd'>
<nodeMember connectorId='connector28'/>
<nodeMember connectorId='connector38'/>
<nodeMember connectorId='connector57'/>
<nodeMember connectorId='connector58'/>
</bus>
<bus id='reset'>
<nodeMember connectorId='connector27'/>
<nodeMember connectorId='connector39'/>
<nodeMember connectorId='connector53'/>
</bus>
<bus id='tx'>
<nodeMember connectorId='connector25'/>
<nodeMember connectorId='connector54'/>
</bus>
<bus id='rx'>
<nodeMember connectorId='connector26'/>
<nodeMember connectorId='connector55'/>
</bus>
<bus id='+5v'>
<nodeMember connectorId='connector40'/>
<nodeMember connectorId='connector56'/>
<nodeMember connectorId='connector59'/>
</bus>
</buses>
</module>
