<?xml version="1.0" encoding="UTF-8"?>
<module fritzingVersion="0.4.0b.06.21.4282" moduleId="7segment56,9an">
    <version>4</version>
    <author>Stefan Hermann</author>
    <title>7 Segment Display</title>
    <label>7 Segment</label>
    <date>2011-08-4</date>
    <tags>
        <tag>fritzing core</tag>
        <tag>led</tag>
        <tag>display</tag>
        <tag>7</tag>
        <tag>segment</tag>
    </tags>



    <properties>
        <property name="family">Character Display</property>
        <property name="type">7 Segment</property>
        <property name="size">56,9 mm</property>
        <property name="common">anode</property>
    </properties>
    <description>7 Segment Display with common anode.</description>
    <views>
        <iconView>
            <layers image="icon/7segment.svg">
                <layer layerId="icon"/>
            </layers>
        </iconView>
        <breadboardView>
            <layers image="breadboard/7segment_56,9.svg">
                <layer layerId="breadboard"/>
            </layers>
        </breadboardView>
        <schematicView>
            <layers image="schematic/7segment_56,9_an.svg">
                <layer layerId="schematic"/>
            </layers>
        </schematicView>
        <pcbView>
            <layers image="pcb/7segment_56,9.svg">
                <layer layerId="copper0"/>
                <layer layerId="silkscreen"/>
                <layer layerId="copper1"/>
            </layers>
        </pcbView>
    </views>
    <connectors>

        <connector id="connector1" name="Segment E" type="male">
            <description>Segment E</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector1pin" terminalId="connector1terminal"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector1pin" terminalId="connector1terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper1" svgId="connector1pin"/>
                    <p layer="copper0" svgId="connector1pin"/>
                </pcbView>
            </views>
        </connector>

        <connector id="connector2" name="Segment D" type="male">
            <description>Segment D</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector2pin" terminalId="connector2terminal"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector2pin" terminalId="connector2terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper1" svgId="connector2pin"/>
                    <p layer="copper0" svgId="connector2pin"/>
                </pcbView>
            </views>
        </connector>

        <connector id="connector3" name="common anode" type="male">
            <description>common anode</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector3pin" terminalId="connector3terminal"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector3pin" terminalId="connector3terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper1" svgId="connector3pin"/>
                    <p layer="copper0" svgId="connector3pin"/>
                </pcbView>
            </views>
        </connector>

        <connector id="connector4" name="Segment C" type="male">
            <description>Segment C</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector4pin" terminalId="connector4terminal"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector4pin" terminalId="connector4terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper1" svgId="connector4pin"/>
                    <p layer="copper0" svgId="connector4pin"/>
                </pcbView>
            </views>
        </connector>

        <connector id="connector5" name="Segment DP" type="male">
            <description>Segment DP</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector5pin" terminalId="connector5terminal"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector5pin" terminalId="connector5terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper1" svgId="connector5pin"/>
                    <p layer="copper0" svgId="connector5pin"/>
                </pcbView>
            </views>
        </connector>

        <connector id="connector6" name="Segment B" type="male">
            <description>Segment B</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector6pin" terminalId="connector6terminal"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector6pin" terminalId="connector6terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper1" svgId="connector6pin"/>
                    <p layer="copper0" svgId="connector6pin"/>
                </pcbView>
            </views>
        </connector>

        <connector id="connector7" name="Segment A" type="male">
            <description>Segment A</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector7pin" terminalId="connector7terminal"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector7pin" terminalId="connector7terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper1" svgId="connector7pin"/>
                    <p layer="copper0" svgId="connector7pin"/>
                </pcbView>
            </views>
        </connector>

        <connector id="connector8" name="common anode" type="male">
            <description>common anode</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector8pin" terminalId="connector8terminal"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector8pin" terminalId="connector8terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper1" svgId="connector8pin"/>
                    <p layer="copper0" svgId="connector8pin"/>
                </pcbView>
            </views>
        </connector>

        <connector id="connector9" name="Segment F" type="male">
            <description>Segment F</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector9pin" terminalId="connector9terminal"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector9pin" terminalId="connector9terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper1" svgId="connector9pin"/>
                    <p layer="copper0" svgId="connector9pin"/>
                </pcbView>
            </views>
        </connector>

        <connector id="connector10" name="Segment G" type="male">
            <description>Segment G</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector10pin" terminalId="connector10terminal"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector10pin" terminalId="connector10terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper1" svgId="connector10pin"/>
                    <p layer="copper0" svgId="connector10pin"/>
                </pcbView>
            </views>
        </connector>
        
    </connectors>
    <buses>
      <bus id="anode">
       <nodeMember connectorId="connector3"/>
       <nodeMember connectorId="connector8"/>
      </bus>
    </buses>
</module>