<?xml version='1.0' encoding='UTF-8'?>
<module fritzingVersion="0.5.2b.02.18.4756" moduleId="intel-arduino_galileo_gen2" referenceFile="intel-arduino_galileo_gen2.fzp">
    <version>5</version>
    <date>11 24 2014</date>
    <author>Fabian Althaus</author>
    <description>Galileo is a microcontroller board based on the Intel&#174; Quark SoC X1000 Application Processor, a 32-bit Intel Pentium-class system on a chip (datasheet). It&#8217;s the first board based on Intel&#174; architecture designed to be hardware and software pin-compatible with Arduino shields designed for the Uno R3. Digital pins 0 to 13 (and the adjacent AREF and GND pins), Analog inputs 0 to 5, the power header, ICSP header, and the UART port pins (0 and 1), are all in the same locations as on the Arduino Uno R3. This is also known as the Arduino 1.0 pinout.
Galileo is designed to support shields that operate at either 3.3V or 5V. The core operating voltage of Galileo is 3.3V. However, a jumper on the board enables voltage translation to 5V at the I/O pins. This provides support for 5V Uno shields and is the default behavior. By switching the jumper position, the voltage translation can be disabled to provide 3.3V operation at the I/O pins.
Of course, the Galileo board is also software compatible with the Arduino Software Development Environment (IDE), which makes usability and introduction a snap. In addition to Arduino hardware and software compatibility, the Galileo board has several PC industry standard I/O ports and features to expand native usage and capabilities beyond the Arduino shield ecosystem. A full sized mini-PCI Express slot, 100Mb Ethernet port, Micro-SD slot, RS-232 serial port, USB Host port, USB Client port, and 8MByte NOR flash come standard on the board.
Visit the FAQ page for further informations.</description>
    <title>Intel Galileo Gen2</title>
    <url>http://arduino.cc/en/ArduinoCertified/IntelGalileo</url>
    <tags>
        <tag>revision 2</tag>
        <tag>x1000</tag>
        <tag>arduino</tag>
        <tag>32 bit</tag>
        <tag>pentium</tag>
        <tag>intel</tag>
        <tag>Quark SoC</tag>        
    </tags>
    
    <properties>
        <property name="family">microcontroller board (intel)</property>
        <property name="part number"/>
        <property name="type">Galileo gen2</property>
    </properties>
    <views>
        <breadboardView>
            <layers image="breadboard/intel-arduino-galileo_gen2_breadboard.svg">
                <layer layerId="breadboardbreadboard"/>
            </layers>
        </breadboardView>
        <schematicView>
            <layers image="schematic/intel-arduino-galileo_gen2_schematic.svg">
                <layer layerId="schematic"/>
            </layers>
        </schematicView>
        <pcbView>
            <layers image="pcb/intel-arduino-galileo_gen2_pcb.svg">
                <layer layerId="copper1"/>
                <layer layerId="silkscreen"/>
                <layer layerId="copper0"/>
            </layers>
        </pcbView>
        <iconView>
            <layers image="icon/intel-arduino-galileo_icon.svg">
                <layer layerId="icon"/>
            </layers>
        </iconView>
    </views>
    <connectors>
        <connector type="female" id="connector0" name="A0">
            <description>A0</description>
            <views>
                <breadboardView>
                    <p svgId="connector0pin" layer="breadboardbreadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector0pin" layer="schematic" terminalId="connector0terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector0pin" layer="copper0"/>
                    <p svgId="connector0pin" layer="copper1"/>
                </pcbView>
            </views>
        </connector>
        <connector type="female" id="connector1" name="A1">
            <description>A1</description>
            <views>
                <breadboardView>
                    <p svgId="connector1pin" layer="breadboardbreadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector1pin" layer="schematic" terminalId="connector1terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector1pin" layer="copper0"/>
                    <p svgId="connector1pin" layer="copper1"/>
                </pcbView>
            </views>
        </connector>
        <connector type="female" id="connector2" name="A2">
            <description>A2</description>
            <views>
                <breadboardView>
                    <p svgId="connector2pin" layer="breadboardbreadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector2pin" layer="schematic" terminalId="connector2terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector2pin" layer="copper0"/>
                    <p svgId="connector2pin" layer="copper1"/>
                </pcbView>
            </views>
        </connector>
        <connector type="female" id="connector3" name="A3">
            <description>A3</description>
            <views>
                <breadboardView>
                    <p svgId="connector3pin" layer="breadboardbreadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector3pin" layer="schematic" terminalId="connector3terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector3pin" layer="copper0"/>
                    <p svgId="connector3pin" layer="copper1"/>
                </pcbView>
            </views>
        </connector>
        <connector type="female" id="connector4" name="A4/SDA">
            <description>A4/SDA</description>
            <views>
                <breadboardView>
                    <p svgId="connector4pin" layer="breadboardbreadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector4pin" layer="schematic" terminalId="connector4terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector4pin" layer="copper0"/>
                    <p svgId="connector4pin" layer="copper1"/>
                </pcbView>
            </views>
        </connector>
        <connector type="female" id="connector5" name="A5/SCL">
            <description>A5/SCL</description>
            <views>
                <breadboardView>
                    <p svgId="connector5pin" layer="breadboardbreadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector5pin" layer="schematic" terminalId="connector5terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector5pin" layer="copper0"/>
                    <p svgId="connector5pin" layer="copper1"/>
                </pcbView>
            </views>
        </connector>
        <connector type="female" id="connector39" name="ICSP MISO">
            <description>ICSP MISO</description>
            <views>
                <breadboardView>
                    <p svgId="connector39pin" layer="unknown"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector39pin" layer="unknown" terminalId="connector39terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector39pin" layer="unknown"/>
                </pcbView>
            </views>
        </connector>
        <connector type="female" id="connector40" name="5V">
            <description>5V</description>
            <views>
                <breadboardView>
                    <p svgId="connector40pin" layer="unknown"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector40pin" layer="unknown" terminalId="connector40terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector40pin" layer="unknown"/>
                </pcbView>
            </views>
        </connector>
        <connector type="female" id="connector41" name="ICSP SCK">
            <description>ICSP SCK</description>
            <views>
                <breadboardView>
                    <p svgId="connector41pin" layer="unknown"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector41pin" layer="unknown" terminalId="connector41terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector41pin" layer="unknown"/>
                </pcbView>
            </views>
        </connector>
        <connector type="female" id="connector42" name="ICSP MOSI">
            <description>ICSP MOSI</description>
            <views>
                <breadboardView>
                    <p svgId="connector42pin" layer="unknown"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector42pin" layer="unknown" terminalId="connector42terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector42pin" layer="unknown"/>
                </pcbView>
            </views>
        </connector>
        <connector type="female" id="connector43" name="RESET">
            <description>RESET</description>
            <views>
                <breadboardView>
                    <p svgId="connector43pin" layer="unknown"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector43pin" layer="unknown" terminalId="connector43terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector43pin" layer="unknown"/>
                </pcbView>
            </views>
        </connector>
        <connector type="female" id="connector44" name="GND">
            <description>GND</description>
            <views>
                <breadboardView>
                    <p svgId="connector44pin" layer="unknown"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector44pin" layer="unknown" terminalId="connector44terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector44pin" layer="unknown"/>
                </pcbView>
            </views>
        </connector>
        <connector type="female" id="connector45" name="ICSP2 MISO">
            <description>ICSP2 MISO</description>
            <views>
                <breadboardView>
                    <p svgId="connector45pin" layer="unknown"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector45pin" layer="unknown" terminalId="connector45terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector45pin" layer="unknown"/>
                </pcbView>
            </views>
        </connector>
        <connector type="female" id="connector46" name="5V">
            <description>5V</description>
            <views>
                <breadboardView>
                    <p svgId="connector46pin" layer="unknown"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector46pin" layer="unknown" terminalId="connector46terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector46pin" layer="unknown"/>
                </pcbView>
            </views>
        </connector>
        <connector type="female" id="connector47" name="ICSP2 SCK">
            <description>ICSP2 SCK</description>
            <views>
                <breadboardView>
                    <p svgId="connector47pin" layer="unknown"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector47pin" layer="unknown" terminalId="connector47terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector47pin" layer="unknown"/>
                </pcbView>
            </views>
        </connector>
        <connector type="female" id="connector48" name="ICSP2 MOSI">
            <description>ICSP2 MOSI</description>
            <views>
                <breadboardView>
                    <p svgId="connector48pin" layer="unknown"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector48pin" layer="unknown" terminalId="connector48terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector48pin" layer="unknown"/>
                </pcbView>
            </views>
        </connector>
        <connector type="female" id="connector49" name="RESET2">
            <description>RESET2</description>
            <views>
                <breadboardView>
                    <p svgId="connector49pin" layer="unknown"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector49pin" layer="unknown" terminalId="connector49terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector49pin" layer="unknown"/>
                </pcbView>
            </views>
        </connector>
        <connector type="female" id="connector50" name="GND">
            <description>GND</description>
            <views>
                <breadboardView>
                    <p svgId="connector50pin" layer="unknown"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector50pin" layer="unknown" terminalId="connector50terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector50pin" layer="unknown"/>
                </pcbView>
            </views>
        </connector>
        <connector type="female" id="connector51" name="D8">
            <description>D8</description>
            <views>
                <breadboardView>
                    <p svgId="connector51pin" layer="breadboardbreadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector51pin" layer="schematic" terminalId="connector51terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector51pin" layer="copper0"/>
                    <p svgId="connector51pin" layer="copper1"/>
                </pcbView>
            </views>
        </connector>
        <connector type="female" id="connector52" name="D9 PWM">
            <description>D9 PWM</description>
            <views>
                <breadboardView>
                    <p svgId="connector52pin" layer="breadboardbreadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector52pin" layer="schematic" terminalId="connector52terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector52pin" layer="copper0"/>
                    <p svgId="connector52pin" layer="copper1"/>
                </pcbView>
            </views>
        </connector>
        <connector type="female" id="connector53" name="D10 PWM/SS">
            <description>D10 PWM/SS</description>
            <views>
                <breadboardView>
                    <p svgId="connector53pin" layer="breadboardbreadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector53pin" layer="schematic" terminalId="connector53terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector53pin" layer="copper0"/>
                    <p svgId="connector53pin" layer="copper1"/>
                </pcbView>
            </views>
        </connector>
        <connector type="female" id="connector54" name="D11 PWM/MOSI">
            <description>D11 PWM/MOSI</description>
            <views>
                <breadboardView>
                    <p svgId="connector54pin" layer="breadboardbreadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector54pin" layer="schematic" terminalId="connector54terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector54pin" layer="copper0"/>
                    <p svgId="connector54pin" layer="copper1"/>
                </pcbView>
            </views>
        </connector>
        <connector type="female" id="connector55" name="D12/MISO">
            <description>D12/MISO</description>
            <views>
                <breadboardView>
                    <p svgId="connector55pin" layer="breadboardbreadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector55pin" layer="schematic" terminalId="connector55terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector55pin" layer="copper0"/>
                    <p svgId="connector55pin" layer="copper1"/>
                </pcbView>
            </views>
        </connector>
        <connector type="female" id="connector56" name="D13/SCK">
            <description>D13/SCK</description>
            <views>
                <breadboardView>
                    <p svgId="connector56pin" layer="breadboardbreadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector56pin" layer="schematic" terminalId="connector56terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector56pin" layer="copper0"/>
                    <p svgId="connector56pin" layer="copper1"/>
                </pcbView>
            </views>
        </connector>
        <connector type="female" id="connector57" name="GND">
            <description>GND</description>
            <views>
                <breadboardView>
                    <p svgId="connector57pin" layer="breadboardbreadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector57pin" layer="schematic" terminalId="connector57terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector57pin" layer="copper0"/>
                    <p svgId="connector57pin" layer="copper1"/>
                </pcbView>
            </views>
        </connector>
        <connector type="female" id="connector58" name="AREF">
            <description>AREF</description>
            <views>
                <breadboardView>
                    <p svgId="connector58pin" layer="breadboardbreadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector58pin" layer="schematic" terminalId="connector58terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector58pin" layer="copper0"/>
                    <p svgId="connector58pin" layer="copper1"/>
                </pcbView>
            </views>
        </connector>
        <connector type="female" id="connector59" name="A4/SDA">
            <description>A4/SDA</description>
            <views>
                <breadboardView>
                    <p svgId="connector59pin" layer="breadboardbreadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector59pin" layer="schematic" terminalId="connector59terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector59pin" layer="copper0"/>
                    <p svgId="connector59pin" layer="copper1"/>
                </pcbView>
            </views>
        </connector>
        <connector type="female" id="connector60" name="A5/SCL">
            <description>A5/SCL</description>
            <views>
                <breadboardView>
                    <p svgId="connector60pin" layer="breadboardbreadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector60pin" layer="schematic" terminalId="connector60terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector60pin" layer="copper0"/>
                    <p svgId="connector60pin" layer="copper1"/>
                </pcbView>
            </views>
        </connector>
        <connector type="female" id="connector61" name="D0/RX">
            <description>D0/RX</description>
            <views>
                <breadboardView>
                    <p svgId="connector61pin" layer="breadboardbreadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector61pin" layer="schematic" terminalId="connector61terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector61pin" layer="copper0"/>
                    <p svgId="connector61pin" layer="copper1"/>
                </pcbView>
            </views>
        </connector>
        <connector type="female" id="connector62" name="D1/TX">
            <description>D1/TX</description>
            <views>
                <breadboardView>
                    <p svgId="connector62pin" layer="breadboardbreadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector62pin" layer="schematic" terminalId="connector62terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector62pin" layer="copper0"/>
                    <p svgId="connector62pin" layer="copper1"/>
                </pcbView>
            </views>
        </connector>
        <connector type="female" id="connector63" name="D2">
            <description>D2</description>
            <views>
                <breadboardView>
                    <p svgId="connector63pin" layer="breadboardbreadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector63pin" layer="schematic" terminalId="connector63terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector63pin" layer="copper0"/>
                    <p svgId="connector63pin" layer="copper1"/>
                </pcbView>
            </views>
        </connector>
        <connector type="female" id="connector64" name="D3 PWM">
            <description>D3 PWM</description>
            <views>
                <breadboardView>
                    <p svgId="connector64pin" layer="breadboardbreadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector64pin" layer="schematic" terminalId="connector64terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector64pin" layer="copper0"/>
                    <p svgId="connector64pin" layer="copper1"/>
                </pcbView>
            </views>
        </connector>
        <connector type="female" id="connector65" name="D4">
            <description>D4</description>
            <views>
                <breadboardView>
                    <p svgId="connector65pin" layer="breadboardbreadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector65pin" layer="schematic" terminalId="connector65terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector65pin" layer="copper0"/>
                    <p svgId="connector65pin" layer="copper1"/>
                </pcbView>
            </views>
        </connector>
        <connector type="female" id="connector66" name="D5 PWM">
            <description>D5 PWM</description>
            <views>
                <breadboardView>
                    <p svgId="connector66pin" layer="breadboardbreadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector66pin" layer="schematic" terminalId="connector66terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector66pin" layer="copper0"/>
                    <p svgId="connector66pin" layer="copper1"/>
                </pcbView>
            </views>
        </connector>
        <connector type="female" id="connector67" name="D6 PWM">
            <description>D6 PWM</description>
            <views>
                <breadboardView>
                    <p svgId="connector67pin" layer="breadboardbreadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector67pin" layer="schematic" terminalId="connector67terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector67pin" layer="copper0"/>
                    <p svgId="connector67pin" layer="copper1"/>
                </pcbView>
            </views>
        </connector>
        <connector type="female" id="connector68" name="D7">
            <description>D7</description>
            <views>
                <breadboardView>
                    <p svgId="connector68pin" layer="breadboardbreadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector68pin" layer="schematic" terminalId="connector68terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector68pin" layer="copper0"/>
                    <p svgId="connector68pin" layer="copper1"/>
                </pcbView>
            </views>
        </connector>
        <connector type="female" id="connector84" name="ioref">
            <description>IOREF</description>
            <views>
                <breadboardView>
                    <p svgId="connector84pin" layer="breadboardbreadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector84pin" layer="schematic" terminalId="connector84terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector84pin" layer="copper0"/>
                    <p svgId="connector84pin" layer="copper1"/>
                </pcbView>
            </views>
        </connector>
        <connector type="female" id="connector85" name="RESET">
            <description>RESET</description>
            <views>
                <breadboardView>
                    <p svgId="connector85pin" layer="breadboardbreadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector85pin" layer="schematic" terminalId="connector85terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector85pin" layer="copper0"/>
                    <p svgId="connector85pin" layer="copper1"/>
                </pcbView>
            </views>
        </connector>
        <connector type="female" id="connector86" name="3V3">
            <description>3V3</description>
            <views>
                <breadboardView>
                    <p svgId="connector86pin" layer="breadboardbreadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector86pin" layer="schematic" terminalId="connector86terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector86pin" layer="copper0"/>
                    <p svgId="connector86pin" layer="copper1"/>
                </pcbView>
            </views>
        </connector>
        <connector type="female" id="connector87" name="5V">
            <description>5V</description>
            <views>
                <breadboardView>
                    <p svgId="connector87pin" layer="breadboardbreadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector87pin" layer="schematic" terminalId="connector87terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector87pin" layer="copper0"/>
                    <p svgId="connector87pin" layer="copper1"/>
                </pcbView>
            </views>
        </connector>
        <connector type="female" id="connector88" name="GND">
            <description>GND</description>
            <views>
                <breadboardView>
                    <p svgId="connector88pin" layer="breadboardbreadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector88pin" layer="schematic" terminalId="connector88terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector88pin" layer="copper0"/>
                    <p svgId="connector88pin" layer="copper1"/>
                </pcbView>
            </views>
        </connector>
        <connector type="female" id="connector89" name="GND">
            <description>GND</description>
            <views>
                <breadboardView>
                    <p svgId="connector89pin" layer="breadboardbreadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector89pin" layer="schematic" terminalId="connector89terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector89pin" layer="copper0"/>
                    <p svgId="connector89pin" layer="copper1"/>
                </pcbView>
            </views>
        </connector>
        <connector type="female" id="connector90" name="VIN">
            <description>VIN</description>
            <views>
                <breadboardView>
                    <p svgId="connector90pin" layer="breadboardbreadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector90pin" layer="schematic" terminalId="connector90terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector90pin" layer="copper0"/>
                    <p svgId="connector90pin" layer="copper1"/>
                </pcbView>
            </views>
        </connector>
        <connector type="female" id="connector91" name="N/C">
            <description>not connected</description>
            <views>
                <breadboardView>
                    <p svgId="connector91pin" layer="breadboardbreadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector91pin" layer="schematic" terminalId="connector91terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector91pin" layer="copper0"/>
                    <p svgId="connector91pin" layer="copper1"/>
                </pcbView>
            </views>
        </connector>
	        <connector type="female" id="connector139" name="none">
            <description>none</description>
            <views>
                <breadboardView>
                    <p svgId="connector139pin" layer="breadboardbreadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector139pin" layer="schematic" terminalId="connector139terminal" hybrid="yes"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector139pin" layer="copper0" hybrid="yes"/>
                    <p svgId="connector139pin" layer="copper1" hybrid="yes"/>
                </pcbView>
            </views>
        </connector>
		        <connector type="female" id="connector140" name="none">
            <description>none</description>
            <views>
                <breadboardView>
                    <p svgId="connector140pin" layer="breadboardbreadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector140pin" layer="schematic" terminalId="connector140terminal" hybrid="yes"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector140pin" layer="copper0" hybrid="yes"/>
                    <p svgId="connector140pin" layer="copper1" hybrid="yes"/>
                </pcbView>
            </views>
        </connector>
	               <connector type="female" id="connector141" name="none">
            <description>none</description>
            <views>
                <breadboardView>
                    <p svgId="connector141pin" layer="breadboardbreadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector141pin" layer="schematic" terminalId="connector141terminal" hybrid="yes"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector141pin" layer="copper0" hybrid="yes"/>
                    <p svgId="connector141pin" layer="copper1" hybrid="yes"/>
                </pcbView>
            </views>
        </connector>
                        <connector type="female" id="connector142" name="none">
            <description>none</description>
            <views>
                <breadboardView>
                    <p svgId="connector142pin" layer="breadboardbreadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector142pin" layer="schematic" terminalId="connector142terminal" hybrid="yes"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector142pin" layer="copper0" hybrid="yes"/>
                    <p svgId="connector142pin" layer="copper1" hybrid="yes"/>
                </pcbView>
            </views>
        </connector>
                                <connector type="female" id="connector143" name="none">
            <description>none</description>
            <views>
                <breadboardView>
                    <p svgId="connector143pin" layer="breadboardbreadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector143pin" layer="schematic" terminalId="connector143terminal" hybrid="yes"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector143pin" layer="copper0" hybrid="yes"/>
                    <p svgId="connector143pin" layer="copper1" hybrid="yes"/>
                </pcbView>
            </views>
        </connector>
                                <connector type="female" id="connector144" name="none">
            <description>none</description>
            <views>
                <breadboardView>
                    <p svgId="connector144pin" layer="breadboardbreadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector144pin" layer="schematic" terminalId="connector144terminal" hybrid="yes"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector144pin" layer="copper0" hybrid="yes"/>
                    <p svgId="connector144pin" layer="copper1" hybrid="yes"/>
                </pcbView>
            </views>
        </connector>
                                        <connector type="female" id="connector145" name="none">
            <description>none</description>
            <views>
                <breadboardView>
                    <p svgId="connector145pin" layer="breadboardbreadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector145pin" layer="schematic" terminalId="connector145terminal" hybrid="yes"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector145pin" layer="copper0" hybrid="yes"/>
                    <p svgId="connector145pin" layer="copper1" hybrid="yes"/>
                </pcbView>
            </views>
        </connector>

                                                <connector type="female" id="connector120" name="none">
            <description>none</description>
            <views>
                <breadboardView>
                    <p svgId="connector120pin" layer="breadboardbreadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector120pin" layer="schematic" terminalId="connector120terminal" hybrid="yes"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector120pin" layer="copper0" hybrid="yes"/>
                    <p svgId="connector120pin" layer="copper1" hybrid="yes"/>
                </pcbView>
            </views>
        </connector>
                                                <connector type="female" id="connector121" name="none">
            <description>none</description>
            <views>
                <breadboardView>
                    <p svgId="connector121pin" layer="breadboardbreadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector121pin" layer="schematic" terminalId="connector121terminal" hybrid="yes"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector121pin" layer="copper0" hybrid="yes"/>
                    <p svgId="connector121pin" layer="copper1" hybrid="yes"/>
                </pcbView>
            </views>
        </connector>
                                        <connector type="female" id="connector122" name="none">
            <description>none</description>
            <views>
                <breadboardView>
                    <p svgId="connector122pin" layer="breadboardbreadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector122pin" layer="schematic" terminalId="connector122terminal" hybrid="yes"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector122pin" layer="copper0" hybrid="yes"/>
                    <p svgId="connector122pin" layer="copper1" hybrid="yes"/>
                </pcbView>
            </views>
        </connector>
                                        <connector type="female" id="connector130" name="coin +">
            <description>coin-cell positive (+)</description>
            <views>
                <breadboardView>
                    <p svgId="connector130pin" layer="breadboardbreadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector130pin" layer="schematic" terminalId="connector130terminal" hybrid="yes"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector130pin" layer="copper0" hybrid="yes"/>
                    <p svgId="connector130pin" layer="copper1" hybrid="yes"/>
                </pcbView>
            </views>
        </connector>
                                        <connector type="female" id="connector131" name="coin -">
            <description>coin-cell negative (-)</description>
            <views>
                <breadboardView>
                    <p svgId="connector131pin" layer="breadboardbreadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector131pin" layer="schematic" terminalId="connector131terminal" hybrid="yes"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector131pin" layer="copper0" hybrid="yes"/>
                    <p svgId="connector131pin" layer="copper1" hybrid="yes"/>
                </pcbView>
            </views>
        </connector>

              <connector type="female" id="connector100" name="jtag 2">
            <description>jtag 2 - tms</description>
            <views>
                <breadboardView>
                    <p svgId="connector100pin" layer="breadboardbreadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector100pin" layer="schematic" terminalId="connector100terminal" hybrid="yes"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector100pin" layer="copper0" hybrid="yes"/>
                    <p svgId="connector100pin" layer="copper1" hybrid="yes"/>
                </pcbView>
            </views>
        </connector>
                       <connector type="female" id="connector101" name="jtag 4">
            <description>jtag 4 - tclk</description>
            <views>
                <breadboardView>
                    <p svgId="connector101pin" layer="breadboardbreadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector101pin" layer="schematic" terminalId="connector101terminal" hybrid="yes"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector101pin" layer="copper0" hybrid="yes"/>
                    <p svgId="connector101pin" layer="copper1" hybrid="yes"/>
                </pcbView>
            </views>
        </connector>
                       <connector type="female" id="connector102" name="jtag 6">
            <description>jtag 6 - tdo</description>
            <views>
                <breadboardView>
                    <p svgId="connector102pin" layer="breadboardbreadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector102pin" layer="schematic" terminalId="connector102terminal" hybrid="yes"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector102pin" layer="copper0" hybrid="yes"/>
                    <p svgId="connector102pin" layer="copper1" hybrid="yes"/>
                </pcbView>
            </views>
        </connector>
                               <connector type="female" id="connector103" name="jtag 8">
            <description>jtag 8 - tdi</description>
            <views>
                <breadboardView>
                    <p svgId="connector103pin" layer="breadboardbreadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector103pin" layer="schematic" terminalId="connector103terminal" hybrid="yes"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector103pin" layer="copper0" hybrid="yes"/>
                    <p svgId="connector103pin" layer="copper1" hybrid="yes"/>
                </pcbView>
            </views>
        </connector>
                               <connector type="female" id="connector104" name="jtag 10">
            <description>jtag 10 - reset</description>
            <views>
                <breadboardView>
                    <p svgId="connector104pin" layer="breadboardbreadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector104pin" layer="schematic" terminalId="connector104terminal" hybrid="yes"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector104pin" layer="copper0" hybrid="yes"/>
                    <p svgId="connector104pin" layer="copper1" hybrid="yes"/>
                </pcbView>
            </views>
        </connector>

                               <connector type="female" id="connector105" name="jtag 1">
            <description>jtag 1 - vcc</description>
            <views>
                <breadboardView>
                    <p svgId="connector105pin" layer="breadboardbreadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector105pin" layer="schematic" terminalId="connector105terminal" hybrid="yes"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector105pin" layer="copper0" hybrid="yes"/>
                    <p svgId="connector105pin" layer="copper1" hybrid="yes"/>
                </pcbView>
            </views>
        </connector>

                               <connector type="female" id="connector106" name="jtag 3">
            <description>jtag 3 - gnd</description>
            <views>
                <breadboardView>
                    <p svgId="connector106pin" layer="breadboardbreadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector106pin" layer="schematic" terminalId="connector106terminal" hybrid="yes"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector106pin" layer="copper0" hybrid="yes"/>
                    <p svgId="connector106pin" layer="copper1" hybrid="yes"/>
                </pcbView>
            </views>
        </connector>

                               <connector type="female" id="connector107" name="jtag 5">
            <description>jtag 5 - gnd</description>
            <views>
                <breadboardView>
                    <p svgId="connector107pin" layer="breadboardbreadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector107pin" layer="schematic" terminalId="connector107terminal" hybrid="yes"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector107pin" layer="copper0" hybrid="yes"/>
                    <p svgId="connector107pin" layer="copper1" hybrid="yes"/>
                </pcbView>
            </views>
        </connector>

                               <connector type="female" id="connector108" name="jtag 7">
            <description>jtag 7 - rtck</description>
            <views>
                <breadboardView>
                    <p svgId="connector108pin" layer="breadboardbreadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector108pin" layer="schematic" terminalId="connector108terminal" hybrid="yes"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector108pin" layer="copper0" hybrid="yes"/>
                    <p svgId="connector108pin" layer="copper1" hybrid="yes"/>
                </pcbView>
            </views>
        </connector>

                               <connector type="female" id="connector109" name="jtag 9">
            <description>jtag 9 - gnd</description>
            <views>
                <breadboardView>
                    <p svgId="connector109pin" layer="breadboardbreadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector109pin" layer="schematic" terminalId="connector109terminal" hybrid="yes"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector109pin" layer="copper0" hybrid="yes"/>
                    <p svgId="connector109pin" layer="copper1" hybrid="yes"/>
                </pcbView>
            </views>
        </connector>

                               <connector type="female" id="connector160" name="ioref 1">
            <description>ioref 1 - 5V</description>
            <views>
                <breadboardView>
                    <p svgId="connector160pin" layer="breadboardbreadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector160pin" layer="schematic" terminalId="connector160terminal" hybrid="yes"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector160pin" layer="copper0" hybrid="yes"/>
                    <p svgId="connector160pin" layer="copper1" hybrid="yes"/>
                </pcbView>
            </views>
        </connector>

                               <connector type="female" id="connector161" name="ioref 2">
            <description>ioref 2</description>
            <views>
                <breadboardView>
                    <p svgId="connector161pin" layer="breadboardbreadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector161pin" layer="schematic" terminalId="connector161terminal" hybrid="yes"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector161pin" layer="copper0" hybrid="yes"/>
                    <p svgId="connector161pin" layer="copper1" hybrid="yes"/>
                </pcbView>
            </views>
        </connector>

                               <connector type="female" id="connector162" name="ioref 3">
            <description>ioref 3 - 3.3V</description>
            <views>
                <breadboardView>
                    <p svgId="connector162pin" layer="breadboardbreadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector162pin" layer="schematic" terminalId="connector162terminal" hybrid="yes"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector162pin" layer="copper0" hybrid="yes"/>
                    <p svgId="connector162pin" layer="copper1" hybrid="yes"/>
                </pcbView>
            </views>
        </connector>
                           <connector type="female" id="connector150" name="vin-2">
            <description>vin-2 - 5V</description>
            <views>
                <breadboardView>
                    <p svgId="connector150pin" layer="breadboardbreadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector150pin" layer="schematic" terminalId="connector150terminal" hybrid="yes"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector150pin" layer="copper0" hybrid="yes"/>
                    <p svgId="connector150pin" layer="copper1" hybrid="yes"/>
                </pcbView>
            </views>
        </connector>
 <connector type="female" id="connector151" name="vin-1">
            <description>vin-1 - vin</description>
            <views>
                <breadboardView>
                    <p svgId="connector151pin" layer="breadboardbreadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector151pin" layer="schematic" terminalId="connector151terminal" hybrid="yes"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector151pin" layer="copper0" hybrid='yes'/>
                    <p svgId="connector151pin" layer="copper1" hybrid="yes"/>
                </pcbView>
            </views>
        </connector>
    </connectors>
    <buses>
        <bus id="+5v">
            <nodeMember connectorId="connector40"/>
            <nodeMember connectorId="connector46"/>
            <nodeMember connectorId="connector87"/>
        </bus>
        <bus id="gnd">
            <nodeMember connectorId="connector44"/>
            <nodeMember connectorId="connector50"/>
            <nodeMember connectorId="connector57"/>
            <nodeMember connectorId="connector88"/>
            <nodeMember connectorId="connector89"/>
        </bus>
        <bus id="mosi">
            <nodeMember connectorId="connector42"/>
            <nodeMember connectorId="connector54"/>
        </bus>
        <bus id="miso">
            <nodeMember connectorId="connector39"/>
            <nodeMember connectorId="connector55"/>
        </bus>
        <bus id="sck">
            <nodeMember connectorId="connector41"/>
            <nodeMember connectorId="connector56"/>
        </bus>
        <bus id="ad4/sda">
            <nodeMember connectorId="connector4"/>
            <nodeMember connectorId="connector59"/>
        </bus>
        <bus id="ad5/scl">
            <nodeMember connectorId="connector5"/>
            <nodeMember connectorId="connector60"/>
        </bus>
        <bus id="reset">
            <nodeMember connectorId="connector43"/>
            <nodeMember connectorId="connector85"/>
        </bus>
    </buses>
</module>
