<?xml version="1.0" encoding="UTF-8"?><module fritzingVersion="0.7.2b" moduleId="SparkFun-Connectors-USB--MB-H">
<!-- generated from Sparkfun Eagle Library 'SparkFun-Connectors' USB -MB-H -->
<version>4</version>
<date>2013-02-13</date>
<label>X</label>
<author>www.fritzing.org</author>
<description>&lt;b&gt;USB Connectors&lt;/b&gt;
&lt;p&gt;USB-B-PTH is fully proven SKU : PRT-00139
&lt;p&gt;USB-miniB is fully proven SKU : PRT-00587
&lt;p&gt;USB-A-PCB is untested.
&lt;p&gt;USB-A-H is throughly reviewed, but untested. Spark Fun Electronics SKU : PRT-00437
&lt;p&gt;USB-B-SMT is throughly reviewed, but untested. Needs silkscreen touching up.
&lt;p&gt;USB-A-S has not been used/tested
&lt;p&gt;USB-MB-H has not been used/tested</description>
<title>USB Connectors</title>
<tags>
<tag>USB</tag>
<tag>USB-MB-H</tag>
<tag>-MB-H</tag>
</tags>
<properties>
<property name="package">usb-mb-h</property>
<property name="target">USB-B</property>
<property name="family">sparkfun USB Connector</property>
<property name="variant">-mb-h</property>
</properties>
<views>
<breadboardView>
<layers image="breadboard/sparkfun-connectors_usb-mb-h_breadboard.svg">
<layer layerId="breadboard"/>
</layers>
</breadboardView>
<schematicView>
<layers image="schematic/sparkfun-connectors_usb_schematic.svg">
<layer layerId="schematic"/>
</layers>
</schematicView>
<pcbView>
<layers image="pcb/sparkfun-connectors_usb-mb-h_pcb.svg">
<layer layerId="copper1"/>
<layer layerId="silkscreen"/>
<layer layerId="copper0"/>
</layers>
</pcbView>
<iconView>
<layers image="icon/USB-MB-H.svg">
<layer layerId="icon"/>
</layers>
</iconView>
</views>
<connectors>
<connector id="connector2" name="D+" type="male">
<description>D+</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector2pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector3pin" terminalId="connector3terminal"/>
</schematicView>
<pcbView>
<p layer="copper0" svgId="connector2pad"/>
<p layer="copper1" svgId="connector2pad"/>
</pcbView>
</views>
</connector>
<connector id="connector3" name="D-" type="male">
<description>D-</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector3pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector2pin" terminalId="connector2terminal"/>
</schematicView>
<pcbView>
<p layer="copper0" svgId="connector3pad"/>
<p layer="copper1" svgId="connector3pad"/>
</pcbView>
</views>
</connector>
<connector id="connector4" name="GND" type="male">
<description>GND</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector4pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector5pin" terminalId="connector5terminal"/>
</schematicView>
<pcbView>
<p layer="copper0" svgId="connector4pad"/>
<p layer="copper1" svgId="connector4pad"/>
</pcbView>
</views>
</connector>
<connector id="connector6" name="VBUS" type="male">
<description>VBUS</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector6pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector4pin" terminalId="connector4terminal"/>
</schematicView>
<pcbView>
<p layer="copper0" svgId="connector6pad"/>
<p layer="copper1" svgId="connector6pad"/>
</pcbView>
</views>
</connector>
</connectors>
<buses>
</buses>
</module>