{
	"cpu":[
		"IERR",
		"Thermal Trip",
		"Upper Critical going high"
	],
	"Memory":[
		"Uncorrectable ECC",
		"Train",
		"Device Disabled"
	],
	"Power":[
		"Failure detected",
		"AC lost"
	],
	"voltage":[
		"Upper Critical going high",
		"Upper Non_recoverable going high",
		"Lower Critical going low",
		"Lower Non_recoverable going low"
	],
	"hdd":[
		"Predictive Failure"
	],
	"fan":[
		"Lower Critical going low"
	],
	"pcie":[
		"Bus Uncorrectable",
		"Bus Fatal"
	],
	"ME_FW_Status":[
		"Controller acces",
		"Management controller"
	],
	"OS":[
		"Run_time critical stop"
	]
}