{
	"cpu":[
		"Throttled",
		"Upper Non_critical going high"
	],
	"Memory":[
		"Correctable ECC"
	],
	"throttled":[
		"Memory MEM_AB_Hot",
		"Memory MEM_CD_Hot",
		"Memory MEM_EF_Hot",
		"Memory MEM_GH_Hot"
	],
	"Power":[
		"Predictive failure"
	],
	"voltage":[
		"Upper Non_critical going high",
		"Lower Non_critical going low"
	],
	"pcie":[
		"Bus Timeout",
		"PCI PERR",
		"PCI SERR"
	],
	"IPMI_Watchdog":[
		"Timer expired",
		"Hard Reset",
		"Power Down",
		"Power Cycle"
	],
	"EventLog":[
		"Log almost full"
	],
	"ME_FW_Status":[
		"Sensor access",
		"FRU Failure"
	]
}