
          DigitalChina DCN-530TX Fast Ethernet Adapter
         NDIS/2 DOS Driver For LAN Manager Installation
           
  Contents:
  ---------
  (A) NDIS 2 Driver Installation on LAN Manager v2.0
  (B) NDIS 2 Driver Installation on LAN Manager v2.1
  (C) NDIS 2 Driver Installation on LAN Manager v2.2
  
(A) NDIS 2 Driver Installation on LAN Manager v2.0
================================================================

  1. Type "Setup" in the LAN Manager directory and press Enter.

  2. Choose "Import Network Drivers..." in the "Action" field.
     Press <Enter> to continue.

  3. Insert your Driver Diskette. Then press <Enter> to see the
     list of Imported Network Drivers on the screen.

  4. Press the <Space> Bar to select the appropriate Network
     Adapter:"DigitalChina DCN-530TX Fast Ethernet Adapter", 
     then press <Enter> to confirm your choice.

  5. Follow screen instructions to complete the process, until
     the Network Driver appears on screen.

  6. Identify your Network Adapter if asked. For example, select
     "DigitalChina DCN-530TX Fast Ethernet Adapter" to confirm.

  7. Select the <Add driver> and the <Add protocol> options.
     Then select <OK> to confirm your choices. The Workstation's
     primary parameters should appear on screen.

  8. Respond to all prompts issued on screen to complete the
     process. Select <OK> to confirm a choice.

  9. Save all selections. Choose "Save" from the "Action Menu".

 10. Press <F3> to exit.


(B) NDIS 2 Driver Installation on LAN Manager v2.1
================================================================

  1. Type "lmsetup" in the LAN Manager directory and press
     <Enter>. The Microsoft LAN Manager Setup screen should
     appear.

  2. Choose "Network Drivers..." in the "Configuration" field.
     Press <Enter> to confirm your choice.

  3. Choose <Add New Configs> and press <Enter> to display a
     list of Network Adapter Drivers.

  4. Choose <Other Driver> and press <Enter>.

  5. Insert the Driver Diskette. Indicate the drive location 
     of the diskette and select <OK> to proceed.

  6. Select "DigitalChina DCN-530TX Fast Ethernet Adapter",
     and Select <OK> to confirm your choice.

  7. Select an appropriate protocol. Use the <Space> bar to
     highlight your choice.

  8. Select <OK> to confirm your choice. A Configuration
     Complete message should appear on screen.

  9. Save the configuration. Select <Save>.

 10. Press <F3> to exit.



(C) NDIS 2 Driver Installation on LAN Manager v2.2
================================================================

  1. Type "Setup" in the LAN Manager directory
     (i.e. C:\LANMAN.DOS) and press <Enter>. The Microsoft LAN
     Manager Setup screen should appear.

  2. Choose "Network Drivers" from the "Configuration" field.
     Press <Enter> to confirm your choice.

  3. Choose <Add New Config> and press <Enter> to display a list
     of Network Adapter Drivers.

  4. Insert the Driver Diskette. Indicate the drive location of
     the diskette.

  5. Choose <Other Driver> and press <Enter>.

  6. Select "DigitalChina DCN-530TX Fast Ethernet Adapter",
     and select <OK> to confirm your choice.

  7. Select an appropriate protocol. Use the <Space bar> to
     highlight your choice. If you have chosen the TCP/IP
     protocol, you will be prompted to key in the IP address,
     the subnet mask, and the default gateway(router). By
     default, the workstation number of the NetBios session is
     set to 6. Please consult Microsoft LAN Manager Installation
     Manual for more details, or check the online help.

  8. Select <OK> to confirm your choice. A Configuration
     Complete message should appear onscreen.

  9. Save the configuration. Select <Save>.

 10. Press <F3> to exit.


Sample Configuration Files
==========================

LAN Manager 2.0

  CONFIG.SYS File

      LASTDRIVE=Z
      BUFFERS = 35
      FILES = 35
      SHELL=C:\DOS50\COMMAND.COM C:\DOS50 /p /E:1024
      DEVICE=C:\HIMEM.SYS
      DEVICE=C:\DOS50\SETVER.EXE
      DOS=HIGH,UMB
      DEVICE=C:\LANMAN.DOS\DRIVERS\PROTMAN\PROTMAN.DOS /i:C:\LANMAN.DOS
      DEVICE=C:\LANMAN.DOS\DRIVERS\DC\DCNND2\DCNND2.DOS
      DEVICE=C:\LANMAN.DOS\DRIVERS\PROTOCOL\NETBEUI\NETBEUI.DOS

  PROTOCOL.INI File

      [PROTOCOL MANAGER]
       DRIVERNAME = PROTMAN$
      [NETBEUI_XIF]
       Drivername = netbeui$
       BINDINGS = "DCNND2_NIF"
      [DCNND2_NIF]
     ;----------------------------------------------------------------------
     ; Sample Protocol.ini file for DCNND2 NDIS 2 driver
     ;----------------------------------------------------------------------
       DriverName = DCNND2$
     ; Slot = 1            ;; {1-4}
     ; MEDIA = AUTODETECT
     ;; {MEDIA = UTP, UTP_FD, UTP_100,UTP_100FD, AUTODETECT}
     ;----------------------------------------------------------------------
     ; End of this sample file

  AUTOEXEC.BAT File

        @echo off
        PROMPT $P$G
        PATH=c:\PE2;C:\DOS50;C:\NC;
        APPEND=C:\PE2;C:\DOS50;
        REM ====== LANMAN 2.0 === DO NOT MODIFY BETWEEN THESE LINES
        SET PATH=C:\LANMAN.DOS\NETPROG;%PATH%
        C:\LANMAN.DOS\DRIVERS\PROTMAN\NETBIND
        NET START WORKSTATION
        REM ====== LANMAN 2.0 === DO NOT MODIFY BETWEEN THESE LINES

LAN Manager 2.1 or LAN Manager 2.2

  CONFIG.SYS File

        LASTDRIVE=Z
        BUFFERS = 35
        FILES = 35
        SHELL=C:\DOS62\COMMAND.COM C:\DOS62 /p /E:1024
        DEVICE=C:\HIMEM.SYS
        REM DEVICE=C:\LANMAN.DOS\DRIVERS\DOSUTILS\EMM386.EXE NoEMS ;;delete
                                                                   ;;this
                                                                   ;;line
        DEVICE=C:\DOS62\SETVER.EXE
        DOS=HIGH,UMB
        DEVICE=C:\LANMAN.DOS\DRIVERS\PROTMAN\PROTMAN.DOS /i:C:\LANMAN.DOS
        DEVICE=C:\LANMAN.DOS\DRIVERS\DC\DCNND2\DCNND2.DOS

  PROTOCOL.INI File

        [PROTMAN]
         DRIVERNAME = PROTMAN$
         DYNAMIC = YES
         PRIORITY = NETBEUI
        [NETBEUI_XIF]
         Drivername = netbeui$
         SESSIONS = 6
         NCBS = 12
         BINDINGS = "DCNND2_NIF"
         LANABASE = 0

        [DCNND2_NIF]
        ;-------------------------------------------------------------------
        ; Sample Protocol.ini file for DCNND2 NDIS 2 driver
        ;-------------------------------------------------------------------
          DriverName = DCNND2$
        ; Slot = 1            ;; {1-4}
        ; MEDIA = AUTODETECT
        ;; {MEDIA = UTP, UTP_FD, UTP_100,UTP_100FD, AUTODETECT}
        ;-------------------------------------------------------------------
        ; End of this sample file

  AUTOEXEC.BAT File

        @echo off
        PROMPT $P$G
        PATH=c:\PE2;C:\DOS62;C:\NC;
        APPEND=C:\PE2;C:\DOS62;
        @REM ====== LANMAN 2.1 === DO NOT MODIFY BETWEEN THESE LINES
        @REM=== LANMAN 2.1 ===
        SET PATH=C:\LANMAN.DOS\NETPROG;%PATH%
        NET START WORKSTATION
        LOAD NETBEUI
        @REM ====== LANMAN 2.1 === DO NOT MODIFY BETWEEN THESE LINES
        @REM === LANMAN 2.1 ===
