; Windows Modem Setup File	
; Copyright (c) 1993-1999 Microsoft Corporation \\MS-IRL\\
; Manufacturer: Dr. Neuhaus Telekommunikation GmbH 

[Version]
Signature="$WINDOWS NT$"
Class=Modem
ClassGUID={4D36E96D-E325-11CE-BFC1-08002BE10318}
Provider=%MSFT%
LayoutFile=layout.inf
DriverVer=07/01/2001,5.1.2535.0

[ControlFlags]
ExcludeFromSelect=*


[Manufacturer]
%Neuhaus% = Neuhaus
%Siemens% = Siemens
[Neuhaus]
%Modem9%  = Modem9, PCMCIA\Modem-CARD_DNT_1186-8DAE 		 ; Modem CARD 33.6 VOICE V.34+ POTS (only pots)

[Siemens]
%Modem10%  = Modem7,PCMCIA\GSM-DSA_Card-619C

[Modem7]        ; GIPSY CARD 9.6 PCMCIA 
DriverVer=05/23/1999
AddReg=All, MfgNeuhaus, PCMCIA, VerboseResultCodes, Modem7.AddReg

[Modem9]      ; Modem CARD 33.6 PCMCIA /POTS /VOICE
DriverVer=05/23/1999
AddReg=All, MfgAttReg, PCMCIA, VerboseResultCodes, Neuhaus_IMAVoice, Modem9.AddReg

[Modem7.AddReg] ; GIPSY CARD 9.6 PCMCIA V.32bis FAX+DATA only GSM
HKR,, Properties, 1, 00,00,00,00, 5a,00,00,00, 5a,00,00,00, 00,00,00,00, 00,00,00,00, 37,02,00,00, 00,c2,01,00, 80,25,00,00
HKR, Init,      2,, "AT&FE0V1&D2&C1Q0S0=0<cr>"
HKR, Settings, ErrorControl_On,, "\N3"
HKR, Settings, ErrorControl_Forced,, "\N2"

[Modem9.AddReg] ; Modem CARD 33.6 PCMCIA /POTS V.34+ DATA+FAX(1,2)+VOICE
HKR,, Properties, 1, 00,01,00,00, 5A,00,00,00, 5A,00,00,00, 00,00,00,00, 0F,00,00,00, 37,03,00,00, 00,C2,01,00, 40,83,00,00
HKR,,PowerDelay,0x10001,2000
HKR,,ConfigDelay,0x10001,2000 
HKR, Init,      2,, "AT&FE0V1&D2&C1Q0S0=0<cr>"

[Strings]
MSFT = "Microsoft"
Neuhaus = "Dr. Neuhaus"
Siemens = "Siemens"

Modem7= "Dr. Neuhaus GIPSY CARD PCMCIA V.32 GSM"
Modem9= "Dr. Neuhaus 33.6 VOICE (only analog)"          ; pots DUO
Modem10= "Siemens DSA GSM Card"

[All]
HKR,,FriendlyDriver,,unimodem.vxd
HKR,,DevLoader,,*vcomm
HKR,,PortSubClass,1,02
HKR,,ConfigDialog,,modemui.dll
HKR,,EnumPropPages,,"modemui.dll,EnumPropPages"
HKR, Init,      1,, "AT<cr>"
HKR, Responses, "<cr><lf>OK<cr><lf>",          1, 00, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>ERROR<cr><lf>",       1, 03, 00, 00,00,00,00, 00,00,00,00

[EXTERNAL]
HKR,, DeviceType, 1, 01
[PCMCIA]
HKR,,PortDriver,,Serial.vxd
HKR,,Contention,,*vcd
HKR,, DeviceType, 1, 03
[MfgNeuhaus]
HKR,, PowerDelay,  0x10001, 1500
HKR,, ConfigDelay, 0x10001, 1500
HKR,, InactivityScale, 1, 3c,00,00,00
HKR, Init,      2,, "AT&FE0V1&D2&C1W2Q0S0=0<cr>"
HKR, Init,      3,, "AT+FCLASS=0<cr>"
HKR, Monitor,   1,, "ATS0=0<cr>"
HKR, Monitor,   2,, "None"
HKR, Hangup,    1,, "ATH<cr>"
HKR, Answer,    1,, "ATA<cr>"
HKR,, Reset,, "AT&F<cr>"
HKR, Settings, Prefix,, "AT"
HKR, Settings, Terminator,, "<cr>"
HKR, Settings, DialPrefix,, "D"
HKR, Settings, SpeakerMode_Off,, "M0"
HKR, Settings, SpeakerMode_Dial,, "M1"
HKR, Settings, SpeakerMode_On,, "M2"
HKR, Settings, SpeakerMode_Setup,, "M3"
HKR, Settings, FlowControl_Off,, "\Q0"
HKR, Settings, FlowControl_Hard,, "\Q3"
HKR, Settings, FlowControl_Soft,, "\Q1"
HKR, Settings, ErrorControl_On,, "\N6"
HKR, Settings, ErrorControl_Off,, "\N0"
HKR, Settings, ErrorControl_Forced,, "\N5"
HKR, Settings, Compression_On,, "%%C1"
HKR, Settings, Compression_Off,, "%%C0"
HKR, Settings, Modulation_CCITT,, "B99"		;Multistandard
HKR, Settings, Modulation_Bell,,  "B90"   ;BELL 212
HKR, Settings, Modulation_CCITT_V23,, "B18"	;V.23
HKR, Settings, Pulse,, "P"
HKR, Settings, Tone,, "T"
HKR, Settings, Blind_Off,, "X4"
HKR, Settings, Blind_On,, "X3"
HKR, Settings, CallSetupFailTimer,, "S7=<#>"
HKR, Settings, InactivityTimeout,, "\T<#>"
HKR, Settings, DialSuffix,,           ""

[VerboseResultCodes]
HKR, Responses, "0<cr>",       1, 00, 00, 00,00,00,00, 00,00,00,00 ; OK
HKR, Responses, "2<cr>",       1, 08, 00, 00,00,00,00, 00,00,00,00 ; RING
HKR, Responses, "3<cr>",       1, 04, 00, 00,00,00,00, 00,00,00,00 ; NO CARRIER
HKR, Responses, "4<cr>",       1, 03, 00, 00,00,00,00, 00,00,00,00 ; ERROR
HKR, Responses, "6<cr>",       1, 05, 00, 00,00,00,00, 00,00,00,00 ; NO DIALTONE
HKR, Responses, "7<cr>",       1, 06, 00, 00,00,00,00, 00,00,00,00 ; BUSY
HKR, Responses, "8<cr>",       1, 07, 00, 00,00,00,00, 00,00,00,00 ; NO ANSWER

HKR, Responses, "<cr><lf>RING<cr><lf>",        1, 08, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>NO CARRIER<cr><lf>",  1, 04, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>FAX<cr><lf>",         1, 03, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>DATA<cr><lf>",        1, 03, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>VOICE<cr><lf>",       1, 03, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>NO DIALTONE<cr><lf>", 1, 05, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>BUSY<cr><lf>",        1, 06, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>NO ANSWER<cr><lf>",   1, 07, 00, 00,00,00,00, 00,00,00,00

HKR, Responses, "<cr><lf>CONNECT<cr><lf>",            1, 02, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 75/1200<cr><lf>",    1, 02, 00, b0,04,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 1200/75<cr><lf>",    1, 02, 00, b0,04,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 1200<cr><lf>",       1, 02, 00, b0,04,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 2400<cr><lf>",       1, 02, 00, 60,09,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 4800<cr><lf>",       1, 02, 00, c0,12,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 7200<cr><lf>",       1, 02, 00, 20,1c,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 9600<cr><lf>",       1, 02, 00, 80,25,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 12000<cr><lf>",      1, 02, 00, e0,2e,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 14400<cr><lf>",      1, 02, 00, 40,38,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 16800<cr><lf>",      1, 02, 00, a0,41,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 19200<cr><lf>",      1, 02, 00, 00,4b,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 21600<cr><lf>",      1, 02, 00, 60,54,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 24000<cr><lf>",      1, 02, 00, c0,5d,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 26400<cr><lf>",      1, 02, 00, 20,67,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 28800<cr><lf>",      1, 02, 00, 80,70,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 31200<cr><lf>",      1, 02, 00, E0,79,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 33600<cr><lf>",      1, 02, 00, 40,83,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 38400<cr><lf>",      1, 02, 00, 00,96,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 57600<cr><lf>",      1, 02, 00, 00,e1,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 115200<cr><lf>",     1, 02, 00, 00,c2,01,00, 00,00,00,00

HKR, Responses, "<cr><lf>CONNECT V.21/REL<cr><lf>",   1, 02, 02, 2c,01,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 300/REL<cr><lf>",    1, 02, 02, 2c,01,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 1200/REL<cr><lf>",   1, 02, 02, b0,04,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 2400/REL<cr><lf>",   1, 02, 02, 60,09,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 4800/REL<cr><lf>",   1, 02, 02, c0,12,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 7200/REL<cr><lf>",   1, 02, 02, 20,1c,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 9600/REL<cr><lf>",   1, 02, 02, 80,25,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 12000/REL<cr><lf>",  1, 02, 02, e0,2e,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 14400/REL<cr><lf>",  1, 02, 02, 40,38,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 16800/REL<cr><lf>",  1, 02, 02, a0,41,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 19200/REL<cr><lf>",  1, 02, 02, 00,4b,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 21600/REL<cr><lf>",  1, 02, 02, 60,54,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 24000/REL<cr><lf>",  1, 02, 02, c0,5d,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 26400/REL<cr><lf>",  1, 02, 02, 20,67,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 28800/REL<cr><lf>",  1, 02, 02, 80,70,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 31200/REL<cr><lf>",  1, 02, 02, E0,79,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 33600/REL<cr><lf>",  1, 02, 02, 40,83,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 38400/REL<cr><lf>",  1, 02, 02, 00,96,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 57600/REL<cr><lf>",  1, 02, 02, 00,e1,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 115200/REL<cr><lf>", 1, 02, 02, 00,c2,01,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 2400/RLP<cr><lf>",   1, 02, 02, 60,09,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 4800/RLP<cr><lf>",   1, 02, 02, c0,12,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 9600/RLP<cr><lf>",   1, 02, 02, 80,25,00,00, 00,00,00,00
[MfgAttReg]
HKR,, InactivityScale, 1, 3c,00,00,00
HKR, Init,      2,, "AT&FE0V1&D2&C1W2Q0S0=0<cr>"
HKR, Init,      3,, "AT+FCLASS=0<cr>"
HKR, Monitor,   1,, "ATS0=0<cr>"
HKR, Monitor,   2,, "None"
HKR, Hangup,    1,, "ATH<cr>"
HKR, Answer,    1,, "ATA<cr>"
HKR,, Reset,, "AT&F<cr>"
HKR, Settings, Prefix,, "AT"
HKR, Settings, DialSuffix,, ""
HKR, Settings, Terminator,, "<cr>"
HKR, Settings, DialPrefix,, "D"
HKR, Settings, SpeakerMode_Off,, "M0"
HKR, Settings, SpeakerMode_Dial,, "M1"
HKR, Settings, SpeakerMode_On,, "M2"
HKR, Settings, SpeakerMode_Setup,, "M3"
HKR, Settings, FlowControl_Off,, "\Q0"
HKR, Settings, FlowControl_Hard,, "\Q3"
HKR, Settings, FlowControl_Soft,, "\Q1"
HKR, Settings, ErrorControl_On,, "\N6"
HKR, Settings, ErrorControl_Off,, "\N0"
HKR, Settings, ErrorControl_Forced,, "\N5"
HKR, Settings, Compression_On,, "%%C1"
HKR, Settings, Compression_Off,, "%%C0"
HKR, Settings, Pulse,, "P"
HKR, Settings, Tone,, "T"
HKR, Settings, Blind_Off,, "X4"
HKR, Settings, Blind_On,, "X3"
HKR, Settings, CallSetupFailTimer,, "S7=<#>"
HKR, Settings, InactivityTimeout,, "\T<#>"
[Neuhaus_IMAVoice]
HKR, WaveDriver,  BaudRate       ,1, 00, c2, 01, 00
HKR, WaveDriver,  XformID        ,1, 03, 00
HKR, WaveDriver,  XformModule    ,, "umdmxfrm.dll"
HKR, WaveDriver,  WaveHardwareID ,, "DRNEUHAUSVoiceModemWave"
HKR, WaveDriver, WaveDevices, 1, 01, 00
HKR,, VoiceBaudRate,    1, 00,c2,01,00
HKR,,Enumerator,,serwave.vxd
HKR,, VoiceProfile,         1, a1,10,09,02
HKR,  StartPlay,                1,, "at+vgt=131<cr>"
HKR,  StartPlay,                2,, "at+vtx<cr>"
HKR,  StopPlay,                 1,, "None"
HKR,  StopPlay,                 2,, "NoResponse"
HKR,  StartRecord,              1,, "at+vgr=130<cr>"
HKR,  StartRecord,              2,, "at+vrx<cr>"
HKR,  StopRecord,               1,, "None"
HKR,  StopRecord,               2,, "NoResponse"
HKR,, TerminateRecord,,      "<h10>!" ; DLE-!
HKR,, TerminatePlay,,        "<h10><h03>" ; DLE-ETX
HKR,, AbortPlay,,            "<h10><h03>" ; DLE-ETX
HKR, LineSetPlayFormat,       1,, "at+vsm=2,7200<cr>"
HKR, LineSetRecordFormat,     1,, "at+vsm=2,7200<cr>"
HKR, VoiceToDataAnswer,       1,, "at+fclass=0<cr>"
HKR, VoiceToDataAnswer,       2,, "ata<cr>"
HKR, VoiceAnswer,             1,, "at+fclass=8<cr>"
HKR, VoiceAnswer,             2,, "at+vls=0<cr>"
HKR, VoiceAnswer,             3,, "at+vtd=12<cr>"
HKR, VoiceAnswer,             4,, "at+vls=2<cr>"
HKR, VoiceDialNumberSetup,    1,, "at+fclass=8<cr>"
HKR, VoiceDialNumberSetup,    2,, "at+vls=0<cr>"
HKR, VoiceDialNumberSetup,    3,, "at+vrn=0<cr>"
HKR, VoiceDialNumberSetup,    4,, "at+vra=0<cr>"
HKR, VoiceDialNumberSetup,    5,, "at+vtd=12<cr>"
HKR, GenerateDigit,           1,, "at+vts=<Digit><cr>"
