;; netrtwlanu.inf 
;;
;; B-Link Wireless 802.11b/g/n USB 2.0 Network Adapter
;;
;; SHENZHEN BILIAN ELECTRONIC CO.,LTD.
;;
;; This release is primarily for WHQL test.
;;

[Version]
Signature		= $Chicago$
Compatible	= 1
Class		= Net
ClassGUID	= {4d36e972-e325-11ce-bfc1-08002be10318}
Provider		= %Realtek%
CatalogFile.NT	= netrtwlanu.cat		;; for WHQL certified
DriverVer = 07/12/2011,1015.0.0712.2011

[Manufacturer]
%Realtek% = Realtek,NTx86
%PCI% = PCI,NTx86
%Sitecom% = Sitecom,NTx86
%EDIMAX% = EDIMAX,NTx86
%Abocom% = Abocom,NTx86
%Amigo% = Amigo,NTx86
%Hercules% = Hercules,NTx86
%DLink% = DLink,NTx86
%Belkin% = Belkin,NTx86
%Zyxel% = Zyxel,NTx86
%ATKK92cu% = ATKK92cu,NTx86
%TRENDnet% = TRENDnet,NTx86
%Feixun92cu% = Feixun92cu,NTx86
%Feixun_Net92cu% = Feixun_Net92cu,NTx86
%XAVI% = XAVI,NTx86
%Netgearcus% = Netgearcus,NTx86
"Oar_Inc"			= Oar_Inc,NTx86, NTamd64
"ASUS"				= ASUS,NTx86, NTamd64

[ControlFlags]
ExcludeFromSelect = *

;;****************************************************************************
;; IDs for X86
;;****************************************************************************
[Realtek.NTx86]
%RTL8188cu.DeviceDesc% = RTL8192cu.ndi, USB\VID_0BDA&PID_8176								; RTK 88CU board for B/G/N      
%RTL8188cu.DeviceDesc% = RTL8192cu.ndi, USB\VID_0BFF&PID_8160								; RTK 88CU board for B/G/N      
%RTL8188cu.DeviceDesc% = RTL8192cu.ndi, USB\VID_0BDA&PID_8176&REV_0200&SS                                                   
%RTL8188cu_G.DeviceDesc% = RTL8192cu_G.ndi, USB\VID_0BDA&PID_8177							; RTK 88CU board for B/G        
%RTL8188cu_G.DeviceDesc% = RTL8192cu_G.ndi, USB\VID_0BDA&PID_8177&REV_0200&SS                                                 
%RTL8188ce_vau.DeviceDesc% = RTL8192cu.ndi, USB\VID_0BDA&PID_8170                           ; RTK 88CE_VAU board for B/G/N  
%RTL8188ce_vau.DeviceDesc% = RTL8192cu.ndi, USB\VID_0BDA&PID_8170&REV_0200&SS                                               
%RTL8188ce_vau_G.DeviceDesc% = RTL8192cu_G.ndi, USB\VID_0BDA&PID_817E                       ; RTK 88CE_VAU board for B/G    
%RTL8188ce_vau_G.DeviceDesc% = RTL8192cu_G.ndi, USB\VID_0BDA&PID_817E&REV_0200&SS                                             
%RTL8192ce_vau.DeviceDesc% = RTL8192cu.ndi, USB\VID_0BDA&PID_817C                           ; RTK 92CE_VAU board for B/G/N  
%RTL8192ce_vau.DeviceDesc% = RTL8192cu.ndi, USB\VID_0BDA&PID_817C&REV_0200&SS                                               
%RTL8192ce_vau.DeviceDesc% = RTL8192cu.ndi, USB\VID_0BDA&PID_8186
%RTL8188cu_slim_solo.DeviceDesc% = RTL8192cu.ndi, USB\VID_0BDA&PID_817A                     ; RTK slim_solo board for B/G/N 
%RTL8188cu_slim_solo.DeviceDesc% = RTL8192cu.ndi, USB\VID_0BDA&PID_817A&REV_0200&SS                                         
%RTL8188cu_slim_combo.DeviceDesc% = RTL8192cu.ndi, USB\VID_0BDA&PID_817B                    ; RTK slim_combo board for B/G/N
%RTL8188cu_slim_combo.DeviceDesc% = RTL8192cu.ndi, USB\VID_0BDA&PID_817B&REV_0200&SS                                        
%RTL8188ru.DeviceDesc% = RTL8192cu.ndi, USB\VID_0BDA&PID_817F                               ; RTK 88RU board for B/G/N      
%RTL8188ru.DeviceDesc% = RTL8192cu.ndi, USB\VID_0BDA&PID_817F&REV_0200&SS                                                   
%RTL8188cu.DeviceDesc% = RTL8192cu.ndi, USB\VID_103C&PID_1629	                			; HP/Liteon board for B/G/N     
%RTL8192cu.DeviceDesc% = RTL8192cu.ndi, USB\VID_0BDA&PID_8192                                                               
%RTL8192cu.DeviceDesc% = RTL8192cu.ndi, USB\VID_0BDA&PID_8178                               ; RTK 92CU board for B/G/N      
%RTK_AZ88vau.DeviceDesc% = RTL8192cu.ndi, USB\VID_13D3&PID_3358								; AZ 88CE_VAU for B/G/N
%RTK_AZ88vau_G.DeviceDesc% = RTL8192cu_G.ndi, USB\VID_13D3&PID_3359							; AZ 88CE_VAU for B/G
%RTK_AZ88cus.DeviceDesc% = RTL8192cu.ndi, USB\VID_13D3&PID_3357								; AZ 88CUS for B/G/N
;; For 8192D RTK common		================================================================
;;%RTL8192du.DeviceDesc% = RTL8192du.ndi, USB\VID_0BDA&PID_8194
;;%RTL8192du0.DeviceDesc% = RTL8192du.ndi, USB\VID_0BDA&PID_8193&MI_00
;;%RTL8192du1.DeviceDesc% = RTL8192du1.ndi, USB\VID_0BDA&PID_8193&MI_01
;; For 8723 RTK common		================================================================
;;%RTL8723u.DeviceDesc%  = RTL8723u.ndi, USB\VID_0BDA&PID_8724
;;%RTL8723u.DeviceDesc%  = RTL8723u.ndi, USB\VID_0BDA&PID_8724&MI_02
;;%RTL8188eu.DeviceDesc%  = RTL8192cu.ndi, USB\VID_0BDA&PID_8179

;; For 8192C Customerize	================================================================
[PCI.NTx86]
%PCI.DeviceDesc% = RTL8192cu.ndi, USB\VID_2019&PID_ED17
%PCI-2.DeviceDesc% = RTL8192cu.ndi, USB\VID_2019&PID_4902
%PCI_Abocom88cu.DeviceDesc% = RTL8192cu.ndi, USB\VID_2019&PID_AB2A
%PCI_Abocom92cu.DeviceDesc% = RTL8192cu.ndi, USB\VID_2019&PID_AB2B
%PCI_Vencer.DeviceDesc% = RTL8192cu.ndi, USB\VID_2019&PID_1201
;; For 8192D Customerize	================================================================
%PCI_Abocom_du0.DeviceDesc% = RTL8192du.ndi, USB\VID_2019&PID_AB2C&MI_00
%PCI_Abocom_du1.DeviceDesc% = RTL8192du1.ndi, USB\VID_2019&PID_AB2C&MI_01
%PCI_3_du0.DeviceDesc% = RTL8192du.ndi, USB\VID_2019&PID_4903&MI_00
%PCI_3_du1.DeviceDesc% = RTL8192du1.ndi, USB\VID_2019&PID_4903&MI_01
%PCI_4_du0.DeviceDesc% = RTL8192du.ndi, USB\VID_2019&PID_4904&MI_00
%PCI_4_du1.DeviceDesc% = RTL8192du1.ndi, USB\VID_2019&PID_4904&MI_01

[Sitecom.NTx86]
%Sitecom.DeviceDesc% = RTL8192cu.ndi, USB\VID_0DF6&PID_0052
%Sitecom_UN.DeviceDesc% = RTL8192cu.ndi, USB\VID_0DF6&PID_005C
%Sitecom_HG.DeviceDesc% = RTL8192cu.ndi, USB\VID_0DF6&PID_0061

[EDIMAX.NTx86]
%EDIMAX.DeviceDesc% = RTL8192cu.ndi, USB\VID_7392&PID_7811
%EDIMAX300.DeviceDesc% = RTL8192cu.ndi, USB\VID_7392&PID_7822

[Abocom.NTx86]
%Abocom.DeviceDesc% = RTL8192cu.ndi, USB\VID_07B8&PID_8189
%Abocom92cu.DeviceDesc% = RTL8192cu.ndi, USB\VID_07B8&PID_8178

[Amigo.NTx86]
%Amigo.DeviceDesc% = RTL8192cu.ndi, USB\VID_0EB0&PID_9071

[Hercules.NTx86]
%Hercules.DeviceDesc% = RTL8192cu.ndi, USB\VID_06F8&PID_E033

[DLink.NTx86]
%DLink-1.DeviceDesc% = RTL8192cu.ndi, USB\VID_2001&PID_330A
%DLink-2.DeviceDesc% = RTL8192cu.ndi, USB\VID_2001&PID_3309
%DLink-3.DeviceDesc% = RTL8192cu.ndi, USB\VID_2001&PID_3308
%DLink-4.DeviceDesc% = RTL8192cu.ndi, USB\VID_2001&PID_3307

[Belkin.NTx86]
%Belkin.DeviceDesc% = Belkin.ndi, USB\VID_050D&PID_1102
%Belkin-2.DeviceDesc% = Belkin.ndi, USB\VID_050D&PID_2102
%Belkin-3.DeviceDesc% = Belkin.ndi, USB\VID_050D&PID_2103

[Zyxel.NTx86]
%Zyxel.DeviceDesc% = RTL8192cu.ndi, USB\VID_0586&PID_341F	

[ATKK92cu.NTx86]
%ATKK92cu.DeviceDesc% = RTL8192cu.ndi, USB\VID_07AA&PID_0056

[TRENDnet.NTx86]
%TRENDnet.DeviceDesc% = RTL8192cu.ndi, USB\VID_20F4&PID_648B
%TRENDnet_2.DeviceDesc% = RTL8192cu.ndi, USB\VID_20F4&PID_624D
;; For 8192D Customerize	================================================================
%TRENDnet_3_du.DeviceDesc% = RTL8192du.ndi, USB\VID_20F4&PID_664B

[Feixun92cu.NTx86]
%Feixun92cu.DeviceDesc% = RTL8192cu.ndi, USB\VID_4855&PID_0090				; Feixun 88CUS for B/G/N
%Feixun92cu.DeviceDesc% = RTL8192cu.ndi, USB\VID_4855&PID_0091				; Feixun 92CU for B/G/N

[Feixun_Net92cu.NTx86]
%Feixun_Net92cu.DeviceDesc% = RTL8192cu.ndi, USB\VID_4856&PID_0091			; Feixun 8188CUS for B/G/N

[XAVI.NTx86]
%XAVI.DeviceDesc% = RTL8192cu.ndi, USB\VID_04F2&PID_AFF7				; XAVI 88CUSlim solo for B/G/N
%XAVI.DeviceDesc% = RTL8192cu.ndi, USB\VID_04F2&PID_AFF9				; XAVI 88CUSlim solo for B/G/N
%XAVI.DeviceDesc% = RTL8192cu.ndi, USB\VID_04F2&PID_AFFA				; XAVI 88CUSlim solo for B/G/N
%XAVI88cusc.DeviceDesc% = RTL8192cu.ndi, USB\VID_04F2&PID_AFF8				; XAVI 88CUSlim combo for B/G/N
%XAVI88cusc.DeviceDesc% = RTL8192cu.ndi, USB\VID_04F2&PID_AFFB				; XAVI 88CUSlim combo for B/G/N
%XAVI88cusc.DeviceDesc% = RTL8192cu.ndi, USB\VID_04F2&PID_AFFC				; XAVI 88CUSlim combo for B/G/N

[Netgearcus.NTx86]
;;%Netgearcus.DeviceDesc% = RTL8192cu.ndi, USB\VID_0846&PID_9041				; Netgear 88CUSfor B/G/N

[Oar_Inc.NTx86]
%Oar_Inc.DeviceDesc% = RTL8192cu.ndi, USB\VID_2019&PID_AB2E

[ASUS.NTx86]
%ASUS.DeviceDesc% = RTL8192cu.ndi, USB\VID_0B05&PID_17AB

;; For 8192D Customerize	================================================================

;; For 8723 Customerize		========================

;;****************************************************************************
;; IDs for X64
;;****************************************************************************
[Realtek.NTamd64]
;; For 8192C RTK common		================================================================
%RTL8188cu.DeviceDesc% = RTL8192cu.ndi, USB\VID_0BDA&PID_8176								; RTK 88CU board for B/G/N      
%RTL8188cu.DeviceDesc% = RTL8192cu.ndi, USB\VID_0BFF&PID_8160								; RTK 88CU board for B/G/N      
%RTL8188cu.DeviceDesc% = RTL8192cu.ndi, USB\VID_0BDA&PID_8176&REV_0200&SS                                                   
%RTL8188cu_G.DeviceDesc% = RTL8192cu_G.ndi, USB\VID_0BDA&PID_8177							; RTK 88CU board for B/G
%RTL8188cu_G.DeviceDesc% = RTL8192cu_G.ndi, USB\VID_0BDA&PID_8177&REV_0200&SS                                                 
%RTL8188ce_vau.DeviceDesc% = RTL8192cu.ndi, USB\VID_0BDA&PID_8170                           ; RTK 88CE_VAU board for B/G/N  
%RTL8188ce_vau.DeviceDesc% = RTL8192cu.ndi, USB\VID_0BDA&PID_8170&REV_0200&SS                                               
%RTL8188ce_vau_G.DeviceDesc% = RTL8192cu_G.ndi, USB\VID_0BDA&PID_817E                       ; RTK 88CE_VAU board for B/G    
%RTL8188ce_vau_G.DeviceDesc% = RTL8192cu_G.ndi, USB\VID_0BDA&PID_817E&REV_0200&SS                                             
%RTL8192ce_vau.DeviceDesc% = RTL8192cu.ndi, USB\VID_0BDA&PID_817C                           ; RTK 92CE_VAU board for B/G/N  
%RTL8192ce_vau.DeviceDesc% = RTL8192cu.ndi, USB\VID_0BDA&PID_817C&REV_0200&SS                                               
%RTL8192ce_vau.DeviceDesc% = RTL8192cu.ndi, USB\VID_0BDA&PID_8186
%RTL8188cu_slim_solo.DeviceDesc% = RTL8192cu.ndi, USB\VID_0BDA&PID_817A                     ; RTK slim_solo board for B/G/N 
%RTL8188cu_slim_solo.DeviceDesc% = RTL8192cu.ndi, USB\VID_0BDA&PID_817A&REV_0200&SS                                         
%RTL8188cu_slim_combo.DeviceDesc% = RTL8192cu.ndi, USB\VID_0BDA&PID_817B                    ; RTK slim_combo board for B/G/N
%RTL8188cu_slim_combo.DeviceDesc% = RTL8192cu.ndi, USB\VID_0BDA&PID_817B&REV_0200&SS                                        
%RTL8188ru.DeviceDesc% = RTL8192cu.ndi, USB\VID_0BDA&PID_817F                               ; RTK 88RU board for B/G/N      
%RTL8188ru.DeviceDesc% = RTL8192cu.ndi, USB\VID_0BDA&PID_817F&REV_0200&SS                                                   
%RTL8188cu.DeviceDesc% = RTL8192cu.ndi, USB\VID_103C&PID_1629	                			; HP/Liteon board for B/G/N     
%RTL8192cu.DeviceDesc% = RTL8192cu.ndi, USB\VID_0BDA&PID_8192                                                               
%RTL8192cu.DeviceDesc% = RTL8192cu.ndi, USB\VID_0BDA&PID_8178                               ; RTK 92CU board for B/G/N      
%RTL8192cu.DeviceDesc% = RTL8192cu.ndi, USB\VID_0586&PID_341F								; Zyxel/Abocom
%RTK_AZ88vau.DeviceDesc% = RTL8192cu.ndi, USB\VID_13D3&PID_3358								; AZ 88CE_VAU for B/G/N
%RTK_AZ88vau_G.DeviceDesc% = RTL8192cu_G.ndi, USB\VID_13D3&PID_3359							; AZ 88CE_VAU for B/G
%RTK_AZ88cus.DeviceDesc% = RTL8192cu.ndi, USB\VID_13D3&PID_3357								; AZ 88CUS for B/G/N
;; For 8192D RTK common		================================================================
;;%RTL8192du.DeviceDesc% = RTL8192du.ndi, USB\VID_0BDA&PID_8194
;;%RTL8192du0.DeviceDesc% = RTL8192du.ndi, USB\VID_0BDA&PID_8193&MI_00
;;%RTL8192du1.DeviceDesc% = RTL8192du1.ndi, USB\VID_0BDA&PID_8193&MI_01
;; For 8723 RTK common		================================================================
;;%RTL8723u.DeviceDesc%  = RTL8723u.ndi, USB\VID_0BDA&PID_8724
;;%RTL8723u.DeviceDesc%  = RTL8723u.ndi, USB\VID_0BDA&PID_8724&MI_02
;;%RTL8188eu.DeviceDesc%  = RTL8192cu.ndi, USB\VID_0BDA&PID_8179

[PCI.NTamd64]
%PCI.DeviceDesc% = RTL8192cu.ndi, USB\VID_2019&PID_ED17
%PCI-2.DeviceDesc% = RTL8192cu.ndi, USB\VID_2019&PID_4902
%PCI_Abocom88cu.DeviceDesc% = RTL8192cu.ndi, USB\VID_2019&PID_AB2A
%PCI_Abocom92cu.DeviceDesc% = RTL8192cu.ndi, USB\VID_2019&PID_AB2B
%PCI_Vencer.DeviceDesc% = RTL8192cu.ndi, USB\VID_2019&PID_1201
;; For 8192D Customerize	================================================================
%PCI_Abocom_du0.DeviceDesc% = RTL8192du.ndi, USB\VID_2019&PID_AB2C&MI_00
%PCI_Abocom_du1.DeviceDesc% = RTL8192du1.ndi, USB\VID_2019&PID_AB2C&MI_01
%PCI_3_du0.DeviceDesc% = RTL8192du.ndi, USB\VID_2019&PID_4903&MI_00
%PCI_3_du1.DeviceDesc% = RTL8192du1.ndi, USB\VID_2019&PID_4903&MI_01
%PCI_4_du0.DeviceDesc% = RTL8192du.ndi, USB\VID_2019&PID_4904&MI_00
%PCI_4_du1.DeviceDesc% = RTL8192du1.ndi, USB\VID_2019&PID_4904&MI_01

[Sitecom.NTamd64]
%Sitecom.DeviceDesc% = RTL8192cu.ndi, USB\VID_0DF6&PID_0052
%Sitecom_UN.DeviceDesc% = RTL8192cu.ndi, USB\VID_0DF6&PID_005C
%Sitecom_HG.DeviceDesc% = RTL8192cu.ndi, USB\VID_0DF6&PID_0061

[EDIMAX.NTamd64]
%EDIMAX.DeviceDesc% = RTL8192cu.ndi, USB\VID_7392&PID_7811
%EDIMAX300.DeviceDesc% = RTL8192cu.ndi, USB\VID_7392&PID_7822

[Abocom.NTamd64]
%Abocom.DeviceDesc% = RTL8192cu.ndi, USB\VID_07B8&PID_8189
%Abocom92cu.DeviceDesc% = RTL8192cu.ndi, USB\VID_07B8&PID_8178

[Amigo.NTamd64]
%Amigo.DeviceDesc% = RTL8192cu.ndi, USB\VID_0EB0&PID_9071

[Hercules.NTamd64]
%Hercules.DeviceDesc% = RTL8192cu.ndi, USB\VID_06F8&PID_E033

[DLink.NTamd64]
%DLink-1.DeviceDesc% = RTL8192cu.ndi, USB\VID_2001&PID_330A
%DLink-2.DeviceDesc% = RTL8192cu.ndi, USB\VID_2001&PID_3309
%DLink-3.DeviceDesc% = RTL8192cu.ndi, USB\VID_2001&PID_3308
%DLink-4.DeviceDesc% = RTL8192cu.ndi, USB\VID_2001&PID_3307

[Belkin.NTamd64]
%Belkin.DeviceDesc% = Belkin.ndi, USB\VID_050D&PID_1102
%Belkin-2.DeviceDesc% = Belkin.ndi, USB\VID_050D&PID_2102
%Belkin-3.DeviceDesc% = Belkin.ndi, USB\VID_050D&PID_2103

[Zyxel.NTamd64]
%Zyxel.DeviceDesc% = RTL8192cu.ndi, USB\VID_0586&PID_341F

[ATKK92cu.NTamd64]
%ATKK92cu.DeviceDesc% = RTL8192cu.ndi, USB\VID_07AA&PID_0056

[TRENDnet.NTamd64]
%TRENDnet.DeviceDesc% = RTL8192cu.ndi, USB\VID_20F4&PID_648B
%TRENDnet_2.DeviceDesc% = RTL8192cu.ndi, USB\VID_20F4&PID_624D
;; For 8192D Customerize	================================================================
%TRENDnet_3_du.DeviceDesc% = RTL8192du.ndi, USB\VID_20F4&PID_664B

[Feixun92cu.NTamd64]
%Feixun92cu.DeviceDesc% = RTL8192cu.ndi, USB\VID_4855&PID_0090				; Feixun 88CUS for B/G/N
%Feixun92cu.DeviceDesc% = RTL8192cu.ndi, USB\VID_4855&PID_0091				; Feixun 92CU for B/G/N

[Feixun_Net92cu.NTamd64]
%Feixun_Net92cu.DeviceDesc% = RTL8192cu.ndi, USB\VID_4856&PID_0091				; Feixun 8188CUS for B/G/N

[XAVI.NTamd64]
%XAVI.DeviceDesc% = RTL8192cu.ndi, USB\VID_04F2&PID_AFF7				; XAVI 88CUSlim solo for B/G/N
%XAVI.DeviceDesc% = RTL8192cu.ndi, USB\VID_04F2&PID_AFF9				; XAVI 88CUSlim solo for B/G/N
%XAVI.DeviceDesc% = RTL8192cu.ndi, USB\VID_04F2&PID_AFFA				; XAVI 88CUSlim solo for B/G/N
%XAVI88cusc.DeviceDesc% = RTL8192cu.ndi, USB\VID_04F2&PID_AFF8				; XAVI 88CUSlim combo for B/G/N
%XAVI88cusc.DeviceDesc% = RTL8192cu.ndi, USB\VID_04F2&PID_AFFB				; XAVI 88CUSlim combo for B/G/N
%XAVI88cusc.DeviceDesc% = RTL8192cu.ndi, USB\VID_04F2&PID_AFFC				; XAVI 88CUSlim combo for B/G/N

[Netgearcus.NTamd64]
;;%Netgearcus.DeviceDesc% = RTL8192cu.ndi, USB\VID_0846&PID_9041				; Netgear 88CUSfor B/G/N

[Oar_Inc.NTamd64]
%Oar_Inc.DeviceDesc% = RTL8192cu.ndi, USB\VID_2019&PID_AB2E

[ASUS.NTamd64]
%ASUS.DeviceDesc% = RTL8192cu.ndi, USB\VID_0B05&PID_17AB

;; For 8192D Customerize	================================================================

;; For 8723 Customerize		================================================================

;;****************************************************************************
;; Windows 2000/XP
;;****************************************************************************
;;----------------------------------------------------------------------------
;; Realtek default installation
;;----------------------------------------------------------------------------
[RTL8192cu.ndi.NT]
AddReg			= RTL8192cu.nt5.reg, RTL8192cu.common.reg, RTLWLAN.reg, 11nWirelessMode.reg
Characteristics		= 0x84
BusType			= 15 
CopyFiles			= RTWlanU.CopyFiles

[RTL8192cu.ndi.NT.Services]
AddService		= RTL8192cu, 2, RTL8192cu.nt5.Service, RTL8192cu.nt5.EventLog

;;----------------------------------------------------------------------------
;; Realtek default installation RTL8192DU
;;----------------------------------------------------------------------------
[RTL8192du.ndi.NT]
AddReg			= RTL8192du.nt5.reg, RTL8192du.common.reg, RTLWLAN.reg
Characteristics		= 0x84
BusType			= 15 
CopyFiles		= RTWlanU.CopyFiles

[RTL8192du.ndi.NT.Services]
AddService		= RTL8192cu, 2, RTL8192cu.nt5.Service, RTL8192cu.nt5.EventLog

[RTL8192du1.ndi.NT]
AddReg			= RTL8192du.nt5.reg, RTL8192du.common.reg, RTLWLAN.reg, ConcurrentMode.reg
Characteristics		= 0x84
BusType			= 15 
CopyFiles		= RTWlanU.CopyFiles

[RTL8192du1.ndi.NT.Services]
AddService		= RTL8192cu, 2, RTL8192cu.nt5.Service, RTL8192cu.nt5.EventLog


;;----------------------------------------------------------------------------
;; Realtek G mode sku installation
;;----------------------------------------------------------------------------
[RTL8192cu_G.ndi.NT]
AddReg			= RTL8192cu.nt5.reg, RTL8192cu.common.reg, RTLWLAN.reg, 11gWirelessMode.reg
Characteristics		= 0x84
BusType			= 15 
CopyFiles			= RTWlanU.CopyFiles

[RTL8192cu_G.ndi.NT.Services]
AddService		= RTL8192cu, 2, RTL8192cu.nt5.Service, RTL8192cu.nt5.EventLog

;;----------------------------------------------------------------------------
;; Realtek 8723u default installation
;;----------------------------------------------------------------------------
[RTL8723u.ndi.NT]
AddReg			= RTL8192cu.nt5.reg, RTL8723u.common.reg, RTLWLAN.reg
Characteristics		= 0x84
BusType			= 15 
CopyFiles		= RTWlanU.CopyFiles

[RTL8723u.ndi.NT.Services]
AddService		= RTL8192cu, 2, RTL8192cu.nt5.Service, RTL8192cu.nt5.EventLog

;;----------------------------------------------------------------------------
;; Belkin customized installation
;;----------------------------------------------------------------------------
[Belkin.ndi.NT]
AddReg			= RTL8192cu.nt5.reg, RTL8192cu.common.reg, RTLWLAN.reg, Belkin.reg
Characteristics		= 0x84
BusType			= 15 
CopyFiles			= RTWlanU.CopyFiles

[Belkin.ndi.NT.Services]
AddService		= RTL8192cu, 2, RTL8192cu.nt5.Service, RTL8192cu.nt5.EventLog


;;****************************************************************************
;; Windows 2000/XP parameters
;;****************************************************************************
[RTL8192cu.nt5.reg]
HKR, Ndi\Interfaces,	UpperRange, 0, "ndis5"
HKR, Ndi\Interfaces,	LowerRange, 0, "ethernet"
HKR, Ndi,		Service,    0, "RTL8192cu"

[RTL8192cu.nt5.Service]
DisplayName    = %RTL8192cu.DeviceDesc%
ServiceType    = 1		; %SERVICE_KERNEL_DRIVER%
StartType      = 3		; %SERRVICE_DEMAND_START%
ErrorControl   = 1		; %SERRVICE_ERROR_NORMAL%
ServiceBinary  = %12%\rtwlanu.sys
LoadOrderGroup = NDIS

[RTL8192cu.nt5.EventLog]
AddReg = RTL8192cu.nt5.AddEventLog.reg

[RTL8192cu.nt5.AddEventLog.reg]
HKR, , EventMessageFile, 0x00020000, "%%SystemRoot%%\System32\netevent.dll"
HKR, , TypesSupported  , 0x00010001, 7

;;****************************************************************************
;; Windows 2000/XP parameters RTL8192DU
;;****************************************************************************
[RTL8192du.nt5.reg]
HKR, Ndi\Interfaces,	UpperRange, 0, "ndis5"
HKR, Ndi\Interfaces,	LowerRange, 0, "ethernet"
HKR, Ndi,		Service,    0, "RTL8192du"

[RTL8192du.nt5.Service]
;DisplayName    = %RTL8192du.DeviceDesc.DispName%
DisplayName    = %RTL8192du.DeviceDesc%
ServiceType    = 1		; %SERVICE_KERNEL_DRIVER%
StartType      = 3		; %SERRVICE_DEMAND_START%
ErrorControl   = 1		; %SERRVICE_ERROR_NORMAL%
ServiceBinary  = %12%\rtwlanu.sys
LoadOrderGroup = NDIS

[RTL8192du.nt5.EventLog]
AddReg = RTL8192du.nt5.AddEventLog.reg

[RTL8192du.nt5.AddEventLog.reg]
HKR, , EventMessageFile, 0x00020000, "%%SystemRoot%%\System32\netevent.dll"
HKR, , TypesSupported  , 0x00010001, 7

;*******************************************************************************
; RTL8192cu common paramters
;*******************************************************************************
[RTL8192cu.common.reg]
HKR,defaults,LedCtrl,0,"1"
HKR,,LedCtrl,0,"1"

HKR,defaults,QoS,0,"1"
HKR,,QoS,0,"1"

HKR,defaults,WiFiConfg,0,"0"
HKR,,WiFiConfg,0,"0"

HKR,defaults,CcxRm,0,"1"
HKR,,CcxRm,0,"1"

HKR,defaults,CcxOffLineDurUpLimit,0,"0"
HKR,,CcxOffLineDurUpLimit,0,"0"

;; For USB selective suspend.
HKR,,EnableUsbSS,0,"0"

;; For GPIO detect setting.
HKR,,TimerGPIO,0,"0"
HKR,,GPIODelay,0,"2000"
HKR,,GPIOBack,0,"2000"

;; For PDN mode switch.
HKR,,PDNMode,0,"0"

;; For PDN mode switch.
HKR,,DongleSS,0,"1"

;; For Different selective suspend power save level. Now support 1 and 2. 2 is better.
HKR,,SSPwrLvl,0,"2"

;-------------------------------------------------------------------------------
;	USB Tx/Rx aggregation
;-------------------------------------------------------------------------------
HKR,defaults,UsbRxAggMode,0,"3"
HKR,,UsbRxAggMode,0,"3"

HKR,defaults,UsbRxAggBlockCount,0,"8"
HKR,,UsbRxAggBlockCount,0,"8"

HKR,defaults,UsbRxAggBlockTimeout,0,"6"
HKR,,UsbRxAggBlockTimeout,0,"6"

HKR,defaults,UsbRxAggPageCount,0,"72"
HKR,,UsbRxAggPageCount,0,"72"

HKR,defaults,UsbRxAggPageTimeout,0,"6"
HKR,,UsbRxAggPageTimeout,0,"6"

HKR,defaults,UsbTxAggMode,0,"1"
HKR,,UsbTxAggMode,0,"1"

HKR,defaults,UsbTxAggDescNum,0,"6"
HKR,,UsbTxAggDescNum,0,"6"

;*******************************************************************************
; RTL8192du common paramters
;*******************************************************************************
[RTL8192du.common.reg]
HKR,defaults,LedCtrl,0,"1"
HKR,,LedCtrl,0,"1"

HKR,defaults,QoS,0,"1"
HKR,,QoS,0,"1"

HKR,defaults,WiFiConfg,0,"0"
HKR,,WiFiConfg,0,"0"

;; For Earlymode 1:Enable 0:Disable
HKR,,bEarlymodeEnable,,"1"

HKR,defaults,CcxRm,0,"1"
HKR,,CcxRm,0,"1"

HKR,defaults,CcxOffLineDurUpLimit,0,"0"
HKR,,CcxOffLineDurUpLimit,0,"0"

;-------------------------------------------------------------------------------
;	USB Tx/Rx aggregation
;-------------------------------------------------------------------------------
HKR,defaults,UsbRxAggMode,0,"2"
HKR,,UsbRxAggMode,0,"2"

HKR,defaults,UsbRxAggBlockCount,0,"18"
HKR,,UsbRxAggBlockCount,0,"18"

HKR,defaults,UsbRxAggBlockTimeout,0,"7"
HKR,,UsbRxAggBlockTimeout,0,"7"

HKR,defaults,UsbRxAggPageCount,0,"72"
HKR,,UsbRxAggPageCount,0,"72"

HKR,defaults,UsbRxAggPageTimeout,0,"6"
HKR,,UsbRxAggPageTimeout,0,"6"

HKR,defaults,UsbTxAggMode,0,"1"
HKR,,UsbTxAggMode,0,"1"

HKR,defaults,UsbTxAggDescNum,0,"4"
HKR,,UsbTxAggDescNum,0,"4"


;*******************************************************************************
; RTL8723u common paramters
;*******************************************************************************
[RTL8723u.common.reg]
HKR,defaults,LedCtrl,0,"1"
HKR,,LedCtrl,0,"1"

HKR,defaults,WiFi11bIbss,0,"0"
HKR,,WiFi11bIbss,0,"0"

HKR,defaults,bRateAdaptive,0,"1"
HKR,,bRateAdaptive,0,"1"

HKR,defaults,QoS,0,"1"
HKR,,QoS,0,"1"

HKR,defaults,WiFiConfg,0,"0"
HKR,,WiFiConfg,0,"0"

HKR,defaults,CcxRm,0,"1"
HKR,,CcxRm,0,"1"

HKR,defaults,CcxOffLineDurUpLimit,0,"0"
HKR,,CcxOffLineDurUpLimit,0,"0"

;; For USB selective suspend.
HKR,,EnableUsbSS,0,"0"

;; For GPIO detect setting.
HKR,,TimerGPIO,0,"0"
HKR,,GPIODelay,0,"1000"
HKR,,GPIOBack,0,"1000"

;; For PDN mode switch.
HKR,,PDNMode,0,"1"

;; For PDN mode switch.
HKR,,DongleSS,0,"1"

;-------------------------------------------------------------------------------
;	USB Tx/Rx aggregation
;-------------------------------------------------------------------------------
HKR,defaults,UsbRxAggMode,0,"3"
HKR,,UsbRxAggMode,0,"3"

HKR,defaults,UsbRxAggBlockCount,0,"8"
HKR,,UsbRxAggBlockCount,0,"8"

HKR,defaults,UsbRxAggBlockTimeout,0,"6"
HKR,,UsbRxAggBlockTimeout,0,"6"

HKR,defaults,UsbRxAggPageCount,0,"72"
HKR,,UsbRxAggPageCount,0,"72"

HKR,defaults,UsbRxAggPageTimeout,0,"6"
HKR,,UsbRxAggPageTimeout,0,"6"

HKR,defaults,UsbTxAggMode,0,"1"
HKR,,UsbTxAggMode,0,"1"

HKR,defaults,UsbTxAggDescNum,0,"6"
HKR,,UsbTxAggDescNum,0,"6"

;;----------------------------------------------------------------------------
;; Realtek WLAN NIC parameters
;;----------------------------------------------------------------------------
[RTLWLAN.reg]
HKR,defaults,SSID,0,"ANY"
HKR,,SSID,0,"ANY"

HKR,defaults,Channel,0,"1"
HKR,,Channel,0,"1"

HKR,Ndi\params\NetworkType,			ParamDesc,  0, %NETWORK_TYPE_STR%
HKR,Ndi\params\NetworkType,			type,       0, "enum"
HKR,Ndi\params\NetworkType,			default,    0, "1"
HKR,Ndi\params\NetworkType\enum,		"0",        0, %AD_HOC_STR%
HKR,Ndi\params\NetworkType\enum,		"1",        0, %INFRASTRUCTURE_STR%
HKR,Ndi\params\NetworkType\enum,		"2",        0, %AUTO_SELECT%
HKR,defaults,NetworkType,0,"1"
HKR,,NetworkType,0,"1"

HKR,defaults,StaUapsd,0,"0"
HKR,,StaUapsd,0,"0"

; For B/G mode and B/G/N mode switch, we will use different wireless mode registry in later section
;HKR,Ndi\params\WirelessMode, 			ParamDesc, 	0, %WL_MODE_STR%
;HKR,Ndi\params\WirelessMode, 			type, 		0, "enum"
;HKR,Ndi\params\WirelessMode, 			default, 	0, "8"
;HKR,Ndi\params\WirelessMode\enum, 		"2", 		0, %IEEE_802_11B_STR%
;HKR,Ndi\params\WirelessMode\enum, 		"4", 		0, %IEEE_802_11BG_STR%
;HKR,Ndi\params\WirelessMode\enum, 		"8", 		0, %IEEE_802_11BGN_STR%
;HKR,defaults,WirelessMode, 0, "8"
;HKR,,WirelessMode, 0, "8"

HKR,defaults,RxReorder,0,"1"
HKR,,RxReorder,0,"1"

HKR,,DefaultKeyID,,"0"
HKR,,DefaultKey0,,""
HKR,,DefaultKey1,,""
HKR,,DefaultKey2,,""
HKR,,DefaultKey3,,""

;Inactive Power Save
HKR,defaults,InactivePs,0,"0"
HKR,,InactivePs,0,"0"

;Leisure Power Save
HKR,defaults,bLeisurePs,0,"2"
HKR,,bLeisurePs,0,"2"

;Fw Control LPS
HKR,defaults,bFwCtrlLPS,0,"3"
HKR,,bFwCtrlLPS,0,"3"

;; LPS Interval
;HKR,defaults,LPSIntvl,0,"5"
HKR,,LPSIntvl,0,"5"

;BTmode
HKR,,bBTMode,0,"1"

; Reset Tx Hang
HKR,defaults,USBResetTxHang,0,"1"
HKR,,USBResetTxHang,0,"1"

HKR,,WEPinNmode,0,"0"

HKR,Ndi\params\PSPXlinkMode,			ParamDesc,  0, %PSP_XLINK_STR%
HKR,Ndi\params\PSPXlinkMode,			type,       0, "enum"
HKR,Ndi\params\PSPXlinkMode,			default,    0, "0"
HKR,Ndi\params\PSPXlinkMode\enum,		"0",        0, %DISABLE_STR%
HKR,Ndi\params\PSPXlinkMode\enum,		"1",        0, %ENABLE_STR%
HKR,defaults,PSPXlinkMode,0,"0"
HKR,,PSPXlinkMode,0,"0"

; Hw Beacon Max Error
HKR,,bBcnMaxErrorRegEnable,0,"0"

;-------------------------------------------------------------------------------
;	USB Tx/Rx aggregation
;-------------------------------------------------------------------------------
HKR,defaults,AggDMEnable,0,"0"
HKR,,AggDMEnable,0,"0"

HKR,defaults,UPDMEnable,0,"1"
HKR,,UPDMEnable,0,"1"

HKR,defaults,LinkSpeedLevel,0,"1"
HKR,,LinkSpeedLevel,0,"1"

HKR,defaults,AutoConnect,0,"1"
HKR,,AutoConnect,0,"1"


;;----------------------------------------------------------------------------
;; Belkin WLAN NIC parameters
;;----------------------------------------------------------------------------
[Belkin.reg]
HKR,Ndi\params\RFOff,			ParamDesc,  0, "Radio"
HKR,Ndi\params\RFOff,			type,       0, "enum"
HKR,Ndi\params\RFOff,			default,    0, "0"
HKR,Ndi\params\RFOff\enum,		"0",        0, "On"
HKR,Ndi\params\RFOff\enum,		"1",        0, "Off"
HKR,defaults,RFOff,0,"0"
HKR,,RFOff,0,"0"

;;----------------------------------------------------------------------------
;; Wireless mode option parameters
;;----------------------------------------------------------------------------
[11gWirelessMode.reg]
HKR,Ndi\params\WirelessMode, 		ParamDesc, 	0, %WL_MODE_STR%
HKR,Ndi\params\WirelessMode, 		type, 		0, "enum"
HKR,Ndi\params\WirelessMode, 		default, 	0, "8"
HKR,Ndi\params\WirelessMode\enum, 	"2", 		0, %IEEE_802_11B_STR%
HKR,Ndi\params\WirelessMode\enum, 	"4", 		0, %IEEE_802_11BG_STR%
HKR,defaults,WirelessMode, 0, "4"
HKR,,WirelessMode, 0, "4"

[11nWirelessMode.reg]
HKR,Ndi\params\WirelessMode, 		ParamDesc, 	0, %WL_MODE_STR%
HKR,Ndi\params\WirelessMode, 		type, 		0, "enum"
HKR,Ndi\params\WirelessMode, 		default, 	0, "8"
HKR,Ndi\params\WirelessMode\enum, 	"2", 		0, %IEEE_802_11B_STR%
HKR,Ndi\params\WirelessMode\enum, 	"4", 		0, %IEEE_802_11BG_STR%
HKR,Ndi\params\WirelessMode\enum, 	"8", 		0, %IEEE_802_11BGN_STR%
HKR,defaults,WirelessMode, 0, "8"
HKR,,WirelessMode, 0, "8"

;*******************************************************************************
; Two STA Concurrent Mode Reg
;*******************************************************************************
[ConcurrentMode.reg]
HKR,Ndi\params\TwoStaConcurrentMode,		ParamDesc,  0, %TWO_STA_CONCURRENT_MODE%
HKR,Ndi\params\TwoStaConcurrentMode,		type,       0, "enum"
HKR,Ndi\params\TwoStaConcurrentMode,			default,    0, "1"
HKR,Ndi\params\TwoStaConcurrentMode\enum,		"0",        0, %SECONDARY_DISABLE%
HKR,Ndi\params\TwoStaConcurrentMode\enum,		"1",        0, %SECONDARY_ENABLE%
HKR,Ndi\params\TwoStaConcurrentMode\enum,		"2",        0, %SECONDARY_AUTO%
HKR,defaults,TwoStaConcurrentMode,0,"0"
HKR,,TwoStaConcurrentMode,0,"0"

;*******************************************************************************
; Destination Directory
;*******************************************************************************
[RTWlanU.CopyFiles]
rtwlanu.sys,,,2

[DestinationDirs]
RTWlanU.CopyFiles	= 12

;;****************************************************************************
;; Source Files
;;****************************************************************************
[SourceDisksFiles]
rtwlanu.sys = 1

[SourceDisksNames]
1=%DISKNAME%,,,

;*******************************************************************************
; Strings
;*******************************************************************************
[Strings]
SSID_STR					= "SSID"
CHANNEL_STR					= "Channel"
NETWORK_TYPE_STR			= "Network Type"
LED_CONTROL_STR				= "LED Control" 
POWER_SAVE_STR				= "Power Save Mode"
WIFI_IBSS_STR				= "IBSS Default 11b Mode"
RATE_ADAPTIVE_STR			= "Rate Adaptive"
QOS_STR						= "QoS"
WiFiConfg_STR	  			= "WiFiConfg"
WMM_APSD					= "WMM APSD"
CCX_RM_STR					= "CCX Radio Measurement"
CCX_OFF_LINE_DUR_UP_LIMIT_STR		= "CCX Max Off-Line Measurement (0: unlimited)"
FORCE_PRIORITY_STR			= "Forced Priority"
HW_PARA_STR					= "Init from HwParaFile"
THREE_WIRE_MODE_STR			= "Three Wire Programming Mode"
BOARD_TYPE_STR				= "Board Type"
PROTECTION_MODE_STR			= "Protection Mode"
TPC_STR						= "Transmit Power Control"
TPC_POLARITY_STR				= "TPC Polarity Select"
HIGH_POWER_STR				= "High Power Mechanism"
INIT_GAIN_STR				= "Initial Gain State"
CW_MAX_MIN_STR				= "Contention Window"
PSP_XLINK_STR				= "PSP XLink Mode"
DISABLE_STR					= "Disable"
ENABLE_STR					= "Enable"
AD_HOC_STR					= "Ad Hoc"
INFRASTRUCTURE_STR			= "Infrastructure"
AUTO_SELECT					= "Auto select"
WL_MODE_STR					= "Wireless Mode"
RX_REORDER_STR				= "Rx Reorder"
CAM_STR						= "CAM"
MAX_PSP_STR					= "MAX_PSP"
Fast_PSP_STR				= "Fast_PSP"
NO_AC_STR					= "No AC (Disable)"
ALL_AC_STR					= "ALL AC"
IEEE_802_11B_STR 			= "IEEE 802.11b"
IEEE_802_11BG_STR 			= "IEEE 802.11b/g"
IEEE_802_11BGN_STR 			= "IEEE 802.11b/g/n"

;-------------------------------------------------------------------------------
;	USB Tx/Rx aggregation strings
;-------------------------------------------------------------------------------
RX_AGG_MODE_STR				= "Rx Aggregation Mode"
RX_AGG_MODE_BLOCK_STR		= "Rx Agg USB Block Mode"
RX_AGG_MODE_PAGE_STR		= "Rx Agg DMA Page Mode"
RX_AGG_MODE_MIXED_STR		= "Rx Agg USB and Page Mixed Mode"
RX_AGG_USB_BLOCK_STR		= "Rx Agg USB Block Threshold"
RX_AGG_USB_TIMEOUT_STR		= "Rx Agg USB Timeout"
RX_AGG_DMA_PAGE_STR			= "Rx Agg DMA Page Threshold"
RX_AGG_DMA_TIMEOUT_STR		= "Rx Agg DMA Timeout"
TX_AGG_MODE_STR				= "Tx Aggregation Mode"
TX_AGG_DESC_PER_OUT_STR		= "Tx Agg Number of descriptor per bulk out"

;-------------------------------------------------------------------------------
;	Two STA Concurrent Mode
;-------------------------------------------------------------------------------
TWO_STA_CONCURRENT_MODE			= "Two STA Concurrent Mode"
SECONDARY_DISABLE			= "Secondary client Disable"
SECONDARY_ENABLE			= "Secondary Client Enable"
SECONDARY_AUTO				= "Secondary Client Auto Select"


;*******************************************************************************
; manufacture description
;*******************************************************************************
Realtek					= "SHENZHEN BILIAN ELECTRONIC CO.,LTD"
PCI             		= "PLANEX COMMUNICATIONS INC"
Sitecom         		= "Sitecom Europe B.V."
EDIMAX					= "EDIMAX"
Abocom					= "AboCom System, Inc."
Amigo					= "Amigo Technology Inc"
Hercules				= "Guillemot Corporation S.A"
DLink					= "D-Link Corporation"
Belkin					= "Belkin International, Inc."
Zyxel					= "ZyXEL"
ATKK92cu				= "Allied Telesis K.K."
TRENDnet				= "TRENDnet"
Feixun92cu				= "Shanghai Feixun Communication Co.,Ltd"
Feixun_Net92cu			= "NetweeN"
XAVI					= "XAVI Technologies Corp."
Netgearcus				= "NETGEAR Inc."
Oar_Inc					= "Oar Inc."
ASUS					= "ASUSTeK Computer Inc."


;*******************************************************************************
;	Source disk name
;*******************************************************************************
;DISKNAME							= "B-Link RTL8192CU Wireless LAN 802.11n USB 2.0 Network Adapter Driver Disk"
DISKNAME							= "B-Link Wireless LAN 802.11n USB 2.0 Network Adapter Driver Disk"
RTL8192cu.DeviceDesc 				= "B-Link RTL8192CU Wireless LAN 802.11n USB 2.0 Network Adapter"
RTL8192cu.DeviceDesc.DispName		= "B-Link RTL8192CU Wireless LAN 802.11n USB 2.0 Network Adapter"
RTL8188cu.DeviceDesc 				= "B-Link RTL8188CU Wireless LAN 802.11n USB 2.0 Network Adapter"
RTL8188cu.DeviceDesc.DispName		= "B-Link RTL8188CU Wireless LAN 802.11n USB 2.0 Network Adapter"
RTL8188cu_G.DeviceDesc 				= "B-Link RTL8188CU Wireless LAN 802.11 USB 2.0 Network Adapter"
RTL8188cu_G.DeviceDesc.DispName		= "B-Link RTL8188CU Wireless LAN 802.11 USB 2.0 Network Adapter"
RTL8188ce_vau.DeviceDesc 			= "B-Link RTL8188CE-VAU Wireless LAN 802.11n USB minicard"
RTL8188ce_vau.DeviceDesc.DispName	= "B-Link RTL8188CE-VAU Wireless LAN 802.11n USB minicard"
RTL8188ce_vau_G.DeviceDesc 			= "B-Link RTL8188CE-VAU Wireless LAN 802.11 USB minicard"
RTL8188ce_vau_G.DeviceDesc.DispName	= "B-Link RTL8188CE-VAU Wireless LAN 802.11 USB minicard"
RTL8192ce_vau.DeviceDesc 			= "B-Link RTL8192CE-VAU Wireless LAN 802.11n USB minicard"
RTL8192ce_vau.DeviceDesc.DispName	= "B-Link RTL8192CE-VAU Wireless LAN 802.11n USB minicard"
RTL8188cu_slim_solo.DeviceDesc		= "B-Link RTL8188CUS Wireless LAN 802.11n USB Slim Solo"
RTL8188cu_slim_solo.DeviceDesc.DispName	= "B-Link RTL8188CUS Wireless LAN 802.11n USB Slim Solo"
RTL8188cu_slim_combo.DeviceDesc		= "B-Link RTL8188CUS Wireless LAN 802.11n USB Slim Combo"
RTL8188cu_slim_combo.DeviceDesc.DispName= "B-Link RTL8188CUS Wireless LAN 802.11n USB Slim Combo"
RTL8188ru.DeviceDesc 				= "B-Link RTL8188RU Wireless LAN 802.11n USB High Power Dongle"
RTL8188ru.DeviceDesc.DispName		= "B-Link RTL8188RU Wireless LAN 802.11n USB High Power Dongle"
RTK_AZ88vau.DeviceDesc				= "B-Link RTL8188CE-VAU Wireless LAN 802.11n USB minicard"
RTK_AZ88vau.DeviceDesc.DispName		= "B-Link RTL8188CE-VAU Wireless LAN 802.11n USB minicard"
RTK_AZ88vau_G.DeviceDesc			= "B-Link RTL8188CE-VAU Wireless LAN 802.11 USB minicard"
RTK_AZ88vau_G.DeviceDesc.DispName	= "B-Link RTL8188CE-VAU Wireless LAN 802.11 USB minicard"
RTK_AZ88cus.DeviceDesc				= "Wireless USB Card"
RTK_AZ88cus.DeviceDesc.DispName		= "Wireless USB Card"
PCI.DeviceDesc 						= "GW-USValue-EZ"
PCI.DeviceDesc.DispName				= "GW-USValue-EZ"
PCI-2.DeviceDesc 					= "GW-USLight"
PCI-2.DeviceDesc.DispName			= "GW-USLight"
PCI_Abocom88cu.DeviceDesc 			= "GW-USNano2"
PCI_Abocom88cu.DeviceDesc.DispName	= "GW-USNano2"
PCI_Abocom92cu.DeviceDesc 			= "GW-USEco300"
PCI_Abocom92cu.DeviceDesc.DispName	= "GW-USEco300"
PCI_Vencer.DeviceDesc 				= "BT-Micro3H2X Wireless LAN"
PCI_Vencer.DeviceDesc.DispName		= "BT-Micro3H2X Wireless LAN"
PCI_Abocom_du0.DeviceDesc 			= "GW-USDual300 MAC0"
PCI_Abocom_du0.DeviceDesc.DispName	= "GW-USDual300 MAC0"
PCI_Abocom_du1.DeviceDesc 			= "GW-USDual300 MAC1"
PCI_Abocom_du1.DeviceDesc.DispName	= "GW-USDual300 MAC1"
PCI_3_du0.DeviceDesc 				= "GW-USFang300"
PCI_3_du0.DeviceDesc.DispName		= "GW-USFang300"
PCI_3_du1.DeviceDesc 				= "GW-USFang300"
PCI_3_du1.DeviceDesc.DispName		= "GW-USFang300"
PCI_4_du0.DeviceDesc 				= "GW-USUltra300"
PCI_4_du0.DeviceDesc.DispName		= "GW-USUltra300"
PCI_4_du1.DeviceDesc 				= "GW-USUltra300"
PCI_4_du1.DeviceDesc.DispName		= "GW-USUltra300"
Sitecom.DeviceDesc 					= "Sitecom Wireless Ultra Nano USB Adapter 150N X1 WL-365"
Sitecom.DeviceDesc.DispName			= "Sitecom Wireless Ultra Nano USB Adapter 150N X1 WL-365"
Sitecom_UN.DeviceDesc 				= "Wireless Ultra Nano Network Adapter 150N"
Sitecom_UN.DeviceDesc.DispName		= "Wireless Ultra Nano Network Adapter 150N"
Sitecom_HG.DeviceDesc 				= "Wireless High-gain Network adapter 300N WLA-4001"
Sitecom_HG.DeviceDesc.DispName		= "Wireless High-gain Network adapter 300N WLA-4001"
EDIMAX.DeviceDesc 					= "150Mbps Wireless 802.11b/g/n Nano USB Adapter"
EDIMAX.DeviceDesc.DispName			= "150Mbps Wireless 802.11b/g/n Nano USB Adapter"
EDIMAX300.DeviceDesc 				= "Edimax 300Mbps wireless 802.11b/g/n USB adapter"
EDIMAX300.DeviceDesc.DispName		= "Edimax 300Mbps wireless 802.11b/g/n USB adapter"
Abocom.DeviceDesc 					= "B-Link 802.11n/b/g Mini Wireless LAN USB2.0 Adapter"
Abocom.DeviceDesc.DispName			= "B-Link 802.11n/b/g Mini Wireless LAN USB2.0 Adapter"
Abocom92cu.DeviceDesc				= "B-Link 802.11n/b/g Mini Wireless LAN USB2.0 Adapter"
Abocom92cu.DeviceDesc.DispName		= "B-Link 802.11n/b/g Mini Wireless LAN USB2.0 Adapter"
Amigo.DeviceDesc 					= "Wireless USB Card"
Amigo.DeviceDesc.DispName			= "Wireless USB Card"
Hercules.DeviceDesc 				= "Hercules Wireless N Pico USB "
Hercules.DeviceDesc.DispName		= "Hercules Wireless N Pico USB "
DLink-1.DeviceDesc 					= "D-Link DWA-133 Wireless N USB Adapter"
DLink-1.DeviceDesc.DispName			= "D-Link DWA-133 Wireless N USB Adapter"
DLink-2.DeviceDesc 					= "D-Link DWA-135 Wireless N USB Adapter"
DLink-2.DeviceDesc.DispName			= "D-Link DWA-135 Wireless N USB Adapter"
DLink-3.DeviceDesc 					= "D-Link DWA-121 Wireless N USB Adapter"
DLink-3.DeviceDesc.DispName			= "D-Link DWA-121 Wireless N USB Adapter"
DLink-4.DeviceDesc 					= "D-Link DWA-130 Wireless N USB Adapter(rev.F1)"
DLink-4.DeviceDesc.DispName			= "D-Link DWA-130 Wireless N USB Adapter(rev.F1)"
Belkin.DeviceDesc 					= "Surf Wireless Micro USB Adapter"
Belkin.DeviceDesc.DispName			= "Surf Wireless Micro USB Adapter"
Belkin-2.DeviceDesc 				= "Belkin Surf & Share Wireless USB Adapter"
Belkin-2.DeviceDesc.DispName		= "Belkin Surf & Share Wireless USB Adapter"
Belkin-3.DeviceDesc 				= "N300 USB Network Adapter"
Belkin-3.DeviceDesc.DispName		= "N300 USB Network Adapter"
ZyXEL.DeviceDesc 					= "ZyXEL Wireless LAN 802.11n USB 2.0 Network Adapter"
ZyXEL.DeviceDesc.DispName			= "ZyXEL Wireless LAN 802.11n USB 2.0 Network Adapter"
ATKK92cu.DeviceDesc					= "Corega CG-WLUSB300NS"
ATKK92cu.DeviceDesc.DispName		= "Corega CG-WLUSB300NS"
TRENDnet.DeviceDesc					= "TRENDnet 150Mbps Micro Wireless N USB Adapter"
TRENDnet.DeviceDesc.DispName		= "TRENDnet 150Mbps Micro Wireless N USB Adapter"
TRENDnet_2.DeviceDesc				= "TRENDnet 300Mbps Mini Wireless N USB Adapter"
TRENDnet_2.DeviceDesc.DispName		= "TRENDnet 300Mbps Mini Wireless N USB Adapter"
TRENDnet_3_du.DeviceDesc			= "TRENDnet 300Mbps Dual Band Wireless USB Adapter"
TRENDnet_3_du.DeviceDesc.DispName	= "TRENDnet 300Mbps Dual Band Wireless USB Adapter"
Feixun92cu.DeviceDesc 				= "FEIXUN Wireless LAN 802.11n USB 2.0 Network Adaptor"
Feixun92cu.DeviceDesc.DispName		= "FEIXUN Wireless LAN 802.11n USB 2.0 Network Adaptor"
Feixun_Net92cu.DeviceDesc 			= "NetweeN Wireless LAN 802.11n USB 2.0 Network Adaptor"
Feixun_Net92cu.DeviceDesc.DispName	= "NetweeN Wireless LAN 802.11n USB 2.0 Network Adaptor"
XAVI.DeviceDesc 					= "B-Link RTL8188CUS Wireless LAN 802.11n USB Slim Solo"
XAVI.DeviceDesc.DispName			= "B-Link RTL8188CUS Wireless LAN 802.11n USB Slim Solo"
XAVI88cusc.DeviceDesc 				= "B-Link RTL8188CUS Wireless LAN 802.11n USB Slim Combo"
XAVI88cusc.DeviceDesc.DispName		= "B-Link RTL8188CUS Wireless LAN 802.11n USB Slim Combo"
Netgearcus.DeviceDesc 				= "NETGEAR WNA1000M N150 Wireless USB Micro Adapter"
Netgearcus.DeviceDesc.DispName		= "NETGEAR WNA1000M N150 Wireless USB Micro Adapter"
Oar_Inc.DeviceDesc 					= "SW-WF02-AD15"
Oar_Inc.DeviceDesc.DispName			= "SW-WF02-AD15"
ASUS.DeviceDesc 					= "ASUS USB-N13 300Mbps 11n  Wireless USB dongle"
ASUS.DeviceDesc.DispName			= "ASUS USB-N13 300Mbps 11n  Wireless USB dongle"
;*******************************************************************************
; RTL8723u Device description
;*******************************************************************************
RTL8723u.DeviceDesc 				= "B-Link RTL8723U Wireless LAN 802.11n USB 2.0 Network Adapter"
RTL8723u.DeviceDesc.DispName		= "B-Link RTL8723U Wireless LAN 802.11n USB 2.0 Network Adapter"
;*******************************************************************************
; RTL8192DU Device description
;*******************************************************************************
RTL8192du.DeviceDesc 				= "B-Link RTL8192DU Wireless LAN 802.11n USB 2.0 Network Adapter"
RTL8192du.DeviceDesc.DispName		= "B-Link RTL8192DU Wireless LAN 802.11n USB 2.0 Network Adapter"
RTL8192du0.DeviceDesc 				= "B-Link RTL8192DU Wireless LAN 802.11n USB 2.0 Network Adapter MAC0"
RTL8192du0.DeviceDesc.DispName		= "B-Link RTL8192DU Wireless LAN 802.11n USB 2.0 Network Adapter MAC0"
RTL8192du1.DeviceDesc 				= "B-Link RTL8192DU Wireless LAN 802.11n USB 2.0 Network Adapter MAC1"
RTL8192du1.DeviceDesc.DispName		= "B-Link RTL8192DU Wireless LAN 802.11n USB 2.0 Network Adapter MAC1"
;*******************************************************************************
; RTL8188EU Device description
;*******************************************************************************
RTL8188eu.DeviceDesc 				= "B-Link RTL8188EU Wireless LAN 802.11n USB 2.0 Network Adapter"
RTL8188eu.DeviceDesc.DispName		= "B-Link RTL8188EU Wireless LAN 802.11n USB 2.0 Network Adapter"