<?xml version="1.0" encoding="UTF-8"?><module fritzingVersion="0.7.2b" moduleId="SparkFun-RF-EM408_OUTLINE-">
<!-- generated from Sparkfun Eagle Library 'SparkFun-RF' EM408_OUTLINE  -->
<version>4</version>
<date>2013-02-13</date>
<label>U</label>
<author>www.fritzing.org</author>
<description>This device is only the outline of the EM408 GPS receiver.  The device is intended to give the
designer an idea of what how the receiver will fit on the board.  THIS DEVICE DOES NOT PROVIDE ANY ELECTRICAL CONNECTION TO THE BOARD!  Include the EM408_CON device in order to connect the EM408 to your design.</description>
<title>EM408_OUTLINE</title>
<tags>
<tag>EM408_OUTLINE</tag>
</tags>
<properties>
<property name="package">em408_outline</property>
<property name="family">sparkfun GPS</property>
</properties>
<views>
<breadboardView>
<layers image="breadboard/sparkfun-rf_em408_outline_breadboard.svg">
<layer layerId="breadboard"/>
</layers>
</breadboardView>
<schematicView>
<layers image="schematic/sparkfun-rf_em408_outline_schematic.svg">
<layer layerId="schematic"/>
</layers>
</schematicView>
<pcbView>
<layers image="pcb/sparkfun-rf_em408_outline_pcb.svg">
<layer layerId="silkscreen"/>
</layers>
</pcbView>
<iconView>
<layers image="icon/EM408_OUTLINE.svg">
<layer layerId="icon"/>
</layers>
</iconView>
</views>
<connectors>
</connectors>
</module>